diff -Naur orig/hal/arm/netarm/current/cdl/hal_arm_netarm.cdl new/hal/arm/netarm/current/cdl/hal_arm_netarm.cdl
--- orig/hal/arm/netarm/current/cdl/hal_arm_netarm.cdl	2004-11-29 17:35:46.000000000 +0100
+++ new/hal/arm/netarm/current/cdl/hal_arm_netarm.cdl	2005-03-10 14:54:13.903367200 +0100
@@ -18,6 +18,26 @@
 		puts $::cdl_system_header "#define CYGBLD_HAL_PLATFORM_H <pkgconf/hal_arm_netarm.h>"
 	}
 
+	cdl_option CYGSEM_HAL_INSTRUCTION_CACHE_SETS {
+	    display "Sets for Instruction Cache"
+	    parent CYGPKG_HAL_CACHE_CONTROL
+	    active_if CYGSEM_HAL_ENABLE_ICACHE_ON_STARTUP
+		flavor data
+		legal_values 0 to 15
+		default_value 0xc
+	    description "MSB: SET1 | SET2 | SET3 | SET4"
+	}
+	
+	cdl_option CYGSEM_HAL_DATA_CACHE_SETS {
+	    display "Sets for Data Cache"
+	    parent CYGPKG_HAL_CACHE_CONTROL
+	    active_if CYGSEM_HAL_ENABLE_DCACHE_ON_STARTUP
+		flavor data
+		legal_values 0 to 15
+		default_value 0x3
+	    description "MSB: SET1 | SET2 | SET3 | SET4"
+	}
+
   	cdl_component CYG_HAL_STARTUP {
     	display "Startup type" 
 		flavor data 
diff -Naur orig/hal/arm/netarm/current/include/hal_cache.h new/hal/arm/netarm/current/include/hal_cache.h
--- orig/hal/arm/netarm/current/include/hal_cache.h	2004-11-29 17:35:46.000000000 +0100
+++ new/hal/arm/netarm/current/include/hal_cache.h	2005-03-10 14:41:51.032173600 +0100
@@ -19,25 +19,57 @@
 #define HAL_ICACHE_WAYS                 4        // Associativity of the cache
 #define HAL_ICACHE_LINE_SIZE            4       // Size of a cache line
 
-#define HAL_ICACHE_BASE					0x08000000
-#define HAL_ICACHE_MASK					0xfe000000
+#if defined(CYG_HAL_STARTUP_ROMRAM) || defined(CYG_HAL_STARTUP_RAM)
+	#define HAL_ICACHE_BASE					0x04000000
+	#define HAL_DCACHE_BASE					0x08000000
+#else
+	#define HAL_ICACHE_BASE					0x02000000
+	#define HAL_DCACHE_BASE					0x04000000
+#endif
+
+#define HAL_ICACHE_MASK					0xff000000
+#define HAL_DCACHE_MASK					0xff000000
+
+
+#ifdef CYGSEM_HAL_ENABLE_ICACHE_ON_STARTUP
+	#define HAL_ICACHE_ENABLE()						\
+	{												\
+		*(CCR0)=(HAL_ICACHE_BASE) |					\
+				(HAL_ICACHE_MASK >> 8) |			\
+				(CCR_ENABLE) |						\
+				(1 << 11)	|						\
+				(CYGSEM_HAL_INSTRUCTION_CACHE_SETS);	\
+	}
+#else
+	#define HAL_ICACHE_ENABLE() (*(CCR0)=0)
+#endif
 
-#define HAL_ICACHE_ENABLE()                     \
+#ifdef CYGSEM_HAL_ENABLE_DCACHE_ON_STARTUP
+	#define HAL_DCACHE_ENABLE()						\
+	{												\
+		*(CCR1)=(HAL_DCACHE_BASE) |					\
+				(HAL_DCACHE_MASK >> 8) |			\
+				(CCR_ENABLE) |						\
+				(1 << 11)	|						\
+				(CYGSEM_HAL_DATA_CACHE_SETS);	\
+	}
+#else
+	#define HAL_DCACHE_ENABLE() (*(CCR1)=0)
+#endif
+
+#define HAL_CACHE_ENABLE()                      \
 {	 											\
 	unsigned int *p;							\
 	int i;									    \
 												\
 	*(SYSCON)|=SYSCON_CINIT|SYSCON_CACHE;		\
 	p=(unsigned int *)0xfff00000;				\
-	for(i=0;i<(0x2000/4);i++,p++)				\
+	for(i=0;i<(0x4000/4);i++,p++)				\
 		*p=0;									\
 												\
-	*(SYSCON)&=~(SYSCON_CINIT);					\
-	*(CCR0)=(HAL_ICACHE_BASE) |					\
-			(HAL_ICACHE_MASK >> 8) |			\
-			(CCR_ENABLE) |						\
-			(CCR_SET1 | CCR_SET2 | CCR_SET3 | CCR_SET4);		\
-	*(CCR1)=0;									\
+	HAL_ICACHE_ENABLE();						\
+	HAL_DCACHE_ENABLE();						\
+												\
 	*(SYSCON)|=SYSCON_CACHE;					\
 	*(SYSCON)&=~SYSCON_WB;						\
 }
@@ -45,17 +77,25 @@
 #define HAL_ICACHE_DISABLE()                    \
 {												\
 	*(CCR0)=0;									\
-	*(SYSCON)&=~SYSCON_CACHE;							\
+	if (HAL_DCACHE_IS_ENABLED == 0)				\
+		*(SYSCON)&=~SYSCON_CACHE;				\
 }
 
-#define HAL_ICACHE_IS_ENABLED(_state_) _state_ = ((*(CCR0) & CCR_ENABLE) >> 15)
+#define HAL_DCACHE_DISABLE()                    \
+{												\
+	*(CCR1)=0;									\
+	if (HAL_ICACHE_IS_ENABLED == 0)				\
+		*(SYSCON)&=~SYSCON_CACHE;				\
+}
+
+#define HAL_ICACHE_IS_ENABLED ((*(CCR0) & CCR_ENABLE) >> 15)
 
-#define HAL_ICACHE_INVALIDATE_ALL()				\
+#define HAL_CACHE_INVALIDATE_ALL()				\
 {												\
 	unsigned *p;								\
 	*(SYSCON)|=SYSCON_CINIT;							\
 	for(p=(unsigned int*)0xfff00000;			\
-		(unsigned int)p<0xfff02000;				\
+		(unsigned int)p<0xfff04000;				\
 		p++)									\
 		*p=0;									\
 												\
@@ -64,25 +104,13 @@
 
 #define HAL_ICACHE_SYNC()
 
-#define HAL_ICACHE_PURGE_ALL()  HAL_ICACHE_INVALIDATE_ALL()
-
-#define HAL_DCACHE_LINE_SIZE 0
-#define HAL_DCACHE_WAYS 0
-#define HAL_DCACHE_SETS 0
-
-#define HAL_DCACHE_ENABLE()
+#define HAL_CACHE_PURGE_ALL()  HAL_ICACHE_INVALIDATE_ALL()
 
-#define HAL_DCACHE_DISABLE()
-
-#define HAL_DCACHE_INVALIDATE_ALL()
+#define HAL_DCACHE_LINE_SIZE 4
+#define HAL_DCACHE_WAYS 4
 
 #define HAL_DCACHE_SYNC()
 
-#define HAL_DCACHE_IS_ENABLED(_state_) 0
-
-#define HAL_DCACHE_FLUSH( _base_ , _size_ )
-
-#define HAL_DCACHE_STORE( _base_ , _size_ )
+#define HAL_DCACHE_IS_ENABLED ((*(CCR1) & CCR_ENABLE) >> 15)
 
 #endif
-
diff -Naur orig/hal/arm/netarm/current/include/hal_platform_setup.h new/hal/arm/netarm/current/include/hal_platform_setup.h
--- orig/hal/arm/netarm/current/include/hal_platform_setup.h	2004-11-29 17:35:46.000000000 +0100
+++ new/hal/arm/netarm/current/include/hal_platform_setup.h	2005-03-15 12:20:27.760534400 +0100
@@ -19,7 +19,7 @@
 // Usage:       #include <cyg/hal/hal_platform_setup.h>
 //
 //####DESCRIPTIONEND####
-// 
+//
 //===========================================================================*/
 
 #include <pkgconf/system.h>           // System-wide configuration info
@@ -34,15 +34,31 @@
 							bic	r0,r0, #((\x & 3)<<1); \
 							str r0,[r1]
 
-#if defined(CYG_HAL_STARTUP_ROMRAM) 
+#if defined(CYG_HAL_STARTUP_ROMRAM)
 #define HAL_FLASH_PHYS_ADDR		0x02000000
-#define UNMAPPED(x) 			((x)-0x08000000)
+#define UNMAPPED(x) 			((x)-0x04000000)
 #elif  defined(CYG_HAL_STARTUP_ROM)
 #define HAL_FLASH_PHYS_ADDR		0x02000000
 #define UNMAPPED(x) 			((x)-0x02000000)
 #endif
 		.macro	PLATFORM_SETUP1
-	
+
+		ldr		r1,=0xffb0000c		// software reset
+		ldr		r0,=0x00000123
+		str		r0,[r1]
+		ldr		r0,=0x00000321
+		str		r0,[r1]
+
+		mov		r0,#1000
+loop:
+		sub		r0,r0,#1
+		cmp		r0,#0
+		bne		loop
+
+		ldr		r0,=0x00000123
+		str		r0,[r1]
+		ldr		r0,=0x00000321
+		str		r0,[r1]
 
 #if defined(CYG_HAL_STARTUP_ROMRAM) || defined(CYG_HAL_STARTUP_ROM)
 		mov		r1,#0xff000000
@@ -51,7 +67,11 @@
 		ldr		r0,=0x4004a800		/* System control register */
 		str		r0,[r1]
 
-		mov		r0,#0				/* PLL config */
+#ifdef CYG_HAL_STARTUP_ROM			/* PLL config */
+		mov		r0,#0
+#else
+		ldr		r0,=0x09000e1e
+#endif
 		str		r0,[r1,#8]
 
 		ldr		r0,=0xfff00000		/* PORT A mode & dir */
@@ -64,7 +84,7 @@
 		str		r0,[r1,#0x28]
 
 		add		r1,r1,#0x100000		/* Setup MEM Module base addr */
-		
+
 		ldr		r0,=0x148C0000		/* Memory Module Config register */
 		str		r0,[r1]
 
@@ -79,7 +99,7 @@
 		ldr		r0,=0xf3f00304		/* CS0 Option register */
 		str		r0,[r1,#0x14]
 
-		ldr		r0,=0x02000001		/* CS0 Base Address register */ 
+		ldr		r0,=0x02000001		/* CS0 Base Address register */
 		str		r0,[r1,#0x10]
 
 		mov		pc,r2				/* Jump to new flash base */
@@ -92,7 +112,7 @@
 
 		/* Configure SDRAM */
 
-		ldr		r0,=0xf38000b0		/* CS1 Option register, BLEN=11 */
+		ldr		r0,=0xf3000070		/* CS1 Option register, BLEN=11 */
 		str		r0,[r1,#0x24]
 
 		ldr		r0,=0x0000022d		/* CS1 Base Address register */
@@ -110,7 +130,7 @@
 #if defined(CYG_HAL_STARTUP_ROMRAM)
 		mov		r1,#0
 		mov		r2,#HAL_FLASH_PHYS_ADDR
-		ldr		r3,=(__heap1 - 0x04000000 + HAL_FLASH_PHYS_ADDR)
+		ldr		r3,=(__heap1 - 0x08000000 + HAL_FLASH_PHYS_ADDR)
 
 		mov		r4,#0
 		mov		r6,#0
@@ -129,11 +149,11 @@
 		nop
 		nop
 		nop
-30:	
+30:
 #endif
 
 #endif
 		.endm
-			
+
 #endif
 
diff -Naur orig/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_ram.ldi new/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_ram.ldi
--- orig/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_ram.ldi	2004-11-29 17:35:46.000000000 +0100
+++ new/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_ram.ldi	2005-03-10 14:56:07.137708600 +0100
@@ -3,34 +3,32 @@
 MEMORY
 {
     noncacheram : ORIGIN = 0, LENGTH = 16*1024*1024
-    dataram : ORIGIN = 0x4000000, LENGTH = 16*1024*1024
-    codecacheram : ORIGIN = 0x8000000, LENGTH = 16*1024*1024
+    codecacheram : ORIGIN = 0x4000000, LENGTH = 16*1024*1024
+    datacacheram : ORIGIN = 0x8000000, LENGTH = 16*1024*1024
 }
 
 SECTIONS
 {
     SECTIONS_BEGIN
-	_dataram = 0x4000000;
+	_dataram = 0x8000000;
     SECTION_rom_vectors (nocacheram, 0x0, LMA_EQ_VMA)
     SECTION_fixed_vectors (nocacheram, ALIGN (0x4), LMA_EQ_VMA)
-	code_start = . + 0x8000000; 
-    SECTION_text (codecacheram, code_start, AT (code_start - 0x8000000))
+	code_start = . + 0x4000000; 
+    SECTION_text (codecacheram, code_start, AT (code_start - 0x4000000))
 	fini = .;
-    SECTION_fini (codecacheram, ALIGN (0x4), AT (fini - 0x8000000))
+    SECTION_fini (codecacheram, ALIGN (0x4), AT (fini - 0x4000000))
 	rodata = .;
-    SECTION_rodata (codecacheram, ALIGN (0x4), AT (rodata - 0x8000000))
+    SECTION_rodata (codecacheram, ALIGN (0x4), AT (rodata - 0x4000000))
 	rodata1 = .;
-    SECTION_rodata1 (codecacheram, ALIGN (0x4), AT (rodata1 - 0x8000000))
+    SECTION_rodata1 (codecacheram, ALIGN (0x4), AT (rodata1 - 0x4000000))
 	fixup = .;
-    SECTION_fixup (codecacheram, ALIGN (0x4), AT (fixup - 0x8000000))
+    SECTION_fixup (codecacheram, ALIGN (0x4), AT (fixup - 0x4000000))
 	gcc_except_table =.;
-    SECTION_gcc_except_table (codecacheram, ALIGN (0x4), AT (gcc_except_table - 0x8000000))
-	data_start = ALIGN(0x4) - 0x4000000; 
-    SECTION_data (dataram, data_start, AT (data_start - 0x4000000))
+    SECTION_gcc_except_table (codecacheram, ALIGN (0x4), AT (gcc_except_table - 0x4000000))
+	data_start = ALIGN(0x4) + 0x4000000; 
+    SECTION_data (datacacheram, data_start, AT (data_start - 0x8000000))
 	bss = .;
-    SECTION_bss (dataram, ALIGN (0x4), AT (bss - 0x4000000))
+    SECTION_bss (datacacheram, ALIGN (0x4), AT (bss - 0x8000000))
     CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
     SECTIONS_END
 }
-
-
diff -Naur orig/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_romram.ldi new/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_romram.ldi
--- orig/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_romram.ldi	2004-11-29 17:35:46.000000000 +0100
+++ new/hal/arm/netarm/current/include/pkgconf/mlt_arm_netarm_romram.ldi	2005-03-10 14:56:18.184583600 +0100
@@ -3,34 +3,32 @@
 MEMORY
 {
     noncacheram : ORIGIN = 0, LENGTH = 16*1024*1024
-    dataram : ORIGIN = 0x4000000, LENGTH = 16*1024*1024
-    codecacheram : ORIGIN = 0x8000000, LENGTH = 16*1024*1024
+    codecacheram : ORIGIN = 0x4000000, LENGTH = 16*1024*1024
+    datacacheram : ORIGIN = 0x8000000, LENGTH = 16*1024*1024
 }
 
 SECTIONS
 {
     SECTIONS_BEGIN
-	_dataram = 0x4000000;
+	_dataram = 0x8000000;
     SECTION_rom_vectors (nocacheram, 0x0, LMA_EQ_VMA)
     SECTION_fixed_vectors (nocacheram, ALIGN (0x4), LMA_EQ_VMA)
-	code_start = . + 0x8000000; 
-    SECTION_text (codecacheram, code_start, AT (code_start -  0x8000000))
+	code_start = . + 0x4000000; 
+    SECTION_text (codecacheram, code_start, AT (code_start - 0x4000000))
 	fini = .;
-    SECTION_fini (codecacheram, ALIGN (0x4), AT (fini -  0x8000000))
+    SECTION_fini (codecacheram, ALIGN (0x4), AT (fini - 0x4000000))
 	rodata = .;
-    SECTION_rodata (codecacheram, ALIGN (0x4), AT (rodata -  0x8000000))
+    SECTION_rodata (codecacheram, ALIGN (0x4), AT (rodata - 0x4000000))
 	rodata1 = .;
-    SECTION_rodata1 (codecacheram, ALIGN (0x4), AT (rodata1 -  0x8000000))
+    SECTION_rodata1 (codecacheram, ALIGN (0x4), AT (rodata1 - 0x4000000))
 	fixup = .;
-    SECTION_fixup (codecacheram, ALIGN (0x4), AT (fixup -  0x8000000))
-	gcc_except_table = .;
-    SECTION_gcc_except_table (codecacheram, ALIGN (0x4), AT (gcc_except_table -  0x8000000))
-	data_start = . - 0x4000000; 
-    SECTION_data (dataram, data_start, AT (data_start -  0x4000000))
+    SECTION_fixup (codecacheram, ALIGN (0x4), AT (fixup - 0x4000000))
+	gcc_except_table =.;
+    SECTION_gcc_except_table (codecacheram, ALIGN (0x4), AT (gcc_except_table - 0x4000000))
+	data_start = ALIGN(0x4) + 0x4000000; 
+    SECTION_data (datacacheram, data_start, AT (data_start - 0x8000000))
 	bss = .;
-    SECTION_bss (dataram, ALIGN (0x4), AT (bss -  0x4000000))
+    SECTION_bss (datacacheram, ALIGN (0x4), AT (bss - 0x8000000))
     CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
     SECTIONS_END
 }
-
-
diff -Naur orig/hal/arm/netarm/current/include/plf_mmap.h new/hal/arm/netarm/current/include/plf_mmap.h
--- orig/hal/arm/netarm/current/include/plf_mmap.h	1970-01-01 01:00:00.000000000 +0100
+++ new/hal/arm/netarm/current/include/plf_mmap.h	2005-04-01 11:13:23.378304500 +0200
@@ -0,0 +1,62 @@
+#ifndef CYGONCE_HAL_NETARM_PLATFORM_PLF_MMAP_H
+#define CYGONCE_HAL_NETARM_PLATFORM_PLF_MMAP_H
+//==========================================================================
+//
+//      plf_mmap.h
+//
+//      Platform specific memory map support
+//
+//==========================================================================
+//####ECOSGPLCOPYRIGHTBEGIN####
+// -------------------------------------------
+// This file is part of eCos, the Embedded Configurable Operating System
+// Copyright (C) 2005 eCosCentric Ltd.
+//
+// eCos is free software; you can redistribute it and/or modify it under
+// the terms of the GNU General Public License as published by the Free
+// Software Foundation; either version 2 or (at your option) any later version.
+//
+// eCos is distributed in the hope that it will be useful, but WITHOUT ANY
+// WARRANTY; without even the implied warranty of MERCHANTABILITY or
+// FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+// for more details.
+//
+// You should have received a copy of the GNU General Public License along
+// with eCos; if not, write to the Free Software Foundation, Inc.,
+// 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA.
+//
+// As a special exception, if other files instantiate templates or use macros
+// or inline functions from this file, or you compile this file and link it
+// with other works to produce a work based on this file, this file does not
+// by itself cause the resulting work to be covered by the GNU General Public
+// License. However the source code for this file must still be made available
+// in accordance with section (3) of the GNU General Public License.
+//
+// This exception does not invalidate any other reasons why a work based on
+// this file might be covered by the GNU General Public License.
+//
+// -------------------------------------------
+//####ECOSGPLCOPYRIGHTEND####
+//==========================================================================
+//#####DESCRIPTIONBEGIN####
+//
+// Author(s):           Harald Brandl (harald.brandl@fh-joanneum.at)
+// Contributors:        Harald Brandl
+// Date:                01.04.2005
+// Purpose:             NET+ARM memory map macro
+// Description:
+//
+//####DESCRIPTIONEND####
+//
+//==========================================================================
+
+
+extern unsigned int _dataram;
+
+
+#define HAL_CACHED_TO_UNCACHED_ADDRESS( caddr, uaddr, type ) CYG_MACRO_START       \
+    uaddr = (type)((cyg_uint32)caddr - (cyg_uint32)(&_dataram)); \
+CYG_MACRO_END
+
+//---------------------------------------------------------------------------
+#endif // CYGONCE_HAL_NETARM_PLATFORM_PLF_MMAP_H
diff -Naur orig/hal/arm/netarm/current/src/netarm_misc.c new/hal/arm/netarm/current/src/netarm_misc.c
--- orig/hal/arm/netarm/current/src/netarm_misc.c	2004-11-29 17:35:48.000000000 +0100
+++ new/hal/arm/netarm/current/src/netarm_misc.c	2005-02-22 11:57:58.296703200 +0100
@@ -7,15 +7,15 @@
 //==========================================================================
 //==========================================================================
 //#####DESCRIPTIONBEGIN####
-// 
+//
 // Author(s):    Peter De Schrijver (p2@mind.be)
 // Contributors: Peter De Schrijver (p2@mind.be)
 // Date:         2002-10-25
 // Purpose:      HAL board support
 // Description:  Implementations of HAL board interfaces
-// 
+//
 //####DESCRIPTIONEND####
-// 
+//
 //========================================================================*/
 
 #include <pkgconf/hal.h>
@@ -29,7 +29,7 @@
 #include <cyg/hal/hal_io.h>             // IO macros
 #include <cyg/hal/hal_arch.h>           // Register state info
 #include <cyg/hal/hal_diag.h>
-#include <cyg/hal/hal_intr.h>           // Interrupt names 
+#include <cyg/hal/hal_intr.h>           // Interrupt names
 #include <cyg/hal/hal_cache.h>
 #include <cyg/hal/hal_netarm.h>         // Hardware definitions
 #include <cyg/hal/hal_if.h>             // calling interface API
@@ -74,9 +74,9 @@
 void hal_clock_read(cyg_uint32 *pvalue) {
 
 	static cyg_uint32 clock_val;
-	
-	clock_val=*TIMERSTAT1 & 0x1ff; 
-	*pvalue = (cyg_uint32)(_period - clock_val); 
+
+	clock_val=*TIMERSTAT1 & 0x1ff;
+	*pvalue = (cyg_uint32)(_period - clock_val);
 
 }
 
@@ -97,24 +97,19 @@
 
 void hal_hardware_init(void) {
 
+#if defined (CYGSEM_HAL_ENABLE_ICACHE_ON_STARTUP) ||	\
+	defined (CYGSEM_HAL_ENABLE_DCACHE_ON_STARTUP)
 
-#ifdef ENABLECACHE
-	/* CS1 BSIZE = 4 */
-	*OR1&=~(3 << 4);
-	*OR1|=1 << 4;
-	
-	HAL_ICACHE_ENABLE();
-#endif /* ENABLECACHE */
+	HAL_CACHE_ENABLE();
 
+#endif /* ENABLECACHE */
 
 	*INTENABLE_CLR=0xffffffff;
-			
+
 	hal_clock_initialize(CYGNUM_HAL_RTC_PERIOD);
 
 	hal_if_init();
 
-//	HAL_ICACHE_DISABLE();
-
 }
 
 int hal_spurious_ints;
@@ -125,8 +120,8 @@
 	int i;
 
 	stat=*INTSTATUS;
-	
-	for(i=0;i<CYGNUM_HAL_ISR_MAX;i++) 
+
+	for(i=0;i<CYGNUM_HAL_ISR_MAX;i++)
 		if(stat & (1<<i))
 			return i+1;
 
@@ -154,7 +149,7 @@
 
 	if((vector>=CYGNUM_HAL_INTERRUPT_C0) && (vector<=CYGNUM_HAL_INTERRUPT_C3)) {
 		*PORTC|=1<< (vector+23);
-    	if(up) 
+    	if(up)
 			*PORTC|=1<< (vector+15);
 		else
 			*PORTC&=~(1<< (vector+15));
