
<CHAPTER id="hal-porting-guide">
<TITLE><!-- <index></index> -->	Porting Guide</TITLE>

<!-- {{{ Intro -->

<section id="hal-porting-intro">
<title>Introduction</title>

<para>
eCos has been designed to be fairly easy to port to new targets. A
target is a specific platform (board) using a given architecture (CPU
type). The porting is facilitated by the hierarchical layering of the
eCos sources - all architecture and platform specific code is
implemented in a HAL (hardware abstraction layer).
</para>

<para>
By porting the eCos HAL to a new target the core functionality of eCos
(infra, kernel, uITRON, etc) will be able to run on the target. It may
be necessary to add further platform specific code such as serial
drivers, display drivers, ethernet drivers, etc. to get a fully
capable system.
</para>

<para>
This document is intended as a help to the HAL porting process. Due to
the nature of a porting job, it is impossible to give a complete
description of what has to be done for each and every potential
target. This should not be considered a clear-cut recipe - you will
probably need to make some implementation decisions, tweak a few
things, and just plain have to rely on common sense.
</para>

<para>
However, what is covered here should be a large part of the
process. If you get stuck, you are advised to read the
<ulink url="http://sourceware.cygnus.com/ml/ecos-discuss/">
ecos-discuss archive
</ulink>
where you may find discussions which apply to the problem at
hand. You are also invited to ask questions on the
<ulink url="http://sourceware.cygnus.com/ecos/intouch.html">
ecos-discuss mailing list
</ulink>
to help you resolve problems - but as is always the case
with community lists, do not consider it an oracle for any and all
questions. Use common sense - if you ask too many questions which
could have been answered by reading the
<ulink
url="http://sourceware.cygnus.com/ecos/docs-latest/">documentation</ulink>,
<ulink url="http://sourceware.cygnus.com/fom/ecos">FAQ</ulink> or
<ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/?cvsroot=ecos">
source code
</ulink>, you are likely to be ignored.
</para>

<para>
This document will be continually improved by Red Hat engineers as
time allows. Feedback and help with improving the document is sought,
so if you have any comments at all, please do not hesitate to post
them on
<ulink url="mailto:ecos-discuss@sourceware.cygnus.com?subject=[porting]<subject>">
ecos-discuss
</ulink>
(please prefix the subject with [porting]).
</para>

<para>
At the moment this document is mostly an outline. There are many
details to fill in before it becomes complete. Many places you'll just
find a list of keywords / concepts that should be described (please
post on ecos-discuss if there are areas you think are not covered).
</para>

<para>
All pages or sections where the caption ends in [TBD] contain little
more than key words and/or random thoughts - there has been no work
done as such on the content. The word FIXME may appear in the text to
highlight places where information is missing.
</para>

</section>

<!-- }}} -->
<!-- {{{ HAL Structure -->

<section id="hal-porting-structure">
<title>HAL Structure</title>

<para>
In order to write an eCos HAL it's a good idea to have at least a
passing understanding of how the HAL interacts with the rest of the
system.
</para>

<!-- {{{ HAL Classes -->

<section>
<title>HAL Classes</title>

<para>
The eCos HAL consists of four HAL sub-classes. This table gives a
brief description of each class and partly reiterates the description
in <xref linkend="hal-architecture-variant-and-platform">. The links
refer to the on-line CVS tree (specifically to the sub-HALs used by
the PowerPC MBX target).
</para>

<informaltable frame=all>
<tgroup cols=3 align=left colsep=1 rowsep=1>
<thead>
<row>
<entry>HAL type</entry>
<entry>Description</entry>
<entry>Functionality Overview</entry>
</row>
</thead>
<tbody>
<row>
<entry>
Common HAL <ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/hal/common/current?cvsroot=ecos">(hal/common)</ulink>
</entry>
<entry>Configuration options and functionality shared by all HALs.</entry>
<entry>Generic debugging functionality, driver API, eCos/ROM monitor
      calling interface, and tests.</entry>
</row>
<row>
  <entry>Architecture HAL <ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/hal/powerpc/arch/current?cvsroot=ecos">(hal/&lt;architecture&gt;/arch)</ulink></entry>
  <entry>Functionality specific to the given architecture. Also default
  implementations of some functionality which can be overridden by
  variant or platform HALs.</entry>
  <entry>Architecture specific debugger functionality (handles single
     stepping, exception-to-signal conversion, etc.),
     exception/interrupt vector definitions and handlers, cache
     definition and control macros, context switching code, assembler
     functions for early system initialization, configuration options,
     and possibly tests. </entry>
</row>
<row>
  <entry>Variant HAL <ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/hal/powerpc/mpc8xx/current?cvsroot=ecos">(hal/&lt;architecture&gt;/&lt;variant&gt;)</ulink></entry>
  <entry>Some CPU architectures consist of a number variants, for example
     MIPS CPUs come in both 32 and 64 bit versions, and some variants
     have embedded features additional to the CPU core.
</entry>
  <entry>Variant extensions to the architecture code (cache,
     exception/interrupt), configuration options, possibly drivers for
     variant on-core devices, and possibly tests.</entry>
</row>
<row>
  <entry>Platform HAL <ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/hal/powerpc/mbx/current?cvsroot=ecos">(hal/&lt;architecture&gt;/&lt;platform&gt;)</ulink></entry>
  <entry>Contains functionality and configuration options specific to the
      platform.
</entry>
  <entry>Early platform initialization code, platform memory layout
     specification, configuration options (processor speed, compiler
     options), diagnostic IO functions, debugger IO functions,
     platform specific extensions to architecture or variant code
     (off-core interrupt controller), and possibly tests.</entry>
</row>
<row>
  <entry>Auxiliary HAL <ulink url="http://sourceware.cygnus.com/cgi-bin/cvsweb.cgi/ecos/packages/hal/powerpc/quicc/current?cvsroot=ecos">(hal/&lt;architecture&gt;/&lt;module&gt;)</ulink></entry>
  <entry>Some variants share common modules on the core. Motorola's PowerPC
      QUICC is an example of such a module.
</entry>
  <entry>Module specific functionality (interrupt controller, simple
      device drivers), possibly tests.
</entry>
</row>
</tbody>
</tgroup>
</informaltable>

</section>

<!-- }}} -->
<!-- {{{ File Descriptions -->

<section>
<title>File Descriptions</title>

<para>
Listed below are the files found in various HALs, with a short
description of what each file contains. When looking in existing HALs
beware that they do not necessarily follow this naming scheme.
If you are writing a new HAL, please try to follow it as
closely as possible. Still, no two targets are the same, so sometimes
it makes sense to use additional files.
</para>

<!-- {{{ Common HAL -->

<section>
<title>Common HAL</title>

<informaltable frame=all>
<tgroup cols=2 align=left colsep=1 rowsep=1>
<thead>
<row>
<entry>File</entry>
<entry>Description</entry>
</row>
</thead>
<tbody>

<row>
<entry><filename>include/dbg-thread-syscall.h</filename></entry>
  <entry>Defines the thread debugging syscall function. This is used by
  the ROM monitor to access the thread debugging API in the RAM
  application.  <!-- FIXME: link thread debug description -->.</entry>
</row>
<row>
<entry><filename>include/dbg-threads-api.h</filename></entry>
  <entry>Defines the thread debugging API. <!-- FIXME: link thread
  debug description -->.</entry>
</row>
<row>
<entry><filename>include/drv_api.h</filename></entry>
  <entry>Defines the driver API.</entry>
</row>
<row>
<entry><filename>include/generic-stub.h</filename></entry>
  <entry>Defines the generic stub features.</entry>
</row>
<row>
<entry><filename>include/hal_if.h</filename></entry>
  <entry>Defines the ROM/RAM calling interface API.</entry>
</row>
<row>
<entry><filename>include/hal_misc.h</filename></entry>
  <entry>Defines miscellaneous helper functions shared by all HALs.</entry>
</row>
<row>
<entry><filename>include/hal_stub.h</filename></entry>
  <entry>Defines eCos mappings of GDB stub features.</entry>
</row>
<row>
<entry><filename>src/dbg-threads-syscall.c</filename></entry>
  <entry>Thread debugging implementation.</entry>
</row>
<row>
<entry><filename>src/drv_api.c</filename></entry>
  <entry>Driver API implementation. Depending on configuration this
  provides either wrappers for the kernel API, or a minimal
  implementation of these features. This allows drivers to be written
  relying only on HAL features.</entry>
</row>
<row>
<entry><filename>src/dummy.c</filename></entry>
  <entry>Empty dummy file ensuring creation of libtarget.a.</entry>
</row>
<row>
<entry><filename>src/generic-stub.c</filename></entry>
  <entry>Generic GDB stub implementation. This provides the
  communication protocol used to communicate with GDB over a serial
  device or via the network.</entry>
</row>
<row>
<entry><filename>src/hal_if.c</filename></entry>
  <entry>ROM/RAM calling interface implementation. Provides wrappers from
  the calling interface API to the eCos features used for the
  implementation.</entry>
</row>
<row>
<entry><filename>src/hal_misc.c</filename></entry>
  <entry>Various helper functions shared by all platforms and
  architectures.</entry>
</row>
<row>
<entry><filename>src/hal_stub.c</filename></entry>
  <entry>Wrappers from eCos HAL features to the features required by the
  generic GDB stub.</entry>
</row>
<row>
<entry><filename>src/stubrom/stubrom.c</filename></entry>
  <entry>The file used to build eCos GDB stub images. Basically a
  cyg_start function with a hard coded breakpoint.</entry>
</row>
<row>
<entry><filename>src/thread-packets.c</filename></entry>
  <entry>More thread debugging related functions.</entry>
</row>
<row>
<entry><filename>src/thread-pkts.h</filename></entry>
  <entry>Defines more thread debugging related function.</entry>
</row>
</tbody>
</tgroup>
</informaltable>

</section>

<!-- }}} -->
<!-- {{{ Architecture HAL -->

<section>
<title>Architecture HAL</title>

<para>Some architecture HALs may add extra files for architecture
specific serial drivers, or for handling interrupts and exceptions if it
makes sense.</para>

<para>Note that many of the definitions in these files are only
conditionally defined - if the equivalent variant or platform headers
provide the definitions, those override the generic architecture
definitions.</para>

<informaltable frame=all>
<tgroup cols=2 align=left colsep=1 rowsep=1>
<thead>
<row>
<entry>File</entry>
<entry>Description</entry>
</row>
</thead>
<tbody>

<row>
<entry><filename>include/arch.inc</filename></entry>
  <entry>Various assembly macros used during system initialization.</entry>
</row>
<row>
<entry><filename>include/basetype.h</filename></entry>
  <entry>Endian, label, alignment, and type size definitions. These
  override common defaults in CYGPKG_INFRA.</entry>
</row>
<row>
<entry><filename>include/hal_arch.h</filename></entry>
  <entry>Saved register frame format, various thread, register and stack
  related macros.</entry>
</row>
<row>
<entry><filename>include/hal_cache.h</filename></entry>
  <entry>Cache definitions and cache control macros.</entry>
</row>
<row>
<entry><filename>include/hal_intr.h</filename></entry>
  <entry>Exception and interrupt definitions. Macros for configuring and
  controlling interrupts. eCos real-time clock control macros.</entry>
</row>
<row>
<entry><filename>include/hal_io.h</filename></entry>
  <entry>Macros for accessing IO devices.</entry>
</row>
<row>
<entry><filename>include/&lt;arch&gt;_regs.h</filename></entry>
  <entry>Architecture register definitions.</entry>
</row>
<row>
<entry><filename>include/&lt;arch&gt;_stub.h</filename></entry>
  <entry>Architecture stub definitions. In particular the register frame
  layout used by GDB. This may differ from the one used by eCos.</entry>
</row>
<row>
<entry><filename>include/&lt;arch&gt;.inc</filename></entry>
  <entry>Architecture convenience assembly macros.</entry>
</row>
<row>
<entry><filename>src/&lt;arch&gt;.ld</filename></entry>
  <entry>Linker macros.</entry>
</row>
<row>
<entry><filename>src/context.S</filename></entry>
  <entry>Functions handling context switching and setjmp/longjmp.</entry>
</row>
<row>
<entry><filename>src/hal_misc.c</filename></entry>
  <entry>Exception and interrupt handlers in C. Various other utility
  functions.</entry>
</row>
<row>
<entry><filename>src/hal_mk_defs.c</filename></entry>
  <entry>Used to export definitions from C header files to assembler
  header files.</entry>
</row>
<row>
<entry><filename>src/hal_intr.c</filename></entry>
  <entry>Any necessary interrupt handling functions.</entry>
</row>
<row>
<entry><filename>src/&lt;arch&gt;stub.c</filename></entry>
  <entry>Architecture stub code. Contains functions for translating eCos
  exceptions to UNIX signals and functions for single-stepping.</entry>
</row>
<row>
<entry><filename>src/vectors.S</filename></entry>
  <entry>Exception, interrupt and early initialization code.</entry>
</row>
</tbody>
</tgroup>
</informaltable>


</section>

<!-- }}} -->
<!-- {{{ Variant HAL -->

<section>
<title>Variant HAL</title>

<para>Some variant HALs may add extra files for variant specific serial
drivers, or for handling interrupts/exceptions if it makes sense.</para>

<para>Note that these files may be mostly empty if the CPU variant can be
controlled by the generic architecture macros. The definitions present
are only conditionally defined - if the equivalent platform headers
provide the definitions, those override the variant definitions.</para>

<informaltable frame=all>
<tgroup cols=2 align=left colsep=1 rowsep=1>
<thead>
<row>
<entry>File</entry>
<entry>Description</entry>
</row>
</thead>
<tbody>

<row>
<entry><filename>include/var_arch.h</filename></entry>
  <entry>Saved register frame format, various thread, register and stack
  related macros.</entry>
</row>
<row>
<entry><filename>include/var_cache.h</filename></entry>
  <entry>Cache related macros.</entry>
</row>
<row>
<entry><filename>include/var_intr.h</filename></entry>
  <entry>Interrupt related macros.</entry>
</row>
<row>
<entry><filename>include/var_regs.h</filename></entry>
  <entry>Extra register definitions for the CPU variant.</entry>
</row>
<row>
<entry><filename>include/variant.inc</filename></entry>
  <entry>Various assembly macros used during system initialization.</entry>
</row>
<row>
<entry><filename>src/var_intr.c</filename></entry>
  <entry>Interrupt functions if necessary.</entry>
</row>
<row>
<entry><filename>src/var_misc.c</filename></entry>
  <entry>hal_variant_init function and any necessary extra functions.</entry>
</row>
<row>
<entry><filename>src/variant.S</filename></entry>
  <entry>Interrupt handler table definition.</entry>
</row>
<row>
<entry><filename>src/&lt;arch&gt;_&lt;variant&gt;.ld</filename></entry>
  <entry>Linker macros.</entry>
</row>
</tbody>
</tgroup>
</informaltable>

</section>

<!-- }}} -->
<!-- {{{ Platform HAL -->

<section>
<title>Platform HAL</title>

<para>Extras files may be added for platform specific serial
drivers. Extra files for handling interrupts and exceptions will be
present if it makes sense.</para>

<informaltable frame=all>
<tgroup cols=2 align=left colsep=1 rowsep=1>
<thead>
<row>
<entry>File</entry>
<entry>Description</entry>
</row>
</thead>
<tbody>

<row>
<entry><filename>include/hal_diag.h</filename></entry>
  <entry>Defines functions used for HAL diagnostics output. This would
  normally be the ROM calling interface wrappers, but may also be the
  low-level IO functions themselves, saving a little overhead.</entry>
</row>
<row>
<entry><filename>include/platform.inc</filename></entry>

  <entry>Platform initialization code. This includes memory controller,
  vectors, and monitor initialization. Depending on the architecture,
  other things may need defining here as well: interrupt decoding,
  status register initialization value, etc.</entry>

</row>
<row>
<entry><filename>include/plf_cache.h</filename></entry>
  <entry>Platform specific cache handling.</entry>
</row>
<row>
<entry><filename>include/plf_intr.h</filename></entry>
  <entry>Platform specific interrupt handling.</entry>
</row>
<row>
<entry><filename>include/plf_io.h</filename></entry>
  <entry>PCI IO definitions and macros. May also be used to override
  generic HAL IO macros if the platform endianness differs from that of
  the CPU.</entry>
</row>
<row>
<entry><filename>include/plf_stub.h</filename></entry>
  <entry>Defines stub initializer and board reset details.</entry>
</row>
<row>
<entry><filename>src/hal_diag.c</filename></entry>
  <entry>May contain the low-level device drivers. But these may also
  reside in plf_stub.c</entry>
</row>
<row>
<entry><filename>src/platform.S</filename></entry>
  <entry>Memory controller setup macro, and if necessary interrupt
  springboard code.</entry>
</row>
<row>
<entry><filename>src/plf_misc.c</filename></entry>
  <entry>Platform initialization code.</entry>
</row>
<row>
<entry><filename>src/plf_mk_defs.c</filename></entry>
  <entry>Used to export definitions from C header files to assembler
  header files.</entry>
</row>
<row>
<entry><filename>src/plf_stub.c</filename></entry>
  <entry>Platform specific stub initialization and possibly the low-level
  device driver.</entry>
</row>
</tbody>
</tgroup>
</informaltable>

<para>The platform HAL also contains files specifying the platform's
memory layout. These files are located in
<filename>include/pkgconf</filename>.</para>

</section>

<!-- }}} -->
<!-- {{{ Auxiliary HAL -->

<section>
<title>Auxiliary HAL</title>

<para>Auxiliary HALs contain whatever files are necessary to provide the
required functionality. There are no predefined set of files required
in an auxiliary HAL.</para>

</section>

<!-- }}} -->

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ ROM Monitor Calling Interface -->

<section id="hal-calling-if">
<TITLE>Virtual Vectors (eCos/ROM Monitor Calling Interface)</TITLE>

<para>
Some eCos platforms have supported full debugging capabilities via
CygMon since day one. Platforms of the architectures PowerPC, ARM, and
SH do not provide those features unless a GDB stub is included in the
application.
</para>

<para>
This is going to change. All platforms will (eventually) support
all the debugging features by relying on a ROM/RAM calling interface
(also referred to as virtual vector table) provided by the ROM
monitor. This calling interface is based on the tables used by libbsp
and is thus backwards compatible with the existing CygMon supported
platforms.
</para>

<!-- {{{ Virtual Vectors -->

<section id="hal-porting-virtual-vectors">
<title>Virtual Vectors</title>

<para>What are virtual vectors, what do they do, and why are they
needed?
</para>

<para>
"Virtual vectors" is the name of a table located at a static
location in the target address space. This table contains 64 vectors
that point to <emphasis>service</emphasis> functions or data.
</para>

<para>The fact that the vectors are always placed at the same location in
the address space means that both ROM and RAM startup configurations
can access these and thus the services pointed to.</para>

<para>The primary goal is to allow services to be provided by ROM
configurations (ROM monitors such as RedBoot in particular) with
<emphasis>clients</emphasis> in RAM configurations being able to use these
services.</para>

<para>Without the table of pointers this would be impossible since the
ROM and RAM applications would be linked separately - in effect having
separate name spaces - preventing direct references from one to the
other.</para>

<para>This decoupling of service from client is needed by RedBoot,
allowing among other things debugging of applications which do not
contain debugging client code (stubs).</para>

<!-- {{{ Initialization -->

<section>
<title>Initialization (or Mechanism vs. Policy)</title>

<para>Virtual vectors are a <emphasis>mechanism</emphasis> for decoupling services
from clients in the address space.</para>

<para>The mechanism allows services to be implemented by a ROM
monitor, a RAM application, to be switched out at run-time, to be
disabled by installing pointers to dummy functions, etc.</para>

<para>The appropriate use of the mechanism is specified loosely by a
<emphasis>policy</emphasis>. The general policy dictates that the vectors are
initialized in whole by ROM monitors (built for ROM or RAM), or by
stand-alone applications.</para>

<para>For configurations relying on a ROM monitor environment, the policy
is to allow initialization on a service by service basis. The default
is to initialize all services, except COMMS services since these are
presumed to already be carrying a communication session to the
debugger / console which was used for launching the application.  This
means that the bulk of the code gets tested in normal builds, and not
just once in a blue moon when building new stubs or a ROM
configuration.</para>

<para>The configuration options are written to comply with this policy by
default, but can be overridden by the user if desired. Defaults
are:</para>

<itemizedlist>
<listitem><para>For application development: the ROM monitor provides
debugging and diagnostic IO services, the RAM application relies
on these by default.</para>
</listitem>
<listitem>
<para>For production systems: the application contains all the
necessary services.</para>
</listitem>

</itemizedlist>

</section>

<!-- }}} -->
<!-- {{{ Pros and Cons -->

<section>
<title>Pros and Cons of Virtual Vectors</title>

<para>
There are pros and cons associated with the use of virtual
vectors. We do believe that the pros generally outweigh the cons by a
great margin, but there may be situations where the opposite is
true.
</para>

<para>
The use of the services are implemented by way of macros, meaning
that it is possible to circumvent the virtual vectors if
desired. There is (as yet) no implementation for doing this, but it is
possible.
</para>

<para>Here is a list of pros and cons:</para>

<variablelist>
<varlistentry><term>Pro: Allows debugging without including stubs</term>

      <listitem><para>This is the primary reason for using virtual vectors. It
          allows the ROM monitor to provide most of the debugging
          infrastructure, requiring only the application to provide
          hooks for asynchronous debugger interrupts and for accessing
          kernel thread information.</para></listitem></varlistentry>

<varlistentry><term>Pro: Allows debugging to be initiated from arbitrary
       channel</term>

      <listitem><para> While this is only true where the application does not
           actively override the debugging channel setup, it is a very
           nice feature during development. In particular it makes it
           possible to launch (and/or debug) applications via Ethernet
           even though the application configuration does not contain
           networking support.</para></listitem></varlistentry>

<varlistentry><term>Pro: Image smaller due to services being provided by ROM
       monitor</term>

      <listitem><para>All service functions except HAL IO are included in the
           default configuration. But if these are all disabled the
           image for download will be a little smaller. Probably
           doesn't matter much for regular development, but it is a
           worthwhile saving for the 20000 daily tests run in the Red
           Hat eCos test farm.</para></listitem></varlistentry>

<varlistentry><term>Con: The vectors add a layer of indirection, increasing application
       size and reducing performance.</term>

      <listitem><para>The size increase is a fraction of what is required to
           implement the services. So for RAM configurations there is
           a net saving, while for ROM configurations there is a small
           overhead.</para>

      <para>The performance loss means little for most of the
           services (of which the most commonly used is diagnostic IO
           which happens via polled routines
           anyway).</para></listitem>
</varlistentry>

<varlistentry><term>Con: The layer of indirection is another point of
       failure.</term>

      <listitem><para> The concern primarily being that of vectors being
           trashed by rogue writes from bad code, causing a complete
           loss of the service and possibly a crash.  But this does
           not differ much from a rogue write to anywhere else in the
           address space which could cause the same amount of
           mayhem. But it is arguably an additional point of failure
           for the service in question.</para></listitem></varlistentry>

<varlistentry><term>Con: All the indirection stuff makes it harder to bring a HAL
       up</term>

      <listitem><para> This is a valid concern. However, seeing as most of the
           code in question is shared between all HALs and should
           remain unchanged over time, the risk of it being broken
           when a new HAL is being worked on should be
           minimal.</para>

      <para> When starting a new port, be sure to implement the HAL
           IO drivers according to the scheme used in other drivers,
           and there should be no problem.</para>

      <para> However, it is still possible to circumvent the vectors
           if they are suspect of causing problems: simply change the
           HAL_DIAG_INIT and HAL_DIAG_WRITE_CHAR macros to use the raw
           IO functions.</para></listitem></varlistentry>
</variablelist>

</section>

<!-- }}} -->
<!-- {{{ Available Services -->

<section>
<title>Available services</title>

<para>
The <filename>hal_if.h</filename> file in the common HAL defines the
complete list of available services. A few worth mentioning in
particular:</para>

<itemizedlist>
<listitem> <para>COMMS services. All HAL IO happens via the communication
        channels.</para>
</listitem>	
<listitem> <para>uS delay. Fine granularity (busy wait) delay function.</para>
</listitem>	
<listitem> <para>Reset. Allows a software initiated reset of the board.</para>
</listitem>	
</itemizedlist>

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ The COMMS Channels -->

<section>
<title>The COMMS channels</title>

<para>As all HAL IO happens via the COMMS channels these deserve to be
described in a little more detail. In particular the controls of where
diagnostic output is routed and how it is treated to allow for display
in debuggers.</para>

<!-- {{{ Console and Debuggers Channels -->

<section>
<title>Console and Debugging Channels</title>

<para>There are two COMMS channels - one for console IO and one for
debugging IO. They can be individually configured to use any of the
actual IO ports (serial or Ethernet) available on the platform.</para>

<para>The console channel is used for any IO initiated by calling the
<function>diag_*()</function> functions. Note that these should only be used during
development for debugging, assertion and possibly tracing
messages. All proper IO should happen via proper devices. This means
it should be possible to remove the HAL device drivers from production
configurations where assertions are disabled.</para>

<para>The debugging channel is used for communication between the
debugger and the stub which remotely controls the target for the
debugger (the stub runs on the target). This usually happens via some
protocol, encoding commands and replies in some suitable form.</para>

<para>Having two separate channels allows, e.g., for simple logging
without conflicts with the debugger or interactive IO which some
debuggers do not allow.</para>

</section>

<!-- }}} --> 
<!-- {{{ Mangling -->

<section>
<title>Mangling</title>

<para>As debuggers usually have a protocol using specialized commands
when communicating with the stub on the target, sending out text as
raw ASCII from the target on the same channel will either result in
protocol errors (with loss of control over the target) or the text may
just be ignored as junk by the debugger.</para>

<para>To get around this, some debuggers have a special command for text
output. Mangling is the process of encoding diagnostic ASCII text
output in the form specified by the debugger protocol.</para>

<para>When it is necessary to use mangling, i.e. when writing console
output to the same port used for debugging, a mangler function is
installed on the console channel which mangles the text and passes it
on to the debugger channel.</para>

</section>

<!-- }}} -->
<!-- {{{ Controlling the Console Channel -->

<section>
<title>Controlling the Console Channel</title>

<para>Console output configuration is either inherited from the ROM
monitor launching the application, or it is specified by the
application. This is controlled by the new option
<literal>CYGSEM_HAL_VIRTUAL_VECTOR_INHERIT_CONSOLE</literal> which
defaults to enabled when the configuration is set to use a ROM
monitor.</para>

<para>If the user wants to specify the console configuration in the
application image, there are two new options that are used for
this.</para>

<para>Defaults are to direct diagnostic output via a mangler to the
debugging channel (<literal>CYGDBG_HAL_DIAG_TO_DEBUG_CHAN</literal>
enabled). The mangler type is controlled by the option
<literal>CYGSEM_HAL_DIAG_MANGLER</literal>. At present there are only
two mangler types:</para>

<variablelist>
<varlistentry><term><acronym>GDB</acronym></term>

  <listitem><para> This causes a mangler appropriate for debugging with GDB to be
       installed on the console channel.</para></listitem></varlistentry>

<varlistentry><term>None</term>

   <listitem><para> This causes a NULL mangler to be installed on the console
        channel.  It will redirect the IO to/from the debug channel
        without mangling of the data. This option differs from setting
        the console channel to the same IO port as the debugging
        channel in that it will keep redirecting data to the debugging
        channel even if that is changed to some other port.</para></listitem></varlistentry>

</variablelist>

<para>Finally, by disabling <literal>CYGDBG_HAL_DIAG_TO_DEBUG_CHAN</literal>, the diagnostic
output is directed in raw form to the specified console IO port.</para>

<para>In summary this results in the following common configuration
scenarios for RAM startup configurations:</para>

<itemizedlist>
<listitem><para> For regular debugging with diagnostic output appearing in the
     debugger, mangling is enabled and stubs disabled.</para>

     <para>Diagnostic output appears via the debugging channel as
     initiated by the ROM monitor, allowing for correct behavior
     whether the application was launched via serial or Ethernet, from
     the RedBoot command line or from a debugger.</para>
</listitem>

<listitem><para> For debugging with raw diagnostic output, mangling is
     disabled.</para>

     <para> Debugging session continues as initiated by the ROM monitor,
     whether the application was launched via serial or
     Ethernet. Diagnostic output is directed at the IO port configured
     in the application configuration.</para>

     <note>
     <title>Note:</title>
     <para> There is one caveat to be aware of. If the
       application uses proper devices (be it serial or Ethernet) on
       the same ports as those used by the ROM monitor, the
       connections initiated by the ROM monitor will be
       terminated.</para>
     </note>
</listitem>

</itemizedlist>

<para>And for ROM startup configurations:</para>

<itemizedlist>
<listitem><para> Production configuration with raw output and no debugging
     features (configured for RAM or ROM), mangling is disabled, no
     stubs are included.</para>

     <para>Diagnostic output appears (in unmangled form) on the specified
     IO port.</para>
</listitem>

<listitem><para> RedBoot configuration, includes debugging features and necessary
     mangling.</para>

     <para>Diagnostic and debugging output port is auto-selected by the
     first connection to any of the supported IO ports. Can change
     from interactive mode to debugging mode when a debugger is
     detected - when this happens a mangler will be installed as
     required.</para>
</listitem>

<listitem><para> GDB stubs configuration (obsoleted by RedBoot configuration),
     includes debugging features, mangling is hardwired to GDB
     protocol.</para>

     <para>Diagnostic and debugging output is hardwired to configured IO
     ports, mangling is hardwired.</para>
</listitem>

</itemizedlist>
</section>

<!-- }}} -->
<!-- {{{ Footnote: Design Reasoning -->

<section>
<title>Footnote: Design Reasoning for Control of Console Channel</title>

<para>The current code for controlling the console channel is a
replacement for an older implementation which had some shortcomings
which addressed by the new implementation.</para>

<para>This is what the old implementation did: on initialization it would
check if the CDL configured console channel differed from the active
debug channel - and if so, set the console channel, thereby disabling
mangling.</para>

<para>The idea was that whatever channel was configured to be used for
console (i.e., diagnostic output) in the application was what should
be used. Also, it meant that if debug and console channels were
normally the same, a changed console channel would imply a request for
unmangled output.</para>

<para>But this prevented at least two things:</para>

<itemizedlist>
<listitem><para> It was impossible to inherit the existing connection by which
     the application was launched (either by RedBoot commands via
     telnet, or by via a debugger).</para>

     <para>This was mostly a problem on targets supporting Ethernet
     access since the diagnostic output would not be returned via the
     Ethernet connection, but on the configured serial port.</para>

     <para>The problem also occurred on any targets with multiple serial
     ports where the ROM monitor was configured to use a different
     port than the CDL defaults.</para>
</listitem>

<listitem><para> Proper control of when to mangle or just write out raw ASCII
        text.</para>

     <para>Sometimes it's desirable to disable mangling, even if the
     channel specified is the same as that used for debugging. This
     usually happens if GDB is used to download the application, but
     direct interaction with the application on the same channel is
     desired (GDB protocol only allows output from the target, no
     input).</para>
</listitem>     
</itemizedlist>

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ The Calling Interface API -->

<section>
<title>The calling Interface API</title>

<para>The calling interface API is defined by hal_if.h and hal_if.c in
hal/common.</para>

<para>The API provides a set of services. Different platforms, or
different versions of the ROM monitor for a single platform, may
implement fewer or extra service. The table has room for growth, and
any entries which are not supported map to a NOP-service (when called
it returns 0 (<literal>false</literal>)).
</para>

<para>A client of a service should either be selected by configuration,
or have suitable fall back alternatives in case the feature is not
implemented by the ROM monitor.
</para>

<note>
<title>Note:</title>
<para>
Checking for unimplemented service when this may be a data
field/pointer instead of a function: suggest reserving the last entry
in the table as the NOP-service pointer. Then clients can compare a
service entry with this pointer to determine whether it's initialized
or not.
</para>
</note>

<para>The header file <filename>cyg/hal/hal_if.h</filename> defines
 the table layout and accessor macros (allowing primitive type
 checking and alternative implementations should it become necessary).
</para>

<para>The source file <filename>hal_if.c</filename> defines the table
 initialization function. All HALs should call this during platform
 initialization - the table will get initialized according to
 configuration.  Also defined here are wrapper functions which map
 between the calling interface API and the API of the used eCos
 functions.
</para>

<!-- {{{ Implemented Services -->

<section>
<title>Implemented Services</title>

<para>This is a brief description of the services, some of which are
described in further detail below.</para>

<variablelist>
<varlistentry><term><literal>VERSION</literal></term>
        <listitem><para>Version of table. Serves as a way to check for how many
        features are available in the table. This is the index of the
        last service in the table.</para></listitem></varlistentry>
<varlistentry><term><literal>KILL_VECTOR</literal></term>
        <listitem><para>[Presently unused by the stub code, but initialized] This
        vector defines a function to execute when the system receives
        a kill signal from the debugger. It is initialized with the
        reset function (see below), but the application (or eCos) can
        override it if necessary.</para></listitem></varlistentry>
<varlistentry><term><literal>CONSOLE_PROCS</literal></term>
        <listitem><para>The communication procedure table used for console IO
        (see <xref linkend="hal-porting-io-channels">.</para></listitem></varlistentry>
<varlistentry><term><literal>DEBUG_PROCS</literal></term>
        <listitem><para>The communication procedure table used for debugger IO
        (see <xref linkend="hal-porting-io-channels">).</para></listitem></varlistentry>
<varlistentry><term><literal>FLUSH_DCACHE</literal></term>
        <listitem><para>Flushes the data cache for the specified
        region. Some implementations may flush the entire data cache.</para></listitem></varlistentry>
<varlistentry><term><literal>FLUSH_ICACHE</literal></term>
        <listitem><para>Flushes (invalidates) the instruction cache
        for the specified region. Some implementations may flush the
        entire instruction cache.</para></listitem></varlistentry>
<varlistentry><term><literal>SET_DEBUG_COMM</literal></term>
        <listitem><para>Change debugging communication channel.</para></listitem></varlistentry>
<varlistentry><term><literal>SET_CONSOLE_COMM</literal></term>
        <listitem><para>Change console communication channel.</para></listitem></varlistentry>
<varlistentry><term><literal>DBG_SYSCALL</literal></term>
        <listitem><para>Vector used to communication between debugger functions in
        ROM and in RAM. RAM eCos configurations may install a function
        pointer here which the ROM monitor uses to get thread
        information from the kernel running in RAM.</para></listitem></varlistentry>
<varlistentry><term><literal>RESET</literal></term>
        <listitem><para>Resets the board on call. If it is not possible to reset
        the board from software, it will jump to the ROM entry point
        which will perform a "software" reset of the board.</para></listitem></varlistentry>
<varlistentry><term><literal>CONSOLE_INTERRUPT_FLAG</literal></term>
        <listitem><para>Set if a debugger interrupt request was detected while
        processing console IO. Allows the actual breakpoint action to
        be handled after return to RAM, ensuring proper backtraces
        etc.</para></listitem></varlistentry>
<varlistentry><term><literal>DELAY_US</literal></term>
        <listitem><para>Will delay the specified number of microseconds. The
        precision is platform dependent to some extend - a small value
        (<100us) is likely to cause bigger delays than requested.</para></listitem></varlistentry>
<varlistentry><term><literal>FLASH_CFG_OP</literal></term>
        <listitem><para>For accessing configuration settings kept in flash memory.</para></listitem></varlistentry>
<varlistentry><term><literal>INSTALL_BPT_FN</literal></term>
        <listitem><para>Installs a breakpoint at the specified address. This is
        used by the asynchronous breakpoint support
	(see <!-- <xref linkend="hal-stubs-async-bps"> -->).</para></listitem></varlistentry>
</variablelist>
</section>

<!-- }}} -->
<!-- {{{ Compatibility -->

<section>
<title>Compatibility</title>

<para>When a platform is changed to support the calling interface,
applications will use it if so configured. That means that if an
application is run on a platform with an older ROM monitor, the
service is almost guaranteed to fail.
</para>

<para>For this reason, applications should only use Console Comm for HAL
diagnostics output if explicitly configured to do so
(<literal>CYGSEM_HAL_VIRTUAL_VECTOR_DIAG</literal>).
</para>

<para>As for asynchronous GDB interrupts, the service will always be
used. This is likely to cause a crash under older ROM monitors, but
this crash may be caught by the debugger. The old workaround still
applies: if you need asynchronous breakpoints or thread debugging
under older ROM monitors, you may have to include the debugging
support when configuring eCos.
</para>

</section>

<!-- }}} -->
<!-- {{{ Implementation Details -->

<section>
<title>Implementation details</title>

<para>During the startup of a ROM monitor, the calling table will be
initialized. This also happens if eCos is configured <emphasis>not</emphasis> to rely on
a ROM monitor.
</para>

<note>
<title>Note:</title>
<para> There is reserved space (256 bytes) for the vector
table whether it gets used or not. This may be something that we want
to change if we ever have to shave off every last byte for a given
target.
</para>
</note>

<para>If thread debugging features are enabled, the function for accessing
the thread information gets registered in the table during startup of
a RAM startup configuration.
</para>

<para>Further implementation details are described where the service itself
is described.</para>

<!-- 
FIXME: Need to describe the CYGARC_HAL_SAVE_GP() and
CYGARC_HAL_RESTORE_GP() macros.
-->

</section>

<!-- }}} -->
<!-- {{{ New Platform Ports -->

<section>
<title>New Platform Ports</title>

<para>The <function>hal_platform_init()</function> function must call
<function>hal_if_init()</function>.
</para>

<para>The HAL serial driver must, when called via
<function>cyg_hal_plf_comms_init()</function> must initialize the
communication channels.
</para>

<para>The <function>reset()</function> function defined in
<filename>hal_if.c</filename> will attempt to do a hardware reset, but
if this fails it will fall back to simply jumping to the reset
entry-point. On most platforms the startup initialization will go a
long way to reset the target to a sane state (there will be
exceptions, of course). For this reason, make sure to define
<literal>HAL_STUB_PLATFORM_RESET_ENTRY</literal> in plf_stub.h.
</para>

<para>All debugging features must be in place in order for the debugging
services to be functional. See general platform porting notes.
</para>

</section>

<!-- }}} -->
<!-- {{{ New Architecture Ports -->

<section>
<title>New architecture ports</title>

<para>There are no specific requirements for a new architecture port in
order to support the calling interface, but the basic debugging
features must be in place. See general architecture porting notes.
</para>
</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ IO Channels -->

<section id="hal-porting-io-channels">
<title>IO channels</title>


<para>The calling interface provides procedure tables for all IO channels on
the platform. These are used for console (diagnostic) and debugger IO,
allowing a ROM monitor to provided all the needed IO routines. At
the same time, this makes it easy to switch console/debugger channels
at run-time (the old implementation had hardwired drivers for console
and debugger IO, preventing these to change at run-time).
</para>

<para>The hal_if provides wrappers which interface these services to the
eCos infrastructure diagnostics routines. This is done in a way which
ensures proper string mangling of the diagnostics output when required
(e.g. O-packetization when using a GDB compatible ROM monitor).
</para>

<!-- {{{ Available Procedures -->

<section>
<title>Available Procedures</title>

<para>This is a brief description of the procedures</para>

<variablelist>
<varlistentry><term><literal>CH_DATA</literal></term>
<listitem><para>Pointer to the controller IO base (or a pointer to a per-device
    structure if more data than the IO base is required). All the
    procedures below are called with this data item as the first
    argument.</para></listitem></varlistentry>

<varlistentry><term><literal>WRITE</literal></term>
        <listitem><para>Writes the buffer to the device.</para></listitem></varlistentry>
<varlistentry><term><literal>READ</literal></term>
        <listitem><para>Fills a buffer from the device.</para></listitem></varlistentry>
<varlistentry><term><literal>PUTC</literal></term>
        <listitem><para>Write a character to the device.</para></listitem></varlistentry>
<varlistentry><term><literal>GETC</literal></term>
        <listitem><para>Read a character from the device.</para></listitem></varlistentry>
<varlistentry><term><literal>CONTROL</literal></term>
        <listitem><para>Device feature control. Second argument specifies function:</para>
  <variablelist>
    <varlistentry><term><literal>SETBAUD</literal></term>
        <listitem><para>Changes baud rate.</para></listitem></varlistentry>
    <varlistentry><term><literal>GETBAUD</literal></term>
        <listitem><para>Returns the current baud rate.</para></listitem></varlistentry>
    <varlistentry><term><literal>INSTALL_DBG_ISR</literal></term>
        <listitem><para>[Unused]</para></listitem></varlistentry>
    <varlistentry><term><literal>REMOVE_DBG_ISR</literal></term>
        <listitem><para>[Unused]</para></listitem></varlistentry>
    <varlistentry><term><literal>IRQ_DISABLE</literal></term>
        <listitem><para>Disable debugging receive interrupts on the device.</para></listitem></varlistentry>
    <varlistentry><term><literal>IRQ_ENABLE</literal></term>
        <listitem><para>Enable debugging receive interrupts on the device.</para></listitem></varlistentry>
    <varlistentry><term><literal>DBG_ISR_VECTOR</literal></term>
        <listitem><para>Returns the ISR vector used by the device for debugging
        receive interrupts.</para></listitem></varlistentry>
    <varlistentry><term><literal>SET_TIMEOUT</literal></term>
        <listitem><para>Set GETC timeout in milliseconds.</para></listitem></varlistentry>
    <varlistentry><term><literal>FLUSH_OUTPUT</literal></term>
        <listitem><para>Forces driver to flush data in its buffers. Note
            that this may not affect hardware buffers
        (e.g. FIFOs).</para></listitem></varlistentry>
   </variablelist>
   </listitem></varlistentry>
   
<varlistentry><term><literal>DBG_ISR</literal></term>
        <listitem><para>ISR used to handle receive interrupts from the
	device (see <!-- <xref linkend="hal-stubs-async-bps"> -->).</para></listitem></varlistentry>
<varlistentry><term><literal>GETC_TIMEOUT</literal></term>
        <listitem><para>Read a character from the device with timeout.</para></listitem></varlistentry>
</variablelist>

</section>

<!-- }}} -->
<!-- {{{ Usage -->

<section><title>Usage</title>

<para>The standard eCos diagnostics IO functions use the channel
procedure table when <literal>CYGSEM_HAL_VIRTUAL_VECTOR_DIAG</literal> is enabled. That
means that when you use diag_printf (or the libc printf function) the
stream goes through the selected console procedure table. If you use
the virtual vector function SET_CONSOLE_COMM you can change the device
which the diagnostics output goes to at run-time.</para>

<para>You can also use the table functions directly if desired
(regardless of the <literal>CYGSEM_HAL_VIRTUAL_VECTOR_DIAG</literal> setting - assuming
the ROM monitor provides the services). Here is a small example which
changes the console to use channel 2, fetches the comm procs pointer
and calls the write function from that table, then restores the
console to the original channel:</para>

<programlisting>
#define T "Hello World!\n"

int
main(void)
{
    hal_virtual_comm_table_t* comm;
    int cur = CYGACC_CALL_IF_SET_CONSOLE_COMM(CYGNUM_CALL_IF_SET_COMM_ID_QUERY_CURRENT);

    CYGACC_CALL_IF_SET_CONSOLE_COMM(2);

    comm = CYGACC_CALL_IF_CONSOLE_PROCS();
    CYGACC_COMM_IF_WRITE(*comm, T, strlen(T));

    CYGACC_CALL_IF_SET_CONSOLE_COMM(cur);
}
</programlisting>

<para>Beware that if doing something like the above, you should only do
it to a channel which does not have GDB at the other end: GDB ignores
raw data, so you would not see the output.</para>

</section>

<!-- }}} --> 
<!-- {{{ Compatibility -->

<section>
<title>Compatibility</title>

<para>The use of this service is controlled by the option
<literal>CYGSEM_HAL_VIRTUAL_VECTOR_DIAG</literal> which is disabled per default on most
older platforms (thus preserving backwards compatibility with older
stubs). On newer ports, this option should always be set.
</para>
</section>

<!-- }}} -->
<!-- {{{ Implementation Details -->

<section><title>Implementation Details</title>

<para>There is an array of procedure tables (raw comm channels) for each
IO device of the platform which get initialized by the ROM monitor, or
optionally by a RAM startup configuration (allowing the RAM
configuration to take full control of the target).  In addition to
this, there's a special table which is used to hold mangler
procedures.</para>

<para>The vector table defines which of these channels are selected for
console and debugging IO respectively: console entry can be empty,
point to mangler channel, or point to a raw channel. The debugger
entry should always point to a raw channel.</para>

<para>During normal console output (i.e., diagnostic output) the console
table will be used to handle IO if defined. If not defined, the debug
table will be used.</para>

<para>This means that debuggers (such as GDB) which require text streams
to be mangled (O-packetized in the case of GDB), can rely on the ROM
monitor install mangling IO routines in the special mangler table and
select this for console output. The mangler will pass the mangled data
on to the selected debugging channel.</para>

<para>If the eCos configuration specifies a different console channel
from that used by the debugger, the console entry will point to the
selected raw channel, thus overriding any mangler provided by the ROM
monitor.</para>

<para>See hal_if_diag_* routines in hal_if.c for more details of the stream
path of diagnostic output. See <function>cyg_hal_gdb_diag_*()</function> routines in
<filename>hal_stub.c</filename> for the mangler used for GDB communication.</para>

<!--
FIXME: Other special channels are reserved for ethernet communication.
-->

</section>

<!-- }}} -->
<!-- {{{ New Platform Ports -->

<section>
<title>New Platform Ports</title>

<para>Define CDL options <literal>CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS</literal>,
<literal>CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL</literal>, and
<literal>CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL</literal>.
</para>

<para>If <literal>CYGSEM_HAL_VIRTUAL_VECTOR_DIAG</literal> is set, make sure the infra diag
code uses the hal_if diag functions:</para>

<programlisting>
 #define HAL_DIAG_INIT() hal_if_diag_init()
 #define HAL_DIAG_WRITE_CHAR(_c_) hal_if_diag_write_char(_c_)
 #define HAL_DIAG_READ_CHAR(_c_) hal_if_diag_read_char(&_c_)
</programlisting>

<para>In addition to the above functions, the platform HAL must also
provide a function cyg_hal_plf_comms_init which initializes the
drivers and the channel procedure tables.
</para>

<para>Most of the other functionality in the table is more or less
possible to copy unchanged from existing ports. Some care is necessary
though to ensure the proper handling of interrupt vectors and timeouts
for various devices handled by the same driver. See PowerPC/Cogent
platform HAL for an example implementation.</para>

<note>
<title>Note:</title>
<para> When vector table console code is <emphasis>not</emphasis> used,
the platform HAL must map the HAL_DIAG_INIT, HAL_DIAG_WRITE_CHAR and
HAL_DIAG_READ_CHAR macros directly to the low-level IO functions,
hardwired to use a compile-time configured channel.</para>
</note>

<note>
<title>Note:</title>
<para> On old ports the hardwired <literal>HAL_DIAG_INIT</literal>,
<literal>HAL_DIAG_WRITE_CHAR</literal> and
<literal>HAL_DIAG_READ_CHAR</literal> implementations will also
contain code to O-packetize the output for GDB. This should
<emphasis>not</emphasis> be adopted for new ports! On new ports the
ROM monitor is guaranteed to provide the necessary mangling via the
vector table. The hardwired configuration should be reserved for ROM
startups where achieving minimal image size is crucial.
</para>
</note>

</section>

<!-- }}} -->

</section>

<!-- }}} -->


</section>

<!-- }}} -->
<!-- {{{ Coding Conventions  -->

<section id="hal-porting-coding-conventions">
<TITLE>HAL Coding Conventions</TITLE>


<para>
To get changes and larger submissions included into the eCos source
repository, we ask that you adhere to a set of coding conventions.
The conventions are defined as an attempt to make a consistent
tree. Consistency makes it easier for people to read, understand and
maintain the code, which is important when many people work on the
same project.
</para>

<para>
The below is only a brief, and probably incomplete, summary of the
rules. Please look through files in the area where you are making
changes to get a feel for any additional conventions. Also feel free
to ask on the list if you have specific questions.
</para>


<section>
<title>Implementation issues</title>

<para>
There are a few implementation issues that should be kept in mind:
</para>

<variablelist>
<varlistentry><term>HALs</term>
	<listitem><para>HALs must be written in C and assembly only. C++ must not
	be used. This is in part to keep the HALs simple since this is
	usually the first part of eCos a newcomer will see, and in
	part to maintain the existing de facto standard.</para></listitem></varlistentry>

<varlistentry><term>IO access</term>
	<listitem><para>Use HAL IO access macros for code that might be reused on
	different platforms than the one you are writing it for.</para></listitem></varlistentry>

<varlistentry><term>MMU</term>
	<listitem><para>If it is necessary to use the MMU (e.g., to prevent
	caching of IO areas), use a simple 1-1 mapping of memory if
	possible. On most platforms where using the MMU is necessary,
	it will be possible to achieve the 1-1 mapping using the MMU's
	provision for mapping large continuous areas (hardwired TLBs or
	BATs). This reduces the footprint (no MMU table) and avoids
	execution overhead (no MMU-related exceptions).</para></listitem></varlistentry>

<varlistentry><term>Assertions</term> 
        <listitem><para>The code should contain assertions to validate argument
	values, state information and any assumptions the code may be
	making. Assertions are not enabled in production builds, so
	liberally sprinkling assertions throughout the code is
	good.</para></listitem></varlistentry>

<varlistentry><term>Testing</term>
	<listitem><para>The ability to test your code is very important. In
	general, do not add new code to the eCos runtime unless you
	also add a new test to exercise that code. The test also
	serves as an example of how to use the new code.</para></listitem></varlistentry>

</variablelist>

</section>

<section>
<title>Source code details</title>

<variablelist>
<varlistentry><term>Line length</term> 
	<listitem><para>Keep line length below 78 columns whenever possible.</para></listitem></varlistentry>

<varlistentry><term>Comments</term>
	<listitem><para>Whenever possible, use // comments instead of /**/.</para></listitem></varlistentry>

<varlistentry><term>Indentation</term>
	<listitem><para>Use spaces instead of TABs. Indentation level is 4. Braces
	start on the same line as the expression. See below for emacs
	mode details.</para>

<programlisting>
;;=================================================================
;; eCos C/C++ mode Setup.
;;
;; bsd mode: indent = 4
;; tail comments are at col 40.
;; uses spaces not tabs in C

(defun ecos-c-mode ()
  "C mode with adjusted defaults for use with the eCos sources."
  (interactive)
  (c++-mode)
  (c-set-style "bsd")
  (setq comment-column 40)
  (setq indent-tabs-mode nil)
  (show-paren-mode 1)
  (setq c-basic-offset 4)

  (set-variable 'add-log-full-name "Your Name")
  (set-variable 'add-log-mailing-address "Your email address"))

(defun ecos-asm-mode ()
  "ASM mode with adjusted defaults for use with the eCos sources."
  (interactive)
  (setq comment-column 40)
  (setq indent-tabs-mode nil)
  (asm-mode)
  (setq c-basic-offset 4)

  (set-variable 'add-log-full-name "Your Name")
  (set-variable 'add-log-mailing-address "Your email address"))

(setq auto-mode-alist
      (append '(("/local/ecc/.*\\.C$"   . ecos-c-mode)
                ("/local/ecc/.*\\.cc$"  . ecos-c-mode)
                ("/local/ecc/.*\\.cpp$" . ecos-c-mode)
                ("/local/ecc/.*\\.inl$" . ecos-c-mode)
                ("/local/ecc/.*\\.c$"   . ecos-c-mode)
                ("/local/ecc/.*\\.h$"   . ecos-c-mode)
		("/local/ecc/.*\\.S$"   . ecos-asm-mode) 
		("/local/ecc/.*\\.inc$" . ecos-asm-mode)
		("/local/ecc/.*\\.cdl$" . tcl-mode)
                ) auto-mode-alist))
</programlisting>
</listitem>
</varlistentry>
</variablelist>
</section>

<section>

<title>Nested Headers</title>

<para>In order to allow platforms to define all necessary details, while
still maintaining the ability to share code between common platforms,
all HAL headers are included in a nested fashion.</para>

<para>The architecture header (usually <filename>hal_XXX.h</filename>) includes the
variant equivalent of the header (<filename>var_XXX.h</filename>) which in turn
includes the platform equivalent of the header
(<filename>plf_XXX.h</filename>).</para>

<para>All definitions that may need to be overridden by a platform are
then only conditionally defined, depending on whether a lower layer
has already made the definition:</para>

<programlisting>
hal_intr.h:     #include &lt;var_intr.h&gt;

                #ifndef MACRO_DEFINED
                # define MACRO ...
                # define MACRO_DEFINED
                #endif



var_intr.h:     #include &lt;plf_intr.h&gt;

                #ifndef MACRO_DEFINED
                # define MACRO ...
                # define MACRO_DEFINED
                #endif


plf_intr.h:

                # define MACRO ...
                # define MACRO_DEFINED
</programlisting>

<para>This means a platform can opt to rely on the variant or
architecture implementation of a feature, or implement it itself.</para>

</section>

</section>

<!-- }}} -->
<!-- {{{ Platform HAL Porting -->

<section id="hal-porting-platform">
<title>Platform HAL Porting</title>

<para>
This is the type of port that takes the least effort. It basically
consists of describing the platform (board) for the HAL: memory
layout, early platform initialization, interrupt controllers, and a
simple serial device driver.
</para>

<para>
Doing a platform port requires a preexisting architecture and
possibly a variant HAL port.
</para>

<!-- {{{ Porting Process -->

<section>
<TITLE>HAL Platform Porting Process</TITLE>

<!-- {{{ Brief Overview -->

<section>
<title>Brief overview</title>

<para>The easiest way to make a new platform HAL is simply to copy an
existing platform HAL of the same architecture/variant and change all
the files to match the new one. In case this is the first platform for
the architecture/variant, a platform HAL from another architecture
should be used as a template.
</para>

<para>
The best way to start a platform port is to concentrate on getting
RedBoot to run. RedBoot is a simpler environment than full eCos, it
does not use interrupts or threads, but covers most of the
basic startup requirements.
</para>

<para>
RedBoot normally runs out of FLASH or ROM and provides program loading
and debugging facilities.  This allows further HAL development to
happen using RAM startup configurations, which is desirable for the
simple reason that downloading an image which you need to test is
often many times faster than either updating a flash part, or indeed,
erasing and reprogramming an EPROM.
</para>

<para>There are two approaches to getting to this first goal:
</para>

<orderedlist>
<listitem>
<para>
The board is equipped with a ROM monitor which allows "load and go" of
ELF, binary, S-record or some other image type which can be created
using <application>objcopy</application>. This allows you to develop
RedBoot by downloading and running the code (saving time).
</para>

<para>
When the stub is running it is a good idea to examine the various
hardware registers to help you write the platform initialization code.
</para>

<para>
Then you may have to fiddle a bit going through step two (getting it
to run from ROM startup). If at all possible, preserve the original
ROM monitor so you can revert to it if necessary.
</para>
</listitem>

<listitem>
<para>
The board has no ROM monitor. You need to get the platform
initialization and stub working by repeatedly making changes, updating
flash or EPROM and testing the changes. If you are lucky, you have a
JTAG or similar CPU debugger to help you. If not, you will probably
learn to appreciate LEDs. This approach may also be needed during the
initial phase of moving RedBoot from RAM startup to ROM, since it is
very unlikely to work first time.
</para>
</listitem>
</orderedlist>

</section>

<!-- }}} -->
<!-- {{{ Step-by-step -->

<section>
<title>Step-by-step</title>

<para>Given that no two platforms are exactly the same, you may have to
deviate from the below. Also, you should expect a fair amount of
fiddling - things almost never go right the first time. See the hints
section below for some suggestions that might help debugging.
</para>

<para>The description below is based on the HAL layout used in the MIPS,
PC and MN10300 HALs. Eventually all HALs should be converted to look like
these - but in a transition period there will be other HALs which look
substantially different. Please try to adhere to the following as much is
possible without causing yourself too much grief integrating with a
HAL which does not follow this layout.
</para>

<!-- ====================================================================== -->

<section>
<title>Minimal requirements</title>

<para>
These are the changes you must make before you attempt to build
RedBoot. You are advised to read all the sources though.
</para>

<orderedlist>
<listitem><para>Copy an existing platform HAL from the same or another
    architecture. Rename the files as necessary to follow the
    standard: CDL and MLT related files should contain the
    &lt;arch&gt;_&lt;variant&gt;_&lt;platform&gt; triplet.</para>
</listitem>

<listitem><para>Adjust CDL options. Primarily option naming, real-time
    clock/counter, and CYGHWR_MEMORY_LAYOUT variables, but also other
    options may need editing. Look through the architecture/variant
    CDL files to see if there are any requirements/features which
    where not used on the platform you copied. If so, add appropriate
    ones. See <xref linkend="hal-porting-cdl-requirements"> for more
    details.</para>
</listitem>

<listitem><para>Add the necessary packages and target descriptions to the
    top-level <filename>ecos.db</filename> file. See <xref
    linkend="hal-porting-ecos-database">. Initially, the target entry
    should only contain the HAL packages. Other hardware support
    packages will be added later.</para>
</listitem>

<listitem><para>Adjust the MLT files in
    <filename>include/pkgconf</filename> to match the memory layout on
    the platform. For initial testing it should be enough to just hand
    edit .h and .ldi files, but eventually you should generate all
    files using the memory layout editor in the configuration
    tool. See <xref linkend="hal-porting-platform-memory-layout"> for
    more details.</para>
</listitem>

<listitem>
    <para>
    Edit the <filename>misc/redboot_&lt;STARTUP&gt;.ecm</filename> for
    the startup type you have chosen to begin with. Rename any
    platform specific options and remove any that do not apply. In the
    <literal>cdl_configuration</literal> section, comment out any
    extra packages that are added, particularly packages such as
    <literal>CYGPKG_IO_FLASH</literal> and
    <literal>CYGPKG_IO_ETH_DRIVERS</literal>. These are not needed for
    initial porting and will be added back later.
    </para>
</listitem>

<listitem><para>If the default IO macros are not correct, override them in
    plf_io.h. This may be necessary if the platform uses a different
    endianness from the default for the CPU.</para>
</listitem>

<listitem><para>Leave out/comment out code that enables caches and/or MMU if
    possible. Execution speed will not be a concern until the port is
    feature complete.</para>
</listitem>

<listitem><para>Implement a simple serial driver (polled mode only). Make sure the
    initialization function properly hooks the procedures up in the
    virtual vector IO channel tables. RedBoot will call the serial
    driver via these tables.</para>
    <para>
    By copying an existing platform HAL most of this code will be
    already done, and will only need the platform specific hardware
    access code to be written.
    </para>
</listitem>

<listitem><para>Adjust/implement necessary platform
    initialization. This can be found in
    <filename>platform.inc</filename> and
    <filename>platform.S</filename> files (ARM:
    <filename>hal_platform_setup.h</filename> and
    <filename>&lt;platform&gt;_misc.c</filename>, PowerPC:
    <filename>&lt;platform&gt;.S</filename>). This step can be
    postponed if you are doing a RAM startup RedBoot first and the
    existing ROM monitor handles board initialization.</para>
</listitem>

<listitem><para>Define <literal>HAL_STUB_PLATFORM_RESET</literal>
    (optionally empty) and
    <literal>HAL_STUB_PLATFORM_RESET_ENTRY</literal> so that RedBoot
    can reset-on-detach - this is very handy, often removing the need
    for physically resetting the board between downloads.</para>
</listitem>

</orderedlist>

<para>You should now be able to build RedBoot. For ROM startup:
</para>

<programlisting width=72>
% ecosconfig new &lt;target_name&gt; redboot
% ecosconfig import $(ECOS_REPOSITORY)/hal/&lt;architecture&gt;/&lt;platform&gt;/&lt;version&gt;/misc/redboot_ROM.ecm
% ecosconfig tree
% make
</programlisting>

<para>You may have to make further changes than suggested above to get
the make command to succeed. But when it does, you should find a
RedBoot image in install/bin. To program this image into flash or
EPROM, you may need to convert to some other file type, and possibly
adjust the start address. When you have the correct
<application>objcopy</application> command to do this, add it to the
<literal>CYGBLD_BUILD_GDB_STUBS</literal> custom build rule in the
platform CDL file.
</para>

<para>Having updated the flash/EPROM on the board, you should see output
on the serial port looking like this when powering on the board:
</para>

<programlisting>
RedBoot(tm) bootstrap and debug environment [ROMRAM]
Non-certified release, version UNKNOWN - built 15:42:24, Mar 14 2002

Platform: &lt;PLATFORM&gt; (&lt;ARCHITECTURE&gt; &lt;VARIANT&gt;)
Copyright (C) 2000, 2001, 2002, Red Hat, Inc.

RAM: 0x00000000-0x01000000, 0x000293e8-0x00ed1000 available
FLASH: 0x24000000 - 0x26000000, 256 blocks of 0x00020000 bytes each.
RedBoot> 
</programlisting>

<para>If you do not see this output, you need to go through all your
changes and figure out what's wrong. If there's a user programmable
LED or LCD on the board it may help you figure out how far RedBoot
gets before it hangs. Unfortunately there's no good way to describe
what to do in this situation - other than that you have to play with
the code and the board.
</para>

</section>

<!-- ====================================================================== -->

<section>
<title>Adding features</title>

<para>Now you should have a basic RedBoot running on the board. This
means you have a the correct board initialization and a working serial
driver. It's time to flesh out the remaining HAL features.
</para>

<orderedlist>
<listitem><para>Reset. As mentioned above it is desirable to get the board to
reset when GDB disconnects. When GDB disconnects it sends RedBoot
a kill-packet, and RedBoot first calls <literal>HAL_STUB_PLATFORM_RESET()</literal>,
attempting to perform a software-invoked reset. Most embedded
CPUs/boards have a watchdog which is capable of triggering a reset.
If your target does not have a watchdog, leave
<literal>HAL_STUB_PLATFORM_RESET()</literal> empty and rely on the fallback approach.
</para>

<para>If <literal>HAL_STUB_PLATFORM_RESET()</literal> did not cause a reset, RedBoot will
jump to <literal>HAL_STUB_PLATFORM_RESET_ENTRY</literal> - this should be the address
where the CPU will start execution after a reset. Re-initializing the
board and drivers will <emphasis>usually</emphasis> be good enough to make a
hardware reset unnecessary.
</para>

<para>After the reset caused by the kill-packet, the target will be ready
for GDB to connect again. During a days work, this will save you from
pressing the reset button many times.
</para>

<para>Note that it is possible to disconnect from the board without
causing it to reset by using the GDB command &quot;detach&quot;.</para>
</listitem>

<listitem>
<para>Single-stepping is necessary for both instruction-level debugging
and for breakpoint support. Single-stepping support should already be
in place as part of the architecture/variant HAL, but you want to give
it a quick test since you will come to rely on it.</para>
</listitem>

<listitem>
<para>Real-time clock interrupts drive the eCos scheduler clock. Many
embedded CPUs have an on-core timer (e.g. SH) or decrementer
(e.g. MIPS, PPC) that can be used, and in this case it will already be
supported by the architecture/variant HAL. You only have to calculate
and enter the proper <literal>CYGNUM_HAL_RTC_CONSTANTS</literal>
definitions in the platform CDL file.
</para>

<para>On some targets it may be necessary to use a platform-specific
timer source for driving the real-time clock. In this case you also
have to enter the proper CDL definitions, but must also define
suitable versions of the <literal>HAL_CLOCK_XXXX</literal> macros.</para>
</listitem>

<listitem>
<para>Interrupt decoding usually differs between platforms because the
number and type of devices on the board differ. In
<filename>plf_intr.h</filename> (ARM:
<filename>hal_platform_ints.h</filename>) you must either extend or
replace the default vector definitions provided by the architecture
or variant interrupt headers. You may also have to define
<literal>HAL_INTERRUPT_XXXX</literal> control macros.</para>
</listitem>

<listitem>
<para>Caching may also differ from architecture/variant definitions.
This maybe just the cache sizes, but there can also be bigger
differences for example if the platform supports 2nd level caches.
</para>

<para>When cache definitions are in place, enable the caches on
startup. First verify that the system is stable for RAM startups, then
build a new RedBoot and install it. This will test if caching, and in
particular the cache sync/flush operations, also work for ROM startup.</para>
</listitem>

<listitem>
<para>Asynchronous breakpoints allow you to stop application execution
and enter the debugger. Asynchronous breakpoint details are described
in <!-- <xref linkend="hal-stubs-async-bps"> -->.</para>
</listitem>

</orderedlist>

<para>You should now have a completed platform HAL port. Verify its
stability and completeness by running all the eCos tests and fix any
problems that show up (you have a working RedBoot now, remember! That
means you can debug the code to see why it fails).
</para>

<para>Given the many configuration options in eCos, there may be hidden
bugs or missing features that do not show up even if you run all the
tests successfully with a default configuration. A comprehensive test
of the entire system will take many configuration permutations and
many many thousands of tests executed.
</para>

</section>

</section>

<!-- }}} -->
<!-- {{{ Hints -->

<section>
<title>Hints</title>

<itemizedlist>

<listitem>
    <para>JTAG or similar CPU debugging hardware can greatly reduce the time
    it takes to write a HAL port since you always have full visibility
    of what the CPU is doing.
    </para>
</listitem>
    
<listitem>
    <para>LEDs can be your friends if you don't have a JTAG
    device. Especially in the start of the porting effort if you don't
    already have a working ROM monitor on the target. Then you have to
    get a basic RedBoot working while basically being blindfolded. The
    LED can make it little easier, as you'll be able to do limited
    tracking of program flow and behavior by switching the LED on and
    off. If the board has multiple LEDs you can show a number (using
    binary notation with the LEDs) and sprinkle code which sets
    different numbers throughout the code.</para>
</listitem>

<listitem>
    <para>Debugging the interrupt processing is possible if you are
    careful with the way you program the very early interrupt entry
    handling. Write it so that as soon as possible in the interrupt
    path, taking a trap (exception) does not harm execution. See the
    SH vectors.S code for an example. Look for
    <literal>cyg_hal_default_interrupt_vsr</literal> and the label
    <literal>cyg_hal_default_interrupt_vsr_bp_safe</literal>, which
    marks the point after which traps/single-stepping is safe.
    </para>

    <para>Being able to display memory content, CPU registers,
    interrupt controller details at the time of an interrupt can save
    a lot of time.</para>
</listitem>

<listitem>
    <para>Using assertions is a good idea. They can sometimes reveal subtle
    bugs or missing features long before you would otherwise have
    found them, let alone notice them.
    </para>

    <para>The default eCos configuration does not use assertions, so you
    have to enable them by switching on the option <literal>CYGPKG_INFRA_DEBUG</literal>
    in the infra package.</para>
</listitem>

<listitem>
    <para>The idle loop can be used to help debug the system.
    </para>

    <para>Triggering clock from the idle loop is a neat trick for
    examining system behavior either before interrupts are fully
    working, or to speed up &quot;the clock&quot;.
    </para>

    <para>Use the idle loop to monitor and/or print out variables or
    hardware registers.</para>
</listitem>

<listitem>
<para><application>hal_mk_defs</application> is used in some of the
HALs (ARM, SH) as a way to generate assembler symbol definitions from
C header files without imposing an assembler/C syntax separation in
the C header files.</para>
</listitem>

<!-- 
<listitem><para>Tracing using buffers [FIXME:TBD]</para>
</listitem>
-->

</itemizedlist>

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ CDL Requirements -->

<section id="hal-porting-cdl-requirements">
<TITLE>HAL Platform CDL</TITLE>

<para>The platform CDL both contains details necessary for the building
of eCos, and platform-specific configuration options. For this reason
the options differ between platforms, and the below is just a brief
description of the most common options.</para>

<para> See <!-- <xref linkend="???"> --> Components Writers Guide
for more details on CDL. Also have a quick look around in
existing platform CDL files to get an idea of what is possible and how
various configuration issues can be represented with CDL.</para>

<!-- {{{ eCos Database -->

<section id="hal-porting-ecos-database">
<title>eCos Database</title>

<para>
The eCos configuration system is made aware of a package by
adding a package description in <filename>ecos.db</filename>. As an
example we use the <literal>TX39/JMR3904</literal> platform:
</para>

<programlisting>
package CYGPKG_HAL_MIPS_TX39_JMR3904 {
	alias		{ "Toshiba JMR-TX3904 board" hal_tx39_jmr3904 tx39_jmr3904_hal }
	directory	hal/mips/jmr3904
	script		hal_mips_tx39_jmr3904.cdl
	hardware
	description "
           The JMR3904 HAL package should be used when targeting the
           actual hardware. The same package can also be used when
           running on the full simulator, since this provides an
           accurate simulation of the hardware including I/O devices.
           To use the simulator in this mode the command
           `target sim --board=jmr3904' should be used from inside gdb."
}
</programlisting>

<para>This contains the title and description presented in the
Configuration Tool when the package is selected. It also specifies
where in the tree the package files can be found (<literal>directory</literal>)
and the name of the CDL file which contains the package details
(<literal>script</literal>).
</para>

<para>
To be able to build and test a configuration for the new target, there
also needs to be a <literal>target</literal> entry in the
<filename>ecos.db</filename> file. 
</para>

<programlisting>
target jmr3904 {
        alias		{ "Toshiba JMR-TX3904 board" jmr tx39 }
	packages        { CYGPKG_HAL_MIPS
                          CYGPKG_HAL_MIPS_TX39
                          CYGPKG_HAL_MIPS_TX39_JMR3904
        }
        description "
           The jmr3904 target provides the packages needed to run
           eCos on a Toshiba JMR-TX3904 board. This target can also
           be used when running in the full simulator, since the simulator provides an
           accurate simulation of the hardware including I/O devices.
           To use the simulator in this mode the command
           `target sim --board=jmr3904' should be used from inside gdb."
}
</programlisting>


<para>
The important part here is the <literal>packages</literal> section
which defines the various hardware specific packages that contribute
to support for this target. In this case the MIPS architecture
package, the TX39 variant package, and the JMR-TX3904 platform
packages are selected. Other packages, for serial drivers, ethernet
drivers and FLASH memory drivers may also appear here.
</para>

</section>

<!-- }}} -->
<!-- {{{ CDL File Layout -->

<section>
<title>CDL File Layout</title>

<para>
All the platform options are contained in a CDL package named
<literal>CYGPKG_HAL_&lt;architecture&gt;_&lt;variant&gt;_&lt;platform&gt;</literal>.
They all share more or less the same <literal>cdl_package</literal>
details:
</para>

<programlisting>
cdl_package CYGPKG_HAL_MIPS_TX39_JMR3904 {
    display       "JMR3904 evaluation board"
    parent        CYGPKG_HAL_MIPS
    requires      CYGPKG_HAL_MIPS_TX39
    define_header hal_mips_tx39_jmr3904.h
    include_dir   cyg/hal
    description   "
           The JMR3904 HAL package should be used when targeting the
           actual hardware. The same package can also be used when
           running on the full simulator, since this provides an
           accurate simulation of the hardware including I/O devices.
           To use the simulator in this mode the command
           `target sim --board=jmr3904' should be used from inside gdb."

    compile       platform.S plf_misc.c plf_stub.c

    define_proc {
        puts $::cdl_system_header "#define CYGBLD_HAL_TARGET_H   &lt;pkgconf/hal_mips_tx39.h&gt;"
        puts $::cdl_system_header "#define CYGBLD_HAL_PLATFORM_H &lt;pkgconf/hal_mips_tx39_jmr3904.h&gt;"
    }

    ...
}
</programlisting>

<para>This specifies that the platform package should be parented under
the MIPS packages, requires the TX39 variant HAL and all configuration
settings should be saved in
<filename>cyg/hal/hal_mips_tx39_jmt3904.h</filename>.
</para>

<para>The <literal>compile</literal> line specifies which files should be built
when this package is enabled, and the <literal>define_proc</literal> defines
some macros that are used to access the variant or architecture (the
<literal>_TARGET_</literal> name is a bit of a misnomer) and platform
configuration options. </para>

</section>

<!-- }}} -->
<!-- {{{ Startup Type -->

<section>
<title>Startup Type</title>

<para>eCos uses an option to select between a set of valid startup
configurations. These are normally RAM, ROM and possibly ROMRAM. This
setting is used to select which linker map to use (i.e., where to link
eCos and the application in the memory space), and how the startup
code should behave.</para>

<programlisting>
cdl_component CYG_HAL_STARTUP {
    display       "Startup type"
    flavor        data
    legal_values  {"RAM" "ROM"}
    default_value {"RAM"}
	no_define
	define -file system.h CYG_HAL_STARTUP
    description   "
       When targeting the JMR3904 board it is possible to build
       the system for either RAM bootstrap, ROM bootstrap, or STUB
       bootstrap. RAM bootstrap generally requires that the board
       is equipped with ROMs containing a suitable ROM monitor or
       equivalent software that allows GDB to download the eCos
       application on to the board. The ROM bootstrap typically
       requires that the eCos application be blown into EPROMs or
       equivalent technology."
}
</programlisting>

<para>The <literal>no_define</literal> and <literal>define</literal>
pair is used to make the setting of this option appear in the file
<filename>system.h</filename> instead of the default specified in the
header.</para>

</section>

<!-- }}} -->
<!-- {{{ Build Options -->

<section>
<title>Build options</title>

<para>
A set of options under the components
<literal>CYGBLD_GLOBAL_OPTIONS</literal> and
<literal>CYGHWR_MEMORY_LAYOUT</literal> specify how eCos should be
built: what tools and compiler options should be used, and which
linker fragments should be used.
</para>

<programlisting>

cdl_component CYGBLD_GLOBAL_OPTIONS {
    display "Global build options"
    flavor  none
    parent  CYGPKG_NONE
    description   "
	    Global build options including control over
	    compiler flags, linker flags and choice of toolchain."


    cdl_option CYGBLD_GLOBAL_COMMAND_PREFIX {
        display "Global command prefix"
        flavor  data
        no_define
        default_value { "mips-tx39-elf" }
        description "
            This option specifies the command prefix used when
            invoking the build tools."
    }

    cdl_option CYGBLD_GLOBAL_CFLAGS {
        display "Global compiler flags"
        flavor  data
        no_define
        default_value { "-Wall -Wpointer-arith -Wstrict-prototypes -Winline -Wundef -Woverloaded-virtual -g -O2 -ffunction-sections -fdata-sections -fno-rtti -fno-exceptions -fvtable-gc -finit-priority" }
        description   "
            This option controls the global compiler flags which
            are used to compile all packages by
            default. Individual packages may define
            options which override these global flags."
    }

    cdl_option CYGBLD_GLOBAL_LDFLAGS {
        display "Global linker flags"
        flavor  data
        no_define
        default_value { "-g -nostdlib -Wl,--gc-sections -Wl,-static" }
        description   "
            This option controls the global linker flags. Individual
            packages may define options which override these global flags."
    }
}

cdl_component CYGHWR_MEMORY_LAYOUT {
    display "Memory layout"
    flavor data
    no_define
    calculated { CYG_HAL_STARTUP == "RAM" ? "mips_tx39_jmr3904_ram" : \
                                            "mips_tx39_jmr3904_rom" }

    cdl_option CYGHWR_MEMORY_LAYOUT_LDI {
        display "Memory layout linker script fragment"
        flavor data
        no_define
        define -file system.h CYGHWR_MEMORY_LAYOUT_LDI
        calculated { CYG_HAL_STARTUP == "RAM" ? "&lt;pkgconf/mlt_mips_tx39_jmr3904_ram.ldi&gt;" : \
                                                "&lt;pkgconf/mlt_mips_tx39_jmr3904_rom.ldi&gt;" }
    }

    cdl_option CYGHWR_MEMORY_LAYOUT_H {
        display "Memory layout header file"
        flavor data
        no_define
        define -file system.h CYGHWR_MEMORY_LAYOUT_H
        calculated { CYG_HAL_STARTUP == "RAM" ? "&lt;pkgconf/mlt_mips_tx39_jmr3904_ram.h&gt;" : \
                                                "&lt;pkgconf/mlt_mips_tx39_jmr3904_rom.h&gt;" }
    }
}

</programlisting>

</section>

<!-- }}} -->
<!-- {{{ Common Target Options -->

<section>
<title>Common Target Options</title>

<para>All platforms also specify real-time clock details:</para>

<programlisting>
# Real-time clock/counter specifics
cdl_component CYGNUM_HAL_RTC_CONSTANTS {
    display       "Real-time clock constants."
    flavor        none

    cdl_option CYGNUM_HAL_RTC_NUMERATOR {
        display       "Real-time clock numerator"
        flavor        data
        calculated    1000000000
    }
    cdl_option CYGNUM_HAL_RTC_DENOMINATOR {
        display       "Real-time clock denominator"
        flavor        data
        calculated    100
    }
    # Isn't a nice way to handle freq requirement!
    cdl_option CYGNUM_HAL_RTC_PERIOD {
        display       "Real-time clock period"
        flavor        data
        legal_values  { 15360 20736 }
        calculated     { CYGHWR_HAL_MIPS_CPU_FREQ == 50 ? 15360 : \
                         CYGHWR_HAL_MIPS_CPU_FREQ == 66 ? 20736 : 0 }
    }
}
</programlisting>

<para> The <literal>NUMERATOR</literal> divided by the
<literal>DENOMINATOR</literal> gives the number of nanoseconds per
tick. The <literal>PERIOD</literal> is the divider to be programmed
into a hardware timer that is driven from an appropriate hardware
clock, such that the timer overflows once per tick (normally
generating a CPU interrupt to mark the end of a tick). The tick
default rate is typically 100Hz.</para>


<para>Platforms that make use of the virtual vector
ROM calling interface (see <xref linkend="hal-calling-if">) will also
specify details necessary to define configuration channels (these
options are from the SH/EDK7707 HAL) :</para>

<programlisting>
cdl_option CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS {
    display      "Number of communication channels on the board"
    flavor       data
    calculated   1
}

cdl_option CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL {
    display          "Debug serial port"
    flavor data
    legal_values     0 to CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS-1
    default_value    0
    description      "
       The EDK/7708 board has only one serial port. This option
       chooses which port will be used to connect to a host
       running GDB."
}

cdl_option CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL {
    display          "Diagnostic serial port"
    flavor data
    legal_values     0 to CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS-1
    default_value    0
    description      "
       The EDK/7708 board has only one serial port.  This option
       chooses which port will be used for diagnostic output."
}
</programlisting>

<para>The platform usually also specify an option controlling the ability
 to co-exist with a ROM monitor:</para>

<programlisting>
cdl_option CYGSEM_HAL_USE_ROM_MONITOR {
    display       "Work with a ROM monitor"
    flavor        booldata
    legal_values  { "Generic" "CygMon" "GDB_stubs" }
    default_value { CYG_HAL_STARTUP == "RAM" ? "CygMon" : 0 }
    parent        CYGPKG_HAL_ROM_MONITOR
    requires      { CYG_HAL_STARTUP == "RAM" }
    description   "
        Support can be enabled for three different varieties of ROM monitor.
        This support changes various eCos semantics such as the encoding
        of diagnostic output, or the overriding of hardware interrupt
        vectors.
        Firstly there is \"Generic\" support which prevents the HAL
        from overriding the hardware vectors that it does not use, to
        instead allow an installed ROM monitor to handle them. This is
        the most basic support which is likely to be common to most
        implementations of ROM monitor.
        \"CygMon\" provides support for the Cygnus ROM Monitor.
        And finally, \"GDB_stubs\" provides support when GDB stubs are
        included in the ROM monitor or boot ROM."
}
</programlisting>

<para>Or the ability to be configured as a ROM monitor:</para>

<programlisting>
cdl_option CYGSEM_HAL_ROM_MONITOR {
    display       "Behave as a ROM monitor"
    flavor        bool
    default_value 0
    parent        CYGPKG_HAL_ROM_MONITOR
    requires      { CYG_HAL_STARTUP == "ROM" }
    description   "
        Enable this option if this program is to be used as a ROM monitor,
        i.e. applications will be loaded into RAM on the board, and this
        ROM monitor may process exceptions or interrupts generated from the
        application. This enables features such as utilizing a separate
        interrupt stack when exceptions are generated."
}
</programlisting>

<para>The latter option is accompanied by a special build rule that
extends the generic ROM monitor build rule in the common HAL:</para>

<programlisting>
cdl_option CYGBLD_BUILD_GDB_STUBS {
    display "Build GDB stub ROM image"
    default_value 0
    requires { CYG_HAL_STARTUP == "ROM" }
    requires CYGSEM_HAL_ROM_MONITOR
    requires CYGBLD_BUILD_COMMON_GDB_STUBS
    requires CYGDBG_HAL_DEBUG_GDB_INCLUDE_STUBS
    requires ! CYGDBG_HAL_DEBUG_GDB_BREAK_SUPPORT
    requires ! CYGDBG_HAL_DEBUG_GDB_THREAD_SUPPORT
    requires ! CYGDBG_HAL_COMMON_INTERRUPTS_SAVE_MINIMUM_CONTEXT
    requires ! CYGDBG_HAL_COMMON_CONTEXT_SAVE_MINIMUM
    no_define
    description "
        This option enables the building of the GDB stubs for the
        board. The common HAL controls takes care of most of the
        build process, but the final conversion from ELF image to
        binary data is handled by the platform CDL, allowing
        relocation of the data if necessary."

    make -priority 320 {
        &lt;PREFIX&gt;/bin/gdb_module.bin : &lt;PREFIX&gt;/bin/gdb_module.img
        $(OBJCOPY) -O binary $< $@
    }
}
</programlisting>

<para>
Most platforms support RedBoot, and some options are needed to
configure for RedBoot.
</para>

<programlisting width=72>
    cdl_component CYGPKG_REDBOOT_HAL_OPTIONS {
        display       "Redboot HAL options"
        flavor        none
        no_define
        parent        CYGPKG_REDBOOT
        active_if     CYGPKG_REDBOOT
        description   "
            This option lists the target's requirements for a valid Redboot
            configuration."
    
        cdl_option CYGBLD_BUILD_REDBOOT_BIN {
            display       "Build Redboot ROM binary image"
            active_if     CYGBLD_BUILD_REDBOOT
            default_value 1
            no_define
            description "This option enables the conversion of the Redboot ELF
                         image to a binary image suitable for ROM programming."
    
            make -priority 325 {
                &lt;PREFIX&gt;/bin/redboot.bin : &lt;PREFIX&gt;/bin/redboot.elf
                $(OBJCOPY) --strip-debug $< $(@:.bin=.img) 
                $(OBJCOPY) -O srec $< $(@:.bin=.srec)
                $(OBJCOPY) -O binary $< $@
            }
        }
    }
</programlisting>

<para>
The important part here is the <literal>make</literal> command in the
<literal>CYGBLD_BUILD_REDBOOT_BIN</literal> option which emits
makefile commands to translate the <filename>.elf</filename> file
generated by the link phase into both a binary file and an S-Record
file. If a different format is required by a PROM programmer or ROM
monitor, then different output formats would need to be generated here.
</para>

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ Platform Memory Layout -->

<section id="hal-porting-platform-memory-layout">
<TITLE>Platform Memory Layout</TITLE>

<para>The platform memory layout is defined using the Memory
Configuration Window <!-- [FIXME: ref] --> in the Configuration Tool.</para>

<note>
<para>If you do not have access to a Windows machine, you can
hand edit the <filename>.h</filename> and <filename>.ldi</filename> files to match the
properties of your platform. If you want to contribute your port back
to the eCos community, ask someone on the list to make proper memory
map files for you.</para>
</note>

<section>
<title>Layout Files</title>

<para>The memory configuration details are saved in three files:</para>

<variablelist>
<varlistentry>
<term><filename>.mlt</filename></term>
	<listitem><para>This is the Configuration Tool save-file. It is only used
	by the Configuration Tool.</para></listitem>
</varlistentry>	
<varlistentry>
<term><filename>.ldi</filename></term>
	<listitem><para>This is the linker script fragment. It defines the memory
	and location of sections by way of macros defined in the
	architecture or variant linker script.</para></listitem>
</varlistentry>
<varlistentry>
<term><filename>.h</filename></term>
	<listitem><para>This file describes some of the memory region details as C
	macros, allowing eCos or the application adapt the memory
	layout of a specific configuration.</para></listitem>
</varlistentry>
</variablelist>

<para>These three files are generated for each startup-type, since the
memory details usually differ.</para>

</section>

<section>
<title>Reserved Regions</title>

<para>Some areas of the memory space are reserved for specific
purposes, making room for exception vectors and various tables. RAM
startup configurations also need to reserve some space at the bottom
of the memory map for the ROM monitor.</para>

<para>These reserved areas are named with the prefix "reserved_" which is
handled specially by the Configuration Tool: instead of referring to a
linker macro, the start of the area is labeled and a gap left in the
memory map.</para>

</section>


</section>

<!-- }}} -->
<!-- {{{ Platform Serial Device Support -->

<section>
<title>Platform Serial Device Support</title>

<para>
The first step is to set up the CDL definitions. The configuration
options that need to be set are the following:
</para>

<variablelist>
  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS</literal></term>
    <listitem><para>The number of channels, usually 0, 1 or 2.</para></listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL</literal></term>
    <listitem><para>The channel to use for GDB.</para></listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL_BAUD</literal></term>
    <listitem><para>Initial baud rate for debug channel.</para></listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL</literal></term>
    <listitem><para>The channel to use for the
    console.</para></listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL_BAUD</literal></term>
    <listitem><para>The initial baud rate for the console
    channel.</para></listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL_DEFAULT</literal></term>
    <listitem><para>The default console channel.</para></listitem>
  </varlistentry>
</variablelist>

<para>
The code in <filename>hal_diag.c</filename> need to be converted to
support the new serial device.
If this the same as a device already supported, copy that.
</para>

<para>
The following functions and types need to be rewritten to support a new serial
device.
</para>

<variablelist>
  <varlistentry>
    <term><literal>struct channel_data_t;</literal></term>
    <listitem>
      <para>
      Structure containing base address, timeout and ISR vector number
      for each serial device supported. Extra fields my be added if
      necessary for the device. For example some devices have
      write-only control registers, so keeping a shadow of the last
      value written here can be useful.
      </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>xxxx_ser_channels[];</literal></term>
    <listitem>
        <para>
	Array of <literal>channel_data_t</literal>, initialized with parameters of each
	channel. The index into this array is the channel number used
	in the CDL options above and is used by the virtual vector
	mechanism to refer to each channel.
        </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>void cyg_hal_plf_serial_init_channel(void
           *__ch_data)</literal></term>
    <listitem>
        <para>
	Initialize the serial device. The parameter is actually a pointer to a
	<literal>channel_data_t</literal> and should be cast back to
	this type before use. This function should use the CDL
	definition for the baud rate for the channel it is initializing.
        </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>void cyg_hal_plf_serial_putc(void * __ch_data,
                    char *c)</literal></term>
    <listitem>
        <para>
        Send a character to the serial device. This function should
	poll for the device being ready to send and then write the character.
        Since this is intended to be a diagnostic/debug channel, it is
	often also a good idea to poll for end of transmission
	too. This ensures that as much data gets out of the system as
	possible.
        </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>bool cyg_hal_plf_serial_getc_nonblock(void*
                    __ch_data, cyg_uint8* ch)</literal></term>
    <listitem>
        <para>
        This function tests the device and if a character is
	available, places it in <parameter>*ch</parameter> and returns
	<literal>TRUE</literal>. If no character is available, then
	the function returns <literal>FALSE</literal> immediately.
        </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>int cyg_hal_plf_serial_control(void *__ch_data,
                    __comm_control_cmd_t __func,
                    ...)</literal></term>
     <listitem>
	<para>
        This is an IOCTL-like function for controlling various aspects
	of the serial device. The only part in which you may need to
	do some work initially is in the
	<literal>__COMMCTL_IRQ_ENABLE</literal> and
	<literal>__COMMCTL_IRQ_DISABLE</literal> cases to
	enable/disable interrupts.
        </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>int cyg_hal_plf_serial_isr(void *__ch_data, int* __ctrlc, 
                       CYG_ADDRWORD __vector, CYG_ADDRWORD
                       __data)</literal></term>
    <listitem>
        <para>
        This interrupt handler, called from the spurious interrupt
        vector, is specifically for dealing with
        <literal>Ctrl-C</literal> interrupts from GDB. When called
        this function should do the following:
        <orderedlist>
        <listitem>
          <para>Check for an incoming character. The code here is very
          similar to that in
          <function>cyg_hal_plf_serial_getc_nonblock()</function>.
          </para>
        </listitem>
        <listitem>
          <para>
	  Read the character and call
	  <function>cyg_hal_is_break()</function>.
          </para>
        </listitem>
        <listitem>
          <para>
	  If result is true, set <parameter>*__ctrlc</parameter> to
	  <literal>1</literal>.
          </para>
        </listitem>
        <listitem>
          <para>
	  Return <literal>CYG_ISR_HANDLED</literal>.
          </para>
        </listitem>
        </orderedlist>
      </para>
    </listitem>
  </varlistentry>

  <varlistentry>
    <term><literal>void cyg_hal_plf_serial_init()</literal></term>
    <listitem>
        <para>
        Initialize each of the serial channels.
	First call <function>cyg_hal_plf_serial_init_channel()</function> for each channel.
	Then call the <literal>CYGACC_COMM_IF_*</literal> macros for
	each channel. This latter set of calls are identical for all
	channels, so the best way to do this is to copy and edit an
	existing example.
        </para>
    </listitem>
  </varlistentry>
</variablelist>

</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ Variant HAL Porting -->

<section id="hal-porting-variant">
<title>Variant HAL Porting</title>

<para>
A variant port can be a fairly limited job, but can also
require quite a lot of work. A variant HAL describes how a specific
CPU variant differs from the generic CPU architecture. The variant HAL
can re-define cache, MMU, interrupt, and other features which override
the default implementation provided by the architecture HAL.
</para>

<para>
Doing a variant port requires a preexisting architecture HAL port. It
is also likely that a platform port will have to be done at the same
time if it is to be tested.
</para>

<!-- {{{ Porting Process -->

<section>
<TITLE>HAL Variant Porting Process</TITLE>

<para>The easiest way to make a new variant HAL is simply to copy an
existing variant HAL and change all the files to match the new
variant. If this is the first variant for an architecture, it may be
hard to decide which parts should be put in the variant - knowledge of
other variants of the architecture is required.</para> 

<para>Looking at existing variant HALs (e.g., MIPS tx39, tx49) may be a
help - usually things such as caching, interrupt and exception
handling differ between variants. Initialization code, and code for
handling various core components (FPU, DSP, MMU, etc.) may also differ
or be missing altogether on some variants. Linker scripts may also require
specific variant versions.</para>

<note>
<title>Note</title>
<para>Some CPU variants may require specific compiler
support. That support must be in place before you can undertake the
eCos variant port.</para>
</note>



</section>

<!-- }}} -->
<!-- {{{ CDL Requirements -->

<section>
<TITLE>HAL Variant CDL</TITLE>

<para>
The CDL in a variant HAL tends to depend on the exact functionality
supported by the variant. If it implements some of the devices
described in the platform HAL, then the CDL for those will be here
rather than there (for example the real-time clock).
</para>

<para>
There may also be CDL to select options in the architecture HAL to
configure it to a particular architectural variant.
</para>

<para>
Each variant needs an entry in the <filename>ecos.db</filename>
file. This is the one for the SH3:
</para>

<programlisting width=72>
package CYGPKG_HAL_SH_SH3 {
    alias         { "SH3 architecture" hal_sh_sh3 }
    directory     hal/sh/sh3
    script        hal_sh_sh3.cdl
    hardware
    description   "
        The SH3 (SuperH 3) variant HAL package provides generic
        support for SH3 variant CPUs."
}
</programlisting>

<para>
As you can see, it is very similar to the platform entry.
</para>

<para>
The variant CDL file will contain a package entry named for the
architecture and variant, matching the package name in the
<filename>ecos.db</filename> file. Here is the initial part of the
MIPS VR4300 CDL file:
</para>

<programlisting width=72>
cdl_package CYGPKG_HAL_MIPS_VR4300 {
    display       "VR4300 variant"
    parent        CYGPKG_HAL_MIPS
    implements    CYGINT_HAL_MIPS_VARIANT
    hardware
    include_dir   cyg/hal
    define_header hal_mips_vr4300.h
    description   "
           The VR4300 variant HAL package provides generic support
           for this processor architecture. It is also necessary to
           select a specific target platform HAL package."
</programlisting>

<para>
This defines the package, placing it under the MIPS architecture
package in the hierarchy. The <literal>implements</literal> line
indicates that this is a MIPS variant. The architecture package uses
this to check that exactly one variant is configured in.
</para>

<para>
The variant defines some options that cause the architecture HAL to
configure itself to support this variant.
</para>

<programlisting width=72>
    cdl_option CYGHWR_HAL_MIPS_64BIT {
        display    "Variant 64 bit architecture support"
        calculated 1
    }

    cdl_option CYGHWR_HAL_MIPS_FPU {
        display    "Variant FPU support"
        calculated 1
    }

    cdl_option CYGHWR_HAL_MIPS_FPU_64BIT {
        display    "Variant 64 bit FPU support"
        calculated 1
    }
</programlisting>

<para>
These tell the architecture that this is a 64 bit MIPS architecture,
that it has a floating point unit, and that we are going to use it in
64 bit mode rather than 32 bit mode.
</para>

<para>
The CDL file finishes off with some build options.
</para>

<programlisting width=72>
    define_proc {
        puts $::cdl_header "#include &lt;pkgconf/hal_mips.h&gt;"
    }

    compile       var_misc.c

    make {
        &lt;PREFIX&gt;/lib/target.ld: &lt;PACKAGE&gt;/src/mips_vr4300.ld
        $(CC) -E -P -Wp,-MD,target.tmp -DEXTRAS=1 -xc $(INCLUDE_PATH) $(CFLAGS) -o $@ $&lt;
        @echo $@ ": \\" &gt; $(notdir $@).deps
        @tail +2 target.tmp &gt;&gt; $(notdir $@).deps
        @echo &gt;&gt; $(notdir $@).deps
        @rm target.tmp
    }

    cdl_option CYGBLD_LINKER_SCRIPT {
        display "Linker script"
        flavor data
	no_define
        calculated  { "src/mips_vr4300.ld" }
    }

}
</programlisting>

<para>
The <literal>define_proc</literal> causes the architecture
configuration file to be included into the configuration file for the
variant. The <literal>compile</literal> causes the single source file
for this variant, <filename>var_misc.c</filename> to be compiled. The
<literal>make</literal> command emits makefile rules to combine the
linker script with the <filename>.ldi</filename> file to generate
<literal>target.ld</literal>. Finally, in the MIPS HALs, the main
linker script is defined in the variant, rather than the architecture,
so <literal>CYGBLD_LINKER_SCRIPT</literal> is defined here.
</para>

</section>

<!-- }}} -->
<!-- {{{ Cache Support -->

<section>
<title>Cache Support</title>

<para>
The main area where the variant is likely to be involved is in cache
support. Often the only thing that distinguishes one CPU variant from
another is the size of its caches.
</para>

<para>
In architectures such as the MIPS and PowerPC where cache instructions
are part of the ISA, most of the actual cache operations are
implemented in the architecture HAL. In this case the variant HAL only
needs to define the cache dimensions. The following are the cache
dimensions defined in the MIPS VR4300 variant
<filename>var_cache.h</filename>.
</para>

<programlisting width=72>
// Data cache
#define HAL_DCACHE_SIZE                 (8*1024)        // Size of data cache in bytes
#define HAL_DCACHE_LINE_SIZE            16              // Size of a data cache line
#define HAL_DCACHE_WAYS                 1               // Associativity of the cache

// Instruction cache
#define HAL_ICACHE_SIZE                 (16*1024)       // Size of cache in bytes
#define HAL_ICACHE_LINE_SIZE            32              // Size of a cache line
#define HAL_ICACHE_WAYS                 1               // Associativity of the cache

#define HAL_DCACHE_SETS (HAL_DCACHE_SIZE/(HAL_DCACHE_LINE_SIZE*HAL_DCACHE_WAYS))
#define HAL_ICACHE_SETS (HAL_ICACHE_SIZE/(HAL_ICACHE_LINE_SIZE*HAL_ICACHE_WAYS))
</programlisting>

<para>
Additional cache macros, or overrides for the defaults, may also
appear in here. While some architectures have instructions for
managing cache lines, overall enable/disable operations may be handled
via variant specific registers. If so then
<filename>var_cache.h</filename> should also define the
<literal>HAL_XCACHE_ENABLE()</literal> and
<literal>HAL_XCACHE_DISABLE()</literal> macros.
</para>

<para>
If there are any generic features that the variant does not support
(cache locking is a typical example) then
<literal>var_cache.h</literal> may need to disable definitions of
certain operations. It is architecture dependent exactly how this is
done.
</para>


</section>

<!-- }}} -->

</section>

<!-- }}} -->
<!-- {{{ Architecture HAL Porting -->

<section id="hal-porting-architecture">

<title>Architecture HAL Porting</title>

<para>
A new architecture HAL is the most complex HAL to write, and it the
least easily described. Hence this section is presently nothing more
than a place holder for the future.
</para>

<!-- {{{ Porting Process -->

<section>
<TITLE>HAL Architecture Porting Process</TITLE>

<para>The easiest way to make a new architecture HAL is simply to copy an
existing architecture HAL of an, if possible, closely matching
architecture and change all the files to match the new
architecture. The MIPS architecture HAL should be used if possible, as
it has the appropriate layout and coding conventions. Other HALs
may deviate from that norm in various ways.</para>

<note>
<title>Note</title>
<para> eCos is written for GCC. It requires C and C++
compiler support as well as a few compiler features introduced during
eCos development - so compilers older than eCos may not provide these
features. Note that there is no C++ support for any 8 or 16 bit
CPUs. Before you can undertake an eCos port, you need the required
compiler support.
</para>
</note>

<para>
The following gives a rough outline of the steps needed to create a
new architecture HAL. The exact order and set of steps needed will
vary greatly from architecture to architecture, so a lot of
flexibility is required. And of course, if the architecture HAL is to
be tested, it is necessary to do variant and  platform ports for the
initial target simultaneously.
</para>

<orderedlist>

<listitem>
<para>
Make a new directory for the new architecture under the
<filename>hal</filename> directory in the source repository. Make an
<filename>arch</filename> directory under this and populate this with
the standard set of package directories.
</para>
</listitem>

<listitem>
<para>
Copy the CDL file from an example HAL changing its name to match the
new HAL. Edit the file, changing option names as appropriate. Delete
any options that are specific to the original HAL, and and any new
options that are necessary for the new architecture. This is likely to
be a continuing process during the development of the HAL. See <xref
linkend="hal-porting-architecture-cdl"> for more details.
</para>
</listitem>

<listitem>
<para>
Copy the <filename>hal_arch.h</filename> file from an example
HAL. Within this file you need to change or define the following:
</para>
<itemizedlist>

<listitem>
<para>
Define the <structname>HAL_SavedRegisters</structname> structure. This
may need to reflect the save order of any group register save/restore
instructions, the interrupt and exception save and restore formats,
and the procedure calling conventions. It may also need to cater for
optional FPUs and other functional units. It can be quite difficult to
develop a layout that copes with all requirements.
</para>
</listitem>

<listitem>
<para>
Define the bit manipulation routines,
<literal>HAL_LSBIT_INDEX()</literal> and
<literal>HAL_MSBIT_INDEX()</literal>. If the architecture contains
instructions to perform these, or related, operations, then these
should be defined as inline assembler fragments. Otherwise make them
calls to functions.
</para>
</listitem>

<listitem>
<para>
Define <literal>HAL_THREAD_INIT_CONTEXT()</literal>. This initializes
a restorable CPU context onto a stack pointer so that a later call to
<literal>HAL_THREAD_LOAD_CONTEXT()</literal> or
<literal>HAL_THREAD_SWITCH_CONTEXT()</literal> will execute it
correctly. This macro needs to take account of the same optional
features of the architecture as the definition of
<structname>HAL_SavedRegisters</structname>.
</para>
</listitem>

<listitem>
<para>
Define <literal>HAL_THREAD_LOAD_CONTEXT()</literal> and
<literal>HAL_THREAD_SWITCH_CONTEXT()</literal>. These should just be
calls to functions in <filename>context.S</filename>.
</para>
</listitem>

<listitem>
<para>
Define <literal>HAL_REORDER_BARRIER()</literal>. This prevents code
being moved by the compiler and is necessary in some order-sensitive
code. This macro is actually defined identically in all architecture,
so it can just be copied.
</para>
</listitem>

<listitem>
<para>
Define breakpoint support. The macro
<literal>HAL_BREAKPOINT(label)</literal> needs to be an inline assembly
fragment that invokes a breakpoint. The breakpoint instruction should
be labeled with the <parameter>label</parameter>
argument. <literal>HAL_BREAKINST</literal> and
<literal>HAL_BREAKINST_SIZE</literal> define the breakpoint
instruction for debugging purposes.
</para>
</listitem>

<listitem>
<para>
Define GDB support. GDB views the registers of the target as a linear
array, with each register having a well defined offset. This array may
differ from the ordering defined in
<structname>HAL_SavedRegisters</structname>. The macros
<literal>HAL_GET_GDB_REGISTERS()</literal> and
<literal>HAL_SET_GDB_REGISTERS()</literal> translate between the GDB
array and the <structname>HAL_SavedRegisters</structname> structure.
The <literal>HAL_THREAD_GET_SAVED_REGISTERS()</literal> translates a
stack pointer saved by the context switch macros into a pointer to a
<structname>HAL_SavedRegisters</structname> structure. Usually this is
a one-to-one translation, but this macro allows it to differ if
necessary.
</para>
</listitem>

<listitem>
<para>
Define long jump support. The type <type>hal_jmp_buf</type> and the
functions <function>hal_setjmp()</function> and
<literal>hal_longjmp()</literal> provide the underlying implementation
of the C library <function>setjmp()</function> and
<function>longjmp()</function>.
</para>
</listitem>

<listitem>
<para>
Define idle thread action. Generally the macro
<literal>HAL_IDLE_THREAD_ACTION()</literal> is defined to call a
function in <filename>hal_misc.c</filename>.
</para>
</listitem>

<listitem>
<para>
Define stack sizes. The macros
<literal>CYGNUM_HAL_STACK_SIZE_MINIMUM</literal> and
<literal>CYGNUM_HAL_STACK_SIZE_TYPICAL</literal> should be defined to
the minimum size for any thread stack and a reasonable default for
most threads respectively. It is usually best to construct these out
of component sizes for the CPU save state and procedure call stack
usage. These definitions should not use anything other than numerical
values since they can be used from assembly code in some HALs.
</para>
</listitem>

<listitem>
<para>
Define memory access macros. These macros provide translation between
cached and uncached and physical memory spaces. They usually consist
of masking out bits of the supplied address and ORing in alternative
address bits.
</para>
</listitem>

<listitem>
<para>
Define global pointer save/restore macros. These really only need
defining if the calling conventions of the architecture require a
global pointer (as does the MIPS architecture), they may be empty
otherwise. If it is necessary to define these, then take a look at the
MIPS implementation for an example.
</para>
</listitem>

</itemizedlist>

</listitem>

<listitem>
<para>
Copy <filename>hal_intr.h</filename> from an example HAL. Within this
file you should change or define the following:
</para>


<itemizedlist>
<listitem>
<para>
Define the exception vectors. These should be detailed in the
architecture specification. Essentially for each exception entry point
defined by the architecture there should be an entry in the VSR
table. The offsets of these VSR table entries should be defined here
by <literal>CYGNUM_HAL_VECTOR_*</literal> definitions. The size of the
VSR table also needs to be defined here.
</para>
</listitem>

<listitem>
<para>
Map any hardware exceptions to standard names. There is a group of
exception vector name of the form
<literal>CYGNUM_HAL_EXCEPTION_*</literal> that define a wide variety
of possible exceptions that many architectures raise. Generic code
detects whether the architecture can raise a given exception by
testing whether a given <literal>CYGNUM_HAL_EXCEPTION_*</literal>
definition is present. If it is present then its value is the vector
that raises that exception. This does not need to be a one-to-one
correspondence, and several <literal>CYGNUM_HAL_EXCEPTION_*</literal>
definitions may have the same value.
</para>

<para>
Interrupt vectors are usually defined in the variant or platform
HALs. The interrupt number space may either be continuous with the VSR
number space, where they share a vector table (as in the i386) or may
be a separate space where a separate decode stage is used (as in MIPS
or PowerPC).
</para>

</listitem>

<listitem>
<para>
Declare any static data used by the HAL to handle interrupts and
exceptions. This is usually three vectors for interrupts:
<literal>hal_interrupt_handlers[]</literal>,
<literal>hal_interrupt_data[]</literal> and
<literal>hal_interrupt_objects[]</literal>, which are sized according
to the interrupt vector definitions. In addition a definition for the
VSR table, <literal>hal_vsr_table[]</literal> should be made. These
vectors are normally defined in either <filename>vectors.S</filename>
or <filename>hal_misc.c</filename>.
</para>
</listitem>

<listitem>
<para>
Define interrupt enable/disable macros. These are normally inline
assembly fragments to execute the instructions, or manipulate the CPU
register, that contains the CPU interrupt enable bit.
</para>
</listitem>

<listitem>
<para>
A feature that many HALs support is the ability to execute DSRs on the
interrupt stack. This is not an essential feature, and is better left
unimplemented in the initial porting effort. If this is required, then
the macro <literal>HAL_INTERRUPT_STACK_CALL_PENDING_DSRS()</literal>
should be defined to call a function in
<filename>vectors.S</filename>.
</para>
</listitem>

<listitem>
<para>
Define the interrupt and VSR attachment macros. If the same arrays as
for other HALs have been used for VSR and interrupt vectors, then
these macro can be copied across unchanged.
</para>
</listitem>

</itemizedlist>

</listitem>

<listitem>
<para>
A number of other header files also need to be filled in:
</para>
<itemizedlist>
<listitem>
<para>
<filename>basetype.h</filename>. This file defines the basic types
used by eCos, together with the endianness and some other
characteristics. This file only really needs to contain definitions
if the architecture differs significantly from the defaults defined
in <filename>cyg_type.h</filename>
</para>
</listitem>

<listitem>
<para>
<filename>hal_io.h</filename>. This file contains macros for accessing
device IO registers. If the architecture uses memory mapped IO, then
these can be copied unchanged from an existing HAL such as MIPS. If
the architecture uses special IO instructions, then these macros must
be defined as inline assembler fragments. See the I386 HAL for an
example. PCI bus access macros are usually defined in the variant or
platform HALs.
</para>
</listitem>

<listitem>
<para>
<filename>hal_cache.h</filename>. This file contains cache access
macros. If the architecture defines cache instructions, or control
registers, then the access macros should be defined here. Otherwise
they must be defined in the variant or platform HAL. Usually the cache
dimensions (total size, line size, ways etc.) are defined in the
variant HAL.
</para>
</listitem>

<listitem>
<para>
<filename>arch.inc</filename> and
<filename>&lt;architecture&gt;.inc</filename>. These files are
assembler headers used by <filename>vectors.S</filename> and
<filename>context.S</filename>.
<filename>&lt;architecture&gt;.inc</filename> is a general purpose
header that should contain things like register aliases, ABI
definitions and macros useful to general assembly
code. If there are no such definitions, then this file need not be
provided. <filename>arch.inc</filename> contains macros for performing
various eCos related operations such as initializing the CPU, caches,
FPU etc. The definitions here may often be configured or overridden by
definitions in the variant or platform HALs. See the MIPS HAL for an
example of this.
</para>
</listitem>

</itemizedlist>

</listitem>

<listitem>
<para>
Write <filename>vectors.S</filename>. This is the most important file
in the HAL. It contains the CPU initialization code, exception and
interrupt handlers. While other HALs should be consulted for
structures and techniques, there is very little here that can be
copied over without major edits.
</para>

<para>
The main pieces of code that need to be defined here are:
</para>

<itemizedlist>
<listitem>
<para>
Reset vector. This usually need to be positioned at the start of the
ROM or FLASH, so should be in a linker section of its own. It can then be
placed correctly by the linker script. Normally this code is little
more than a jump to the label <literal>_start</literal>.
</para>
</listitem>

<listitem>
<para>
Exception vectors. These are the trampoline routines connected to the
hardware exception entry points that vector through the VSR table. In
many architectures these are adjacent to the reset vector, and should
occupy the same linker section. If the architecture allow the vectors
to be moved then it may be necessary for these trampolines to be
position independent so they can be relocated at runtime.
</para>

<para>
The trampolines should do the minimum necessary to transfer control
from the hardware vector to the VSR pointed to by the matching table
entry. Exactly how this is done depends on the architecture. Usually
the trampoline needs to get some working registers by either saving
them to CPU special registers (e.g. PowerPC SPRs), using reserved
general registers (MIPS K0 and K1), using only memory based
operations (IA32), or just jumping directly (ARM). The VSR table index
to be used is either implicit in the entry point taken (PowerPC, IA32,
ARM), or must be determined from a CPU register (MIPS).
</para>
</listitem>

<listitem>
<para>
Write kernel startup code. This is the location the reset vector jumps
to, and can be in the main text section of the executable, rather than
a special section. The code here should first initialize the CPU and other
hardware subsystems. The best approach is to use a set of macro
calls that are defined either in <filename>arch.inc</filename> or
overridden in the variant or platform HALs. Other jobs that this code
should do are: initialize stack pointer; copy the data section from
ROM to RAM if necessary; zero the BSS; call variant and platform
initializers; call <function>cyg_hal_invoke_constructors()</function>;
call <function>initialize_stub()</function> if necessary. Finally it
should call <function>cyg_start()</function>. See <xref
linkend="hal-startup"> for details.
</para>
</listitem>

<listitem>
<para>
Write the default exception VSR. This VSR is installed in the VSR
table for all synchronous exception vectors. See <xref
linkend="hal-default-synchronous-exception-handling"> for details of
what this VSR does.
</para>
</listitem>

<listitem>
<para>
Write the default interrupt VSR. This is installed in all VSR table
entries that correspond to external interrupts. See <xref
linkend="hal-default-synchronous-exception-handling"> for details of
what this VSR does.
</para>
</listitem>

<listitem>
<para>
Write
<function>hal_interrupt_stack_call_pending_dsrs()</function>. If this
function is defined in <filename>hal_arch.h</filename> then it should
appear here. The purpose of this function is to call DSRs on the
interrupt stack rather than the current thread's stack. This is not an
essential feature, and may be left until later. However it interacts
with the stack switching that goes on in the interrupt VSR, so it may
make sense to write these pieces of code at the same time to ensure
consistency.
</para>

<para>
When this function is implemented it should do the following:
</para>

<itemizedlist>
<listitem>
<para>
Take a copy of the current SP and then switch to the interrupt stack.
</para>
</listitem>

<listitem>
<para>
Save the old SP, together with the CPU status register (or whatever
register contains the interrupt enable status) and any other
registers that may be corrupted by a function call (such as any link
register) to locations in the interrupt stack.
</para>
</listitem>

<listitem>
<para>
Enable interrupts.
</para>
</listitem>

<listitem>
<para>
Call <function>cyg_interrupt_call_pending_DSRs()</function>. This is a
kernel functions that actually calls any pending DSRs.
</para>
</listitem>

<listitem>
<para>
Retrieve saved registers from the interrupt stack and switch back to
the current thread stack.
</para>
</listitem>

<listitem>
<para>
Merge the interrupt enable state recorded in the save CPU status
register with the current value of the status register to restore the
previous enable state. If the status register does not contain any
other persistent state then this can be a simple restore of the
register. However if the register contains other state bits that might
have been changed by a DSR, then care must be taken not to disturb
these.
</para>
</listitem>

</itemizedlist>

</listitem>


<listitem>
<para>
Define any data items needed. Typically <filename>vectors.S</filename>
may contain definitions for the VSR table, the interrupt tables and the
interrupt stack. Sometimes these are only default definitions that may
be overridden by the variant or platform HALs.
</para>
</listitem>

</itemizedlist>

</listitem>

<listitem>
<para>
Write <filename>context.S</filename>. This file contains the context
switch code. See <xref linkend="hal-context-switch"> for details of
how these functions operate. This file may also contain the
implementation of <function>hal_setjmp()</function> and
<function>hal_longjmp()</function>.
</para>
</listitem>

<listitem>
<para>
Write <filename>hal_misc.c</filename>. This file contains any C
data and functions needed by the HAL. These might include:
</para>

<itemizedlist>
<listitem>
<para>
<varname>hal_interrupt_*[]</varname>. In some HALs, if these arrays
are not defined in <filename>vectors.S</filename> then they must be
defined here.
</para>
</listitem>

<listitem>
<para>
<function>cyg_hal_exception_handler()</function>. This function is
called from the exception VSR. It usually does extra decoding of the
exception and invokes any special handlers for things like FPU traps,
bus errors or memory exceptions. If there is nothing special to be
done for an exception, then it either calls into the GDB stubs, by
calling <function>__handle_exception()</function>, or
invokes the kernel by calling
<function>cyg_hal_deliver_exception()</function>.
</para>
</listitem>

<listitem>
<para>
<function>hal_arch_default_isr()</function>. The
<varname>hal_interrupt_handlers[]</varname> array is usually
initialized with pointers to <filename>hal_default_isr()</filename>,
which is defined in the common HAL. This function handles things like
Ctrl-C processing, but if that is not relevant, then it will call
<function>hal_arch_default_isr()</function>. Normally this function
should just return zero.
</para>
</listitem>

<listitem>
<para>
<function>cyg_hal_invoke_constructors()</function>. This calls the
constructors for all static objects before the program starts. eCos
relies on these being called in the correct order for it to function
correctly. The exact way in which constructors are handled may differ
between architectures, although most use a simple table of function
pointers between labels <literal>__CTOR_LIST__</literal> and
<literal>__CTOR_END__</literal> which must called in order from the
top down. Generally, this function can be copied directly from an
existing architecture HAL.
</para>
</listitem>

<listitem>
<para>
Bit indexing functions. If the macros
<literal>HAL_LSBIT_INDEX()</literal> and
<literal>HAL_MSBIT_INDEX()</literal> are defined as function calls,
then the functions should appear here. The main reason for doing this
is that the architecture does not have support for bit indexing and
these functions must provide the functionality by conventional
means. While the trivial implementation is a simple for loop, it is
expensive and non-deterministic. Better, constant time,
implementations can be found in several HALs (MIPS for example).
</para>
</listitem>

<listitem>
<para>
<function>hal_delay_us()</function>. If the macro
<literal>HAL_DELAY_US()</literal> is defined in <filename
class="headerfile">hal_intr.h</filename> then it should be defined to
call this function. While most of the time this function is called
with very small values, occasionally (particularly in some ethernet
drivers) it is called with values of several seconds. Hence the
function should take care to avoid overflow in any calculations.
</para>
</listitem>

<listitem>
<para>
<function>hal_idle_thread_action()</function>. This function is called
from the idle thread via the
<literal>HAL_IDLE_THREAD_ACTION()</literal> macro, if so
defined. While normally this function does nothing, during development
this is often a good place to report various important system
parameters on LCDs, LED or other displays. This function can also
monitor system state and report any anomalies. If the architecture
supports a <literal>halt</literal> instruction then this is a good
place to put an inline assembly fragment to execute it. It is also a
good place to handle any power saving activity.
</para>
</listitem>

</itemizedlist>
</listitem>

<listitem>
<para>
Create the <filename>&lt;architecture&gt;.ld</filename> file. While
this file may need to be moved to the variant HAL in the future, it
should initially be defined here, and only moved if necessary.
</para>
<para>
This file defines a set of macros that are used by the platform
<literal>.ldi</literal> files to generate linker scripts. Most GCC
toolchains are very similar so the correct approach is to copy the
file from an existing architecture and edit it. The main things that
will need editing are the <literal>OUTPUT_FORMAT()</literal> directive
and maybe the creation or allocation of extra sections to various
macros. Running the target linker with just the
<literal>--verbose</literal> argument will cause it to output its
default linker script. This can be compared with the
<literal>.ld</literal> file and appropriate edits made.
</para>
</listitem>

<listitem>
<para>
If GDB stubs are to be supported in RedBoot or eCos, then support must
be included for these. The most important of these are <filename
class="headerfile">include/&lt;architecture&gt;-stub.h</filename> and
<filename>src/&lt;architecture&gt;-stub.c</filename>. In all existing
architecture HALs these files, and any support files they need, have
been derived from files supplied in <literal>libgloss</literal>, as
part of the GDB toolchain package. If this is a totally new
architecture, this may not have been done, and they must be created
from scratch.
</para>

<para>
<filename
class="headerfile">include/&lt;architecture&gt;-stub.h</filename>
contains definitions that are used by the GDB stubs to describe the
size, type, number and names of CPU registers. This information is
usually found in the GDB support files for the architecture. It also
contains prototypes for the functions exported by
<filename>src/&lt;architecture&gt;-stub.c</filename>; however, since
this is common to all architectures, it can be copied from some other
HAL.
</para>

<para>
<filename>src/&lt;architecture&gt;-stub.c</filename> implements the
functions exported by the header. Most of this is fairly straight
forward: the implementation in existing HALs should show exactly what
needs to be done. The only complex part is the support for
single-stepping. This is used a lot by GDB, so it cannot be
avoided. If the architecture has support for a trace or single-step
trap then that can be used for this purpose. If it does not then this
must be simulated by planting a breakpoint in the next
instruction. This can be quite involved since it requires some
analysis of the current instruction plus the state of the CPU to
determine where execution is going to go next.
</para>

</listitem>

</orderedlist>


</section>

<!-- }}} -->
<!-- {{{ CDL Requirements -->

<section id="hal-porting-architecture-cdl">
<title>CDL Requirements</title>

<para>
The CDL needed for any particular architecture HAL depends to a large
extent on the needs of that architecture. This includes issues such as
support for different variants, use of FPUs, MMUs and caches. The
exact split between the architecture, variant and platform HALs for
various features is also somewhat fluid. 
</para>

<para>
To give a rough idea about how the CDL for an architecture is
structured, we will take as an example the I386 CDL.
</para>

<para>
This first section introduces the CDL package and placed it under the
main HAL package. Include files from this package will be put in the
<filename>include/cyg/hal</filename> directory, and definitions from
this file will be placed in
<filename>include/pkgconf/hal_i386.h</filename>. The
<literal>compile</literal> line specifies the files in the
<filename>src</filename> directory that are to be compiled as part of
this package.
</para>

<programlisting width=72>
cdl_package CYGPKG_HAL_I386 {
    display       "i386 architecture"
    parent        CYGPKG_HAL
    hardware
    include_dir   cyg/hal
    define_header hal_i386.h
    description   "
        The i386 architecture HAL package provides generic
        support for this processor architecture. It is also
        necessary to select a specific target platform HAL
        package."

    compile       hal_misc.c context.S i386_stub.c hal_syscall.c
</programlisting>

<para>
Next we need to generate some files using non-standard make rules. The
first is <filename>vectors.S</filename>, which is not put into the
library, but linked explicitly with all applications. The second is
the generation of the <filename>target.ld</filename> file from
<filename>i386.ld</filename> and the startup-selected
<filename>.ldi</filename> file. Both of these are essentially
boilerplate code that can be copied and edited.
</para>

<programlisting width=72>

    make {
        &lt;PREFIX&gt;/lib/vectors.o : &lt;PACKAGE&gt;/src/vectors.S
        $(CC) -Wp,-MD,vectors.tmp $(INCLUDE_PATH) $(CFLAGS) -c -o $@ $&lt;
        @echo $@ ": \\" &gt; $(notdir $@).deps
        @tail +2 vectors.tmp &gt;&gt; $(notdir $@).deps
        @echo &gt;&gt; $(notdir $@).deps
        @rm vectors.tmp
    }

    make {
        &lt;PREFIX&gt;/lib/target.ld: &lt;PACKAGE&gt;/src/i386.ld
        $(CC) -E -P -Wp,-MD,target.tmp -DEXTRAS=1 -xc $(INCLUDE_PATH) $(CFLAGS) -o $@ $&lt;
        @echo $@ ": \\" &gt; $(notdir $@).deps
        @tail +2 target.tmp &gt;&gt; $(notdir $@).deps
        @echo &gt;&gt; $(notdir $@).deps
        @rm target.tmp
    }
</programlisting>

<para>
The i386 is currently the only architecture that supports SMP. The
following CDL simply enabled the HAL SMP support if
required. Generally this will get enabled as a result of a
<literal>requires</literal> statement in the kernel. The
<literal>requires</literal> statement here turns off lazy FPU
switching in the FPU support code, since it is inconsistent with SMP
operation.
</para>

<programlisting width=72>

    cdl_component CYGPKG_HAL_SMP_SUPPORT {
	display       "SMP support"
	default_value 0
	requires { CYGHWR_HAL_I386_FPU_SWITCH_LAZY == 0 }
	
	cdl_option CYGPKG_HAL_SMP_CPU_MAX {
	    display       "Max number of CPUs supported"
	    flavor        data
	    default_value 2
	}
    }
</programlisting>

<para>
The i386 HAL has optional FPU support, which is enabled by default. It
can be disabled to improve system performance. There are two FPU
support options: either to save and restore the FPU state on every
context switch, or to only switch the FPU state when necessary.
</para>

<programlisting width=72>
        
    cdl_component CYGHWR_HAL_I386_FPU {
	display       "Enable I386 FPU support"
	default_value 1
	description   "This component enables support for the
	              I386 floating point unit."

	cdl_option CYGHWR_HAL_I386_FPU_SWITCH_LAZY {
	    display       "Use lazy FPU state switching"
	    flavor        bool
	    default_value 1

	    description "
	                This option enables lazy FPU state switching.
                        The default behaviour for eCos is to save and
                        restore FPU state on every thread switch, interrupt
	                and exception. While simple and deterministic, this
	                approach can be expensive if the FPU is not used by
	                all threads. The alternative, enabled by this option,
	                is to use hardware features that allow the FPU state
	                of a thread to be left in the FPU after it has been
	                descheduled, and to allow the state to be switched to
	                a new thread only if it actually uses the FPU. Where
	                only one or two threads use the FPU this can avoid a
	                lot of unnecessary state switching."
	}
    }
</programlisting>

<para>
The i386 HAL also has support for different classes of CPU. In
particular, Pentium class CPUs have extra functional units, and some
variants of GDB expect more registers to be reported. These options
enable these features. Generally these are enabled by
<literal>requires</literal> statements in variant or platform
packages, or in <literal>.ecm</literal> files.
</para>

<programlisting width=72>

    cdl_component CYGHWR_HAL_I386_PENTIUM {
	display       "Enable Pentium class CPU features"
	default_value 0
	description   "This component enables support for various
	              features of Pentium class CPUs."

	cdl_option CYGHWR_HAL_I386_PENTIUM_SSE {
	    display       "Save/Restore SSE registers on context switch"
	    flavor        bool
	    default_value 0

	    description "
	                This option enables SSE state switching. The default
                        behaviour for eCos is to ignore the SSE registers.
                        Enabling this option adds SSE state information to
                        every thread context."
	}

	cdl_option CYGHWR_HAL_I386_PENTIUM_GDB_REGS {
	    display       "Support extra Pentium registers in GDB stub"
	    flavor        bool
	    default_value 0

	    description "
	                This option enables support for extra Pentium registers
			in the GDB stub. These are registers such as CR0-CR4, and
                        all MSRs. Not all GDBs support these registers, so the
                        default behaviour for eCos is to not include them in the
			GDB stub support code."
	}
    }
</programlisting>

<para>
In the i386 HALs, the linker script is provided by the architecture
HAL. In other HALs, for example MIPS, it is provided in the variant
HAL. The following option provides the name of the linker script to
other elements in the configuration system.
</para>

<programlisting width=72>
    cdl_option CYGBLD_LINKER_SCRIPT {
        display "Linker script"
        flavor data
	no_define
        calculated  { "src/i386.ld" }
    }
</programlisting>

<para>
Finally, this interface indicates whether the platform supplied an
implementation of the
<function>hal_i386_mem_real_region_top()</function> function. If it
does then it will contain a line of the form: <literal>implements
CYGINT_HAL_I386_MEM_REAL_REGION_TOP</literal>. This allows packages
such as RedBoot to detect the presence of this function so that they
may call it.
</para>

<programlisting width=72>

    cdl_interface CYGINT_HAL_I386_MEM_REAL_REGION_TOP {
        display  "Implementations of hal_i386_mem_real_region_top()"
    }
    
}
</programlisting>

</section>

<!-- }}} -->

<!--
<para><a href="hal-arch-process.html">Porting process</a>
<para><a href="hal-cache.html">HAL Cache Controls</a>
<para><a href="hal-linking.html">Linker Script Macros</a>
<para><a href="hal-arch-cdl.html">CDL requirements</a>

-->

</section>

<!-- }}} -->

</CHAPTER>

<!--

Notes added by Nickg:

The following are my notes from the HAL Porting course I did at
Agilent in Feb 2002. It was my intention to incorporate some stuff
from here into the Platform Porting section and to include some of
the things I learned while doing the course. The main things I wanted
to do were: to change the porting process to concentrate on getting
RedBoot to run rather than the GDB stubs ROM; update the descriptions
to match current practice - some of it is now quite old; remove all
the TBDs and FIXMEs; mend the worst of Jesper's danglish :-)

Also the variant and architecture porting guides are still in the
incomplete state that Jesper left them; and there are some other bits
and pieces in the original HTML porting guide that I have not yet
moved over.

The ridiculous demands of management to sacrifice quality to
expediency mean that this is not now possible and this document has to
be abandoned in mid-flux. So I'm just dumping this stuff here. Maybe
one day someone will get around to doing it properly.




Porting Principals
==================

Copy an existing HAL.
     - choose a HAL with which you are familiar and/or which is
       similar to the intended target.
     - copy the files
     - rename them appropriately
     - rename configuration variables
     - empty/reimplement platform specific code.
       - old code is a good indicator of what you need to do.
       - concentrate on getting it all to compile, so just commenting
         out the platform specific bits is often a good idea.

Follow execution order.
     - gives a good indication of what to do next.

Concentrate on RedBoot first.
     - simpler environment - no interrupts, no threads.


CDL
===

CDL changes made as part of the copy/edit above should be done.

Need to add entries to ecos.db for the new packages.

Platform:

package CYGPKG_HAL_ARM_ARM9_XXXXXXXX {
	alias		{ "XXXXXXXX unit" hal_arm_arm9_xxxxxxxx xxxxxxxx }
	directory	hal/arm/arm9/xxxxxxxx
	script		hal_arm_arm9_xxxxxxxx.cdl
	hardware
        description "
        The XXXXXXXX HAL package provides the support needed to run
        eCos on an XXXXXXXX board."
}

Target:

target xxxxxxxx {
	alias { "XXXXXXXX unit" aaed }
	packages { CYGPKG_HAL_ARM
                   CYGPKG_HAL_ARM_ARM9
                   CYGPKG_HAL_ARM_ARM9_XXXXXXXX
        }
        description "
        The XXXXXXXX target provides the packages needed to run
        eCos on an XXXXXXXX board."
}

==================================================================

Getting RedBoot Going
=====================

Startup
=======

1. Reset entry point. At location 0.
   Transfer control to ROM entry point: reset_vector.

2. Here we call invoke PLATFORM_SETUP1 macro. This does the following:
   - disable interrupts
   - disable and clear caches
   - Init memory controllers. may involve discovery of what RAM is
     present.
   - Set up clock frequencies.
   - Init MMU table
     - sets up TTBR and DACR to default values
     - fills in MMU table to map
       - DRAM at 0x00000000 cacheable/buffered
       - Device registers elsewhere uncacheable/unbuffered usually 1-1
       - DRAM at 0xF0000000 uncacheable/unbuffered (1-1 in aaed2000)
       - remap ROM at 0 elsewhere
   - Enable MMU
   - Relocate image to RAM for ROMRAM startup
   - Any other CPU setup required
      
3. Jump to HAL startup.
   - Plant vector intructions at 0+
   - copy .data section to RAM
   - Init CPSR and SPSR
   - Set SP
   - Clear .bss
   - Call hal_hardware_init()
   - call initialize_stub() if GDB stubs included
   - call hal_ctrlc_isr_init()
   - call cyg_hal_invoke_constructors()
   - call cyg_start()


HAL Serial support
==================

Set up CDL in platform CDL file.
    CYGNUM_HAL_VIRTUAL_VECTOR_COMM_CHANNELS
	number of channels usually 0, 1 or 2
    CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL
	channel to use for GDB
    CYGNUM_HAL_VIRTUAL_VECTOR_DEBUG_CHANNEL_BAUD
	initial baud rate
    CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL
	channel to use for console
    CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL_BAUD
	initial baud rate
    CYGNUM_HAL_VIRTUAL_VECTOR_CONSOLE_CHANNEL_DEFAULT
	default console channel

The code in hal_diag.c need to be converted to the new serial device.
If this the same as a device already supported, copy that.

Things that need to be written:

struct channel_data_t;
       Structure containing base address, timeout and ISR vector
       number for each serial device.

xxxx_ser_channels[];
	Array of channel_data_t, initialized with parameters of each
	channel.

void cyg_hal_plf_serial_init_channel(void *__ch_data)
	Initialize the serial device. parameter is a pointer to a
	channel_data_t.

void cyg_hal_plf_serial_putc(void * __ch_data, char *c)
        Send a character to the serial device.
	Poll for ready, write the char.
	Maybe poll for char sent.

bool cyg_hal_plf_serial_getc_nonblock(void* __ch_data, cyg_uint8* ch)
        Look for a character and return it if available.
	If none available, return false.

int cyg_hal_plf_serial_control(void *__ch_data, __comm_control_cmd_t
__func, ...)
	An IOCTL-like function for controlling various aspects of the
	serial device.
	May need to do some work in __COMMCTL_IRQ_ENABLE and
	__COMMCTL_IRQ_DISABLE cases to enable/disable interrupts.

int cyg_hal_plf_serial_isr(void *__ch_data, int* __ctrlc, 
                       CYG_ADDRWORD __vector, CYG_ADDRWORD __data)
        Interrupt handler, specifically for dealing with Ctrl-C.
	- Check for an incoming character.
	- Read the character and call cyg_hal_is_break().
	- If result is true, set *__ctrlc to 1.
	- return CYG_ISR_HANDLED;

void cyg_hal_plf_serial_init()
        Initialize each of the serial channels.
	- call cyg_hal_plf_serial_init_channel() for each channel.
	- call CYGACC_COMM_IF_* macros for each channel -
          cut/paste/edit these.

		
Interrupt Controller
====================

ARM platforms have interrupt controller access in functions in variant
or platform source file.

void hal_interrupt_mask(int vector)
        Manipulate interrupt controller to mask the interrupt.

void hal_interrupt_unmask(int vector)
        Manipulate interrupt controller to unmask the interrupt.

void hal_interrupt_acknowledge(int vector)
        Manipulate interrupt controller to acknowledge the interrupt.
	May not be needed in some platforms.

void hal_interrupt_configure(int vector, int level, int up)
        Set interrupt detection: level vs. edge; high/low
        rising/falling.
	Leave empty where not implemented.	

void hal_interrupt_set_level(int vector, int level)
        Set interrupt priority level.
	Leave empty where not implemented.	


Redboot Configuration
=====================

Having done all of the above, you should be in a position to get
RedBoot running.

If the platform you copied has redboot, there should be some .ecm
files in the misc directory. Named redboot_<startup>.ecm.

Choose a startup and edit the .ecm file.
       - remove any options that are not relevant
       - comment out FLASH, ETH and COMPRESS packages

Configure for redboot:

% setenv ECOS_REPOSITORY <path to source repository>
% ecosconfig new xxxxxxxx redboot
% ecosconfig import $ECOS_REPOSITORY/hal/arm/arm9/xxxxxxxx/current/misc/redboot_ROM.ecm
% ecosconfig tree
% make

Repeat until successful.

Load into hardware by either programming FLASH from existing ROM
monitor, via JTAG or whatever.

Run. Debug. Edit. Repeat.

==================================================================

Getting eCos Going
==================

Once RedBoot is up and running, it should be possible to configure and
build eCos.

Use the kernel template to start with.


Clock Support
=============

We will use the RTC to test that interrupts are working. First step is
to get RTC working.

void hal_clock_initialize(cyg_uint32 period)
     Initialize the RTC device to interrupt every period ticks. The
     CDL should have defined period according to the frequency
     required.
     This should start the clock going.

void hal_clock_reset(cyg_uint32 vector, cyg_uint32 period)
     Perform any work to cause the clock to start another timing
     period. On many platforms this can be empty. On others the
     counter or compare register may need to be reloaded.

void hal_clock_read(cyg_uint32 *pvalue)
     Returns the number of hardware ticks since the last interrupt.
     For count-up timers this is just the value of the timer.
     For count-down timers the result needs to be subtracted from the
     initial period.

void hal_delay_us(cyg_int32 usecs)
     Busy delay for the given number of microseconds.
     Normally this works by polling the timer device until the
     required number of usecs has passed.
     Beware of timer wrap-around, resets, and arithmetic overflows.
     This function does not have to be very accurate - it's used
     mostly to provide short timing delays during hardware access.

Interrupt Handling
==================

Quick overview of interrupt handling:


1. Hardware interrupts are delivered to either the IRQ or FIQ vectors at
   0x18 and 0x1c respectively.

2. These contain single instructions that load the contents of the memory
   location 0x20 later in memory and jump there.

3. The code called is a VSR - Vector Service Routine. FIQ VSR fakes
   CPU state to make it look like an IRQ, then drops into IRQ.

4. Switch back to supervisor mode. Save CPU state onto current stack. 

5. Switch to interrupt stack if not already there.

6. Lock scheduler.

7. Call hal_IRQ_handler(). This function inspects the interrupt
   controller and returns the number of the highest priority pending,
   unmasked interrupt.

8. Use vector number to index hal_interrupt_handlers[] and
   hal_interrupt_data[] to get ISR and data.

9. Call ISR. keep the return value.

10. Switch back to original stack.

11. Index hal_interrupt_objects[] with vector number to get interrupt
    object pointer.

12. Call interrupt_end(isr_ret, *object, *save_regs).
    This will:
    - post the onterrupt object's DSR if CYG_ISR_CALL_DSR is set in
      return code.
    - Unlock scheduler. During this the following may happen:
      - Any pending DSRs may be called
      - The current thread may be preempted, either by a higher
        priority thread scheduled by a DSR, or it may be timesliced.

13. The return from interrupt_end() may occur some time after the
    call: lots of threads may have run in the meantime.

14. Restore CPU state and resume interrupted code.


The only thing that needs doing in a platform port is to write
hal_IRQ_handler().



Once the clock and IRQ code is done, eCos should be able to run all of
the kernel tests. The best all-round test is tm_basic. Other tests
that should be run are:
     clocktruth - tests accuracy of timer setup
     except1 - checks exception handling works
     timeslice - checks timeslicing works

Run. Debug. Edit. Repeat.




-->


