<!-- DOCTYPE refentry  PUBLIC "-//OASIS//DTD DocBook V3.1//EN" -->

<!-- {{{ Banner                         -->

<!-- =============================================================== -->
<!--                                                                 -->
<!--     ds1307.sgml                                                 -->
<!--                                                                 -->
<!--     Documentation for the ds1307 wallclock driver               -->
<!--                                                                 -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTBEGIN####                                   -->
<!-- =============================================================== -->
<!-- Copyright (C) 2004 Free Software Foundation, Inc.               -->
<!-- This material may be distributed only subject to the terms      -->
<!-- and conditions set forth in the Open Publication License, v1.0  -->
<!-- or later (the latest version is presently available at          -->
<!-- http://www.opencontent.org/openpub/)                            -->
<!-- Distribution of the work or derivative of the work in any       -->
<!-- standard (paper) book form is prohibited unless prior           -->
<!-- permission obtained from the copyright holder                   -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTEND####                                     -->
<!-- =============================================================== -->
<!-- =============================================================== -->
<!-- #####DESCRIPTIONBEGIN####                                       -->
<!--                                                                 -->
<!-- Author(s):   bartv                                              -->
<!-- Contact(s):  bartv                                              -->
<!-- Date:        2004/10/09                                         -->
<!-- Version:     0.01                                               -->
<!--                                                                 -->
<!-- ####DESCRIPTIONEND####                                          -->
<!-- =============================================================== -->

<!-- }}} -->

<part id="devs-wallclock-dallas-ds1307-part"><title>Dallas DS1307 Wallclock Device Driver</title>

<refentry id="devs-wallclock-dallas-ds1307">
  <refmeta>
    <refentrytitle>Dallas DS1307 Wallclock Device Driver</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname><varname>CYGPKG_DEVICES_WALLCLOCK_DALLAS_DS1307</varname></refname>
    <refpurpose>eCos Support for the Dallas DS1307 Serial Real-Time Clock</refpurpose>
  </refnamediv>

  <refsect1 id="devs-wallclock-dallas-ds1307-description"><title>Description</title>
    <para>
This package
<varname>CYGPKG_DEVICES_WALLCLOCK_DALLAS_DS1307</varname> provides a
device driver for the wallclock device in the Dallas DS1307 Serial
Real-Time Clock chips. This combines a real-time clock and 56 bytes of
battery-backed RAM in a single package. The driver can also be used
with any other chips that provide the same interface to the clock
hardware.
    </para>
    <para>
The package will usually be loaded into the configuration
automatically whenever selecting a target which contains a compatible
chip. By default it will provide the standard eCos wallclock device,
although another implementation such as software emulation may be
selected if desired. The only other configuration options related to
this package allow users to change the compiler flags. If the
application does not actually use the wallclock device, directly or
indirectly, then the code should get removed automatically at
link-time to ensure that the application does not suffer any
unnecessary overheads.
    </para>
  </refsect1>

  <refsect1 id="devs-wallclock-dallas-ds1307-functions"><title>Functionality</title>
    <para>
This wallclock device driver package implements the standard
functionality required by the generic wallclock support
<varname>CYGPKG_IO_WALLCLOCK</varname>. The functionality is not
normally accessed directly. Instead it is used by the C library time
package to implement standard calls such as <function>time</function>
and <function>gmtime</function>. The eCos C library also provides a
non-standard function <function>cyg_libc_time_settime</function> for
changing the current wallclock setting. In addition RedBoot provides
a <command>date</command> command which interacts with the wallclock
device.
    </para>
  </refsect1>

  <refsect1 id="devs-wallclock-dallas-ds1307-porting"><title>Porting</title>
    <para>
DS1307 platform support can be implemented in one of two ways. The
preferred approach involves the generic I2C API, as defined by the
package <varname>CYGPKG_IO_I2C</varname>. The platform HAL can just
provide a <structname>cyg_i2c_device</structname> structure
<varname>cyg_i2c_wallclock_ds1307</varname> and implement the CDL
interface
<varname>CYGINT_DEVICES_WALLCLOCK_DALLAS_DS1307_I2C</varname>. The
DS1307 driver will now use I2C rx and tx operations to interact with
the chip.
    </para>
    <para>
Alternatively the DS1307 driver can use macros or functions provided
by another package to access the chip. This is intended primarily for
older platforms that predate the <varname>CYGPKG_IO_I2C</varname>
package. The other package should export a header file containing
macros <function>DS_GET</function> and <function>DS_PUT</function>
that transfer the eight bytes corresponding to the chip's clock
registers. It should also export the name of this header via a
<literal>#define</literal>
<varname>CYGDAT_DEVS_WALLCLOCK_DS1307_INL</varname> in the global
configuration header <filename
class="headerfile">pkgconf/system.h</filename>. For full details see
the source code.
    </para>
    <para>
In addition the DS1307 device driver package
<varname>CYGPKG_DEVICES_WALLCLOCK_DALLAS_DS1307</varname> should be
included in the CDL target entry so that it gets loaded automatically
whenever eCos is configured for that target.
    </para>
  </refsect1>

</refentry>

</part>
