<!-- DOCTYPE part  PUBLIC "-//OASIS//DTD DocBook V3.1//EN" -->

<!-- {{{ Banner                                                     -->

<!-- =============================================================== -->
<!--                                                                 -->
<!--     ek_lm3s811.sgml                                             -->
<!--                                                                 -->
<!--     ek_lm3s811 board documentation.                             -->
<!--                                                                 -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTBEGIN####                                   -->
<!-- =============================================================== -->
<!-- Copyright (C) 2011 Free Software Foundation, Inc. -->
<!-- This material may be distributed only subject to the terms      -->
<!-- and conditions set forth in the Open Publication License, v1.0  -->
<!-- or later (the latest version is presently available at          -->
<!-- http://www.opencontent.org/openpub/)                            -->
<!-- Distribution of the work or derivative of the work in any       -->
<!-- standard (paper) book form is prohibited unless prior           -->
<!-- permission obtained from the copyright holder                   -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTEND####                                     -->
<!-- =============================================================== -->
<!-- #####DESCRIPTIONBEGIN####                                       -->
<!--                                                                 -->
<!-- Author(s):   ccoutand                                           -->
<!-- Contact(s):  ccoutand                                           -->
<!-- Date:        2011/01/18                                         -->
<!-- Version:     0.01                                               -->
<!--                                                                 -->
<!-- ####DESCRIPTIONEND####                                          -->
<!-- =============================================================== -->

<!-- }}} -->

<part id="hal-cortexm-lm3s-ek_lm3s811"><title>Stellaris EKK-LM3S811 Board Support</title>

<refentry id="lm3s-ek_lm3s811">
  <refmeta>
    <refentrytitle>Overview</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname>eCos Support for the Stellaris EKK-LM3S811 Board</refname>
    <refpurpose>Overview</refpurpose>
  </refnamediv>

  <refsect1 id="lm3s-ek_lm3s811-description"><title>Description</title>
    <para>
The Stellaris EKK-LM3S811 evaluation kit uses the Stellaris LM3S811 microcontroller from the 
800 Series. The LM3S811 is an ARM cortex-M3 based microcontroller with 64KB of FLASH 
and 8KB of SRAM. The device has various peripherals such as UART, I2C, ADC or Analog
Comparator. The kit features an OLED graphical display and UART0 is accessible via the 
on-board USB to UART converter.
    </para>
    <para>
Due to extreme limited RAM ressources (8KB SRAM only), the eCos port targets standalone ROM  
application using the eCos kernel in single user thread environment. The cortex-M architecture HAL 
requires a seperate stack to handle interrupts, thus the minimum kernel enable application requires 3 
stacks. The interrupt stack, the Idle thread stack and the user stack. All stacks are set to the architecture 
minimum allowed size of CYGNUM_HAL_STACK_SIZE_MINIMUM ( 1360 bytes ). 
    </para>
  </refsect1>

  <refsect1 id="lm3s-ek_lm3s811-config"><title>Configuration</title>
    <para>
The minimum board configuration includes the Microcontroller HAL alongs with the ADC and I2C device 
drivers.
    </para>
    <variablelist>
      <varlistentry>
        <term><varname>LM3S811 Microcontroller</varname></term>
        <listitem>
        <para>
CYGPKG_HAL_CORTEXM_LM3S8XX - The microcontroller configuration 
requirements are minimal. With the default setup, the microcontroller runs from the 
external clock source, a crystal of 6MHz. The chip internal PLL generates a fix 
200MHz clock that is divided down to the default system clock frequency of 50MHz. 
In this scenario, the device uses full processing power. The system clock divider 
allows down scaling of the system clock frequency to reduce the overall power 
consumption of the device. The microcontroller also offers the option to run from an
internal oscillator. This option has 2 modes, 3MHz or 12MHz. When selecting the
internal oscillator, the PLL is bypassed. The system clock frequency becomes at
best 12MHz if no further clock division is applied.
        </para>
        </listitem>
      </varlistentry>

      <varlistentry>
        <term><varname>I2C Interface</varname></term>
        <listitem><para>
CYGPKG_DEVS_I2C_CORTEXM_LM3S - The microcontroller uses the I2C bus 
to communicate with the SD1300 controller of the OLED 96 x 16 display. The SD1300 
controller eCos driver is not currently available.
The I2C is default set to use the low frequency mode ( 100KHz bus clock ). The high 
frequency mode ( 400 KHz ) is available by changing CYGNUM_HAL_CORTEXM_LM3S_I2C_CLK_SPEED.
        </para></listitem>
      </varlistentry>
      <varlistentry>
        <term><varname>ADC Interface</varname></term>
        <listitem><para>
CYGPKG_DEVS_ADC_CORTEXM_LM3S - The LM3S811 includes 4 ADC channels including an
optional internal temperature probe. There are many ways to use the on-chip ADC.
The current eCos driver uses a single sequencer (sequencer 0) to schedule sampling of all 
channels. This practically means that all channels are sampled from the same trigger, a periodic timer
interrupt in the current driver. The timer to use
is selected from CYGNUM_DEVS_ADC_CORTEXM_LM3S_ADC0_SELECT_TIMER, with timer 0 as
default value. The timer is used in 32 bits periodic mode, therefore cannot be re-used
for any other user purpose. While the ADC has the possibility to trigger sampling on external 
IO events, the driver does not offer that flexibility. Finally, the driver only allows measurement of
single-ended IOs.
        </para></listitem>
      </varlistentry>
    </variablelist>
  </refsect1>

  <refsect1 id="lm3s-ek_lm3s811-rebuild"><title>Build ROM type applications</title>
    <para>
The steps needed to build the HAL library for the EKK-LM3S811 board are:
    </para>
    <screen>
$ mkdir ek_lm3s811
$ cd ek_lm3s811
$ ecosconfig new ek-lm3s811 minimal
$ ecosconfig import $ECOS_REPOSITORY/hal/cortexm/lm3s/ek_lm3s811/current/misc/default_ROM.ecm
$ ecosconfig resolve
$ ecosconfig tree
$ make
    </screen>
    <para>
At the end of the build the <filename
class="directory">install/lib</filename> subdirectory should contain the library and linker script and the <filename
class="directory">install/include</filename> subdirectory the necessary includes to compile the application.
    </para>
  </refsect1>


</refentry>

</part>
