<!-- DOCTYPE part  PUBLIC "-//OASIS//DTD DocBook V3.1//EN" -->

<!-- {{{ Banner                         -->

<!-- =============================================================== -->
<!--                                                                 -->
<!--     spi.sgml                                                    -->
<!--                                                                 -->
<!--     Generic SPI documentation.                                  -->
<!--                                                                 -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTBEGIN####                                   -->
<!-- =============================================================== -->
<!-- Copyright (C) 2004, 2009 Free Software Foundation, Inc.         -->
<!-- This material may be distributed only subject to the terms      -->
<!-- and conditions set forth in the Open Publication License, v1.0  -->
<!-- or later (the latest version is presently available at          -->
<!-- http://www.opencontent.org/openpub/)                            -->
<!-- Distribution of the work or derivative of the work in any       -->
<!-- standard (paper) book form is prohibited unless prior           -->
<!-- permission obtained from the copyright holder                   -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTEND####                                     -->
<!-- =============================================================== -->
<!-- #####DESCRIPTIONBEGIN####                                       -->
<!--                                                                 -->
<!-- Author(s):   bartv                                              -->
<!-- Date:        2004/04/23                                         -->
<!--                                                                 -->
<!-- ####DESCRIPTIONEND####                                          -->
<!-- =============================================================== -->

<!-- }}} -->

<part id="io-spi"><title>SPI Support</title>

<refentry id="spi">
  <refmeta>
    <refentrytitle>Overview</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname>Overview</refname>
    <refpurpose>eCos Support for SPI, the Serial Peripheral Interface</refpurpose>
  </refnamediv>

  <refsect1 id="spi-description"><title>Description</title>
    <para>
The Serial Peripheral Interface (SPI) is one of a number of serial bus
technologies. It can be used to connect a processor to one or more
peripheral chips, for example analog-to-digital convertors or real
time clocks, using only a small number of pins and PCB tracks. The
technology was originally developed by Motorola but is now also
supported by other vendors.
    </para>
    <para>
A typical SPI system might look like this:
    </para>
    <informalfigure PgWide=1>
      <mediaobject>
        <imageobject>
          <imagedata fileref="spi_net.png" Scalefit=1 Align="Center">
        </imageobject>
      </mediaobject>
    </informalfigure>
    <para>
At the start of a data transfer the master cpu asserts one of the chip
select signals and then generates a clock signal. During each clock
tick the cpu will output one bit on its master-out-slave-in line and
read one bit on the master-in-slave-out line. Each device is connected
to the clock line, the two data lines, and has its own chip select. If
a device's chip select is not asserted then it will ignore any
incoming data and will tristate its output. If a device's chip select
is asserted then during each clock tick it will read one bit of data
on its input pin and output one bit on its output pin.
    </para>
    <para>
The net effect is that the cpu can write an arbitrary amount of data
to one of the attached devices at a time, and simultaneously read the
same amount of data. Some devices are inherently uni-directional. For
example an LED unit would only accept data from the cpu: it will not
send anything meaningful back; the cpu will still sample its input
every clock tick, but this should be discarded.
    </para>
    <para>
A useful feature of SPI is that there is no flow control from the
device back to the cpu. If the cpu tries to communicate with a device
that is not currently present, for example an MMC socket which does
not contain a card, then the I/O will still proceed. However the cpu
will read random data. Typically software-level CRC checksums or
similar techniques will be used to allow the cpu to detect this.
    </para>
    <para>
SPI communication is not fully standardized. Variations between
devices include the following:
    </para>
    <orderedlist>
      <listitem><para>
Many devices involve byte transfers, where the unit of data is 8 bits.
Others use larger units, up to 16 bits.
      </para></listitem>
      <listitem><para>
Chip selects may be active-high or active-low. If the attached devices
use a mixture of polarities then this can complicate things.
      </para></listitem>
      <listitem><para>
Clock rates can vary from 128KHz to 20MHz or greater. With some
devices it is necessary to interrogate the device using a slow clock,
then use the obtained information to select a faster clock for
subsequent transfers.
      </para></listitem>
      <listitem><para>
The clock is inactive between data transfers. When inactive the
clock's polarity can be high or low.
      </para></listitem>
      <listitem><para>
Devices depend on the phase of the clock. Data may be sampled on
either the rising edge or the falling edge of the clock.
      </para></listitem>
      <listitem><para>
A device may need additional delays, for example between asserting
the chip select and the first clock tick.
      </para></listitem>
      <listitem><para>
Some devices involve complicated transactions: perhaps a command from
cpu to device; then an initial status response from the device; a data
transfer; and a final status response. From the cpu's perspective
these are separate stages and it may be necessary to abort the
operation after the initial status response. However the device may
require that the chip select remain asserted for the whole
transaction. A side effect of this is that it is not possible to do a
quick transfer with another device in the middle of the transaction.
      </para></listitem>
      <listitem><para>
Certain devices, for example MMC cards, depend on a clock signal after
a transfer has completed and the chip select has dropped. This clock
is used to finish some processing within the device.
      </para></listitem>
    </orderedlist>
    <para>
Inside the cpu the clock and data signals are usually managed by
dedicated hardware. Alternatively SPI can be implemented using
bit-banging, but that approach is normally used for other serial bus
technologies such as I2C. The chip selects may also be implemented by
the dedicated SPI hardware, but often GPIO pins are used instead.
    </para>
  </refsect1>

  <refsect1 id="spi-ecos-implementation"><title>eCos Support for SPI</title>
    <para>
The eCos SPI support for any given platform is spread over a number of
different packages:
    </para>
    <itemizedlist>
      <listitem><para>
This package, <varname>CYGPKG_IO_SPI</varname>, exports an API for
accessing devices attached to an SPI bus. This API handles issues such
as locking between threads. The package does not contain any
hardware-specific code, instead it will call into an SPI bus driver
package.
      </para>
      <para>
In future this package may be extended with a bit-banging
implementation of an SPI bus driver. This would depend on lower-level
code for manipulating the GPIO pins used for the clock, data and chip
select signals, but timing and framing could be handled by generic code.
      </para></listitem>
      <listitem><para>
There will be a bus driver package for the specific SPI hardware on
the target hardware, for example
<varname>CYGPKG_DEVS_SPI_MCF52xx_QSPI</varname>. This is responsible
for the actual I/O. A bus driver may be used on many different boards,
all with the same SPI bus but with different devices attached to that
bus. Details of the actual devices should be supplied by other code.
      </para></listitem>
      <listitem><para>
The generic API depends on <structname>cyg_spi_device</structname>
data structures. These contain the information needed by a bus driver,
for example the appropriate clock rate and the chip select to use.
Usually the data structures are provided by the platform HAL since it
is that package which knows about all the devices on the board.
      </para>
      <para>
On some development boards the SPI pins are brought out to expansion
connectors, allowing end users to add extra devices. In such cases the
platform HAL may not know about all the devices on the board. Data
structures for the additional devices can instead be supplied by
application code.
      </para></listitem>
      <listitem><para>
Some types of SPI devices may have their own driver package. For
example one common use for SPI buses is to provide low-cost
MultiMediaCard (MMC) support. An MMC is a non-trivial device so there
is an eCos package specially for that, providing a block device
interface for higher-level code such as file systems. Other SPI
devices such as analog-to-digital converters are much simpler and
come in many varieties. There are no dedicated packages to support
each such device: the chances are low that another board would use the
exact same device, so there are no opportunities for code re-use.
Instead the devices may be accessed directly by application code or by
extra functions in the platform HAL.
      </para></listitem>
    </itemizedlist>
    <para>
Typically all appropriate packages will be loaded automatically when
you configure eCos for a given target. If the application does not use
any of the SPI I/O facilities, directly or indirectly, then linker
garbage collection should eliminate all unnecessary code and data. All
necessary initialization should happen automatically. However the
exact details may depend on the target, so the platform HAL
documentation should be checked for further details.
    </para>
    <para>
There is one important exception to this: if the SPI devices are
attached to an expansion connector then the platform HAL will not know
about these devices. Instead more work will have to be done by
application code.
    </para>
  </refsect1>

</refentry>

<refentry id="spi-api">
  <refmeta>
    <refentrytitle>SPI Interface</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname>SPI Functions</refname>
    <refpurpose>allow applications and other packages to access SPI devices</refpurpose>
  </refnamediv>
  <refsynopsisdiv>
    <funcsynopsis>
      <funcsynopsisinfo>
#include &lt;cyg/io/spi.h&gt;
      </funcsynopsisinfo>
      <funcprototype>
        <funcdef>void <function>cyg_spi_transfer</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_bool <parameter>polled</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>count</parameter></paramdef>
        <paramdef>const cyg_uint8* <parameter>tx_data</parameter></paramdef>
        <paramdef>cyg_uint8* <parameter>rx_data</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>void <function>cyg_spi_tick</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_bool <parameter>polled</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>count</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>int <function>cyg_spi_get_config</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>key</parameter></paramdef>
        <paramdef>void* <parameter>buf</parameter></paramdef>
        <paramdef>cyg_uint32* <parameter>len</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>int <function>cyg_spi_set_config</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>key</parameter></paramdef>
        <paramdef>const void* <parameter>buf</parameter></paramdef>
        <paramdef>cyg_uint32* <parameter>len</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>void <function>cyg_spi_transaction_begin</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>cyg_bool <function>cyg_spi_transaction_begin_nb</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>void <function>cyg_spi_transaction_transfer</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_bool <parameter>polled</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>count</parameter></paramdef>
        <paramdef>const cyg_uint8* <parameter>tx_data</parameter></paramdef>
        <paramdef>cyg_uint8* <parameter>rx_data</parameter></paramdef>
        <paramdef>cyg_bool <parameter>drop_cs</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>void <function>cyg_spi_transaction_tick</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
        <paramdef>cyg_bool <parameter>polled</parameter></paramdef>
        <paramdef>cyg_uint32 <parameter>count</parameter></paramdef>
      </funcprototype>
      <funcprototype>
        <funcdef>void <function>cyg_spi_transaction_end</function></funcdef>
        <paramdef>cyg_spi_device* <parameter>device</parameter></paramdef>
      </funcprototype>
    </funcsynopsis>
  </refsynopsisdiv>

  <refsect1 id="spi-api-description"><title>Description</title>
    <para>
All SPI functions take a pointer to a
<structname>cyg_spi_device</structname> structure as their first
argument. This is an opaque data structure, usually provided by the
platform HAL. It contains the information needed by the SPI bus driver
to interact with the device, for example the required clock rate and
polarity.
    </para>
    <para>
An SPI transfer involves the following stages:
    </para>
    <orderedlist>
      <listitem><para>
Perform thread-level locking on the bus. Only one thread at a time is
allowed to access an SPI bus. This eliminates the need to worry about
locking at the bus driver level. If a platform involves multiple SPI
buses then each one will have its own lock. Prepare the bus for
transfers to the specified device, for example by making sure it will
tick at the right clock rate.
      </para></listitem>
      <listitem><para>
Assert the chip select on the specified device, then transfer data to
and from the device. There may be a single data transfer or a
sequence. It may or may not be necessary to keep the chip select
asserted throughout a sequence.
      </para></listitem>
      <listitem><para>
Optionally generate some number of clock ticks without asserting a
chip select, for those devices which need this to complete an
operation.
      </para></listitem>
      <listitem><para>
Return the bus to a quiescent state. Then unlock the bus, allowing
other threads to perform SPI operations on devices attached to this
bus.
      </para></listitem>
    </orderedlist>
    <para>
The simple functions <function>cyg_spi_transfer</function> and
<function>cyg_spi_tick</function> perform all these steps in a single
call. These are suitable for simple I/O operations. The alternative
transaction-oriented functions each perform just one of these steps.
This makes it possible to perform multiple transfers while only
locking and unlocking the bus once, as required for more complicated
devices.
    </para>
    <para>
With the exception of
<function>cyg_spi_transaction_begin_nb</function> all the functions
will block until completion. There are no error conditions. An SPI
transfer will always take a predictable amount of time, depending on
the transfer size and the clock rate. The SPI bus does not receive any
feedback from a device about possible errors, instead those have to be
handled by software at a higher level. If a thread cannot afford the
time it will take to perform a complete large transfer then a number
of smaller transfers can be used instead.
    </para>
    <para>
SPI operations should always be performed at thread-level or during
system initialization, and not inside an ISR or DSR. This greatly
simplifies locking. Also a typical ISR or DSR should not perform a
blocking operation such as an SPI transfer.
    </para>
    <para>
SPI transfers can happen in either polled or interrupt-driven mode.
Typically polled mode should be used during system initialization,
before the scheduler has been started and interrupts have been
enabled. Polled mode should also be used in single-threaded
applications such as RedBoot. A typical multi-threaded application
should normally use interrupt-driven mode because this allows for more
efficient use of cpu cycles. Polled mode may be used in a
multi-threaded application but this is generally undesirable: the cpu
will spin while waiting for a transfer to complete, wasting cycles;
also the current thread may get preempted or timesliced, making the
timing of an SPI transfer much less predictable. On some hardware
interrupt-driven mode is impossible or would be very inefficient. In
such cases the bus drivers will only support polled mode and will
ignore the <varname>polled</varname> argument.
    </para>
  </refsect1>

  <refsect1 id="spi-api-transfer"><title>Simple Transfers</title>
    <para>
<function>cyg_spi_transfer</function> can be used for SPI operations
to simple devices. It takes the following arguments:
    </para>
    <variablelist>
      <varlistentry>
        <term><type>cyg_spi_device*</type> <varname>device</varname></term>
        <listitem><para>
This identifies the SPI device that should be used.
        </para></listitem>
      </varlistentry>
      <varlistentry>
        <term><type>cyg_bool</type> <varname>polled</varname></term>
        <listitem><para>
Polled mode should be used during system initialization and in a
single-threaded application. Interrupt-driven mode should normally be
used in a multi-threaded application.
        </para></listitem>
      </varlistentry>
      <varlistentry>
        <term><type>cyg_uint32</type> <varname>count</varname></term>
        <listitem><para>
This identifies the number of data items to be transferred. Usually
each data item is a single byte, but some devices use a larger size up
to 16 bits.
        </para></listitem>
      </varlistentry>
      <varlistentry>
        <term><type>const cyg_uint8*</type> <varname>tx_data</varname></term>
        <listitem><para>
The data to be transferred to the device. If the device will only
output data and ignore its input then a null pointer can be used.
Otherwise the array should contain <varname>count</varname> data
items, usually bytes. For devices where each data item is larger than
one byte the argument will be interpreted as an array of shorts
instead, and should be aligned to a 2-byte boundary. The bottom n bits
of each short will be sent to the device. The buffer need not be
aligned to a cache-line boundary, even for SPI devices which use DMA
transfers, but some bus drivers may provide better performance if the
buffer is suitably aligned. The buffer will not be modified by the
transfer. 
        </para></listitem>
      </varlistentry>
      <varlistentry>
        <term><type>cyg_uint8*</type> <varname>rx_data</varname></term>
        <listitem><para>
A buffer for the data to be received from the device. If the device
does not generate any output then a null pointer can be used.
The same size and alignment rules apply as for <varname>tx_data</varname>.
        </para></listitem>
      </varlistentry>
    </variablelist>
    <para>
<function>cyg_spi_transfer</function> performs all the stages of an
SPI transfer: locking the bus; setting it up correctly for the
specified device; asserting the chip select and transferring the data;
dropping the chip select at the end of the transfer; returning the bus
to a quiescent state; and unlocking the bus.
    </para>
  </refsect1>

  <refsect1 id="spi-api-tick"><title>Additional Clock Ticks</title>
    <para>
Some devices require a number of clock ticks on the SPI bus between
transfers so that they can complete some internal processing. These
ticks must happen at the appropriate clock rate but no chip select
should be asserted and no data transfer will happen.
<function>cyg_spi_tick</function> provides this functionality.
The <varname>device</varname> argument identifies the SPI bus, the
required clock rate and the size of each data item. The
<varname>polled</varname> argument has the usual meaning. The
<varname>count</varname> argument specifies the number of data items
that would be transferred, which in conjunction with the size of each
data item determines the number of clock ticks.
    </para>
  </refsect1>

  <refsect1 id="spi-api-transaction"><title>Transactions</title>
    <para>
A transaction-oriented API is available for interacting with more
complicated devices. This provides separate functions for each of the
steps in an SPI transfer.
    </para>
    <para>
<function>cyg_spi_transaction_begin</function> must be used at the
start of a transaction. This performs thread-level locking on the bus,
blocking if it is currently in use by another thread. Then it prepares
the bus for transfers to the specified device, for example by making
sure it will tick at the right clock rate.
    </para>
    <para>
<function>cyg_spi_transaction_begin_nb</function> is a non-blocking
variant, useful for threads which cannot afford to block for an
indefinite period. If the bus is currently locked the function returns
false immediately. If the bus is not locked then it acts as
<filename>cyg_spi_transaction_begin</filename> and returns true.
    </para>
    <para>
Once the bus has been locked it is possible to perform one or more
data transfers by calling
<function>cyg_spi_transaction_transfer</function>. This takes the same
arguments as <function>cyg_spi_transfer</function>, plus an additional
one <varname>drop_cs</varname>. A non-zero value specifies that
the device's chip select should be dropped at the end of the transfer,
otherwise the chip select remains asserted. It is essential that the
chip select be dropped in the final transfer of a transaction. If the
protocol makes this difficult then
<function>cyg_spi_transaction_tick</function> can be used to generate
dummy ticks with all chip selects dropped.
    </para>
    <para>
If the device requires additional clock ticks in the middle of a
transaction without being selected,
<function>cyg_spi_transaction_tick</function> can be used. This will
drop the device's chip select if necessary, then generate the
appropriate number of ticks. The arguments are the same as for
<function>cyg_spi_tick</function>.
    </para>
    <para>
<function>cyg_spi_transaction_end</function> should be called at the
end of a transaction. It returns the SPI bus to a quiescent state,
then unlocks it so that other threads can perform I/O.
    </para>
    <para>
A typical transaction might involve the following. First a command
should be sent to the device, consisting of four bytes. The device
will then respond with a single status byte, zero for failure,
non-zero for success. If successful then the device can accept another
n bytes of data, and will generate a 2-byte response including a
checksum. The device's chip select should remain asserted throughout.
The code for this would look something like:
    </para>
    <programlisting>
#include &lt;cyg/io/spi.h&gt;
#include &lt;cyg/hal/hal_io.h&gt;    // Defines the SPI devices
&hellip;
    cyg_spi_transaction_begin(&amp;hal_spi_eprom);
    // Interrupt-driven transfer, four bytes of command
    cyg_spi_transaction_transfer(&amp;hal_spi_eprom, 0, 4, command, NULL, 0);
    // Read back the status
    cyg_spi_transaction_transfer(&amp;hal_spi_eprom, 0, 1, NULL, status, 0);
    if (!status[0]) {
        // Command failed, generate some extra ticks to drop the chip select
        cyg_spi_transaction_tick(&amp;hal_spi_eprom, 0, 1);
    } else {
        // Transfer the data, then read back the final status. The
        // chip select should be dropped at the end of this.
        cyg_spi_transaction_transfer(&amp;hal_spi_eprom, 0, n, data, NULL, 0);
        cyg_spi_transaction_transfer(&amp;hal_spi_eprom, 0, 2, NULL, status, 1);
        // Code for checking the final status should go here 
    }
    // Transaction complete so clean up
    cyg_spi_transaction_end(&amp;hal_spi_eprom);
    </programlisting>
    <para>
A number of variations are possible. For example the command and
status could be packed into the beginning and end of two 5-byte
arrays, allowing a single transfer.
    </para>
  </refsect1>

  <refsect1 id="spi-api-config"><title>Device Configuration</title>
    <para>
The functions <function>cyg_spi_get_config</function> and
<function>cyg_spi_set_config</function> can be used to examine and
change parameters associated with SPI transfers. The only keys that
are defined for all devices are
<varname>CYG_IO_GET_CONFIG_SPI_CLOCKRATE</varname> and
<varname>CYG_IO_SET_CONFIG_SPI_CLOCKRATE</varname>. Some types of
device, for example MMC cards, support a range of clock rates. The
<structname>cyg_spi_device</structname> structure will be initialized
with a low clock rate. During system initialization the device will be
queried for the optimal clock rate, and the
<structname>cyg_spi_device</structname> should then be updated. The
argument should be a clock rate in Hertz. For example the following
code switches communication to 1Mbit/s:
    </para>
    <programlisting>
    cyg_uint32    new_clock_rate = 1000000;
    cyg_uint32    len            = sizeof(cyg_uint32);
    if (cyg_spi_set_config(&amp;hal_mmc_device,
                           CYG_IO_SET_CONFIG_SPI_CLOCKRATE,
                           (const void *)&amp;new_clock_rate, &amp;len)) {
        // Error recovery code
    }
    </programlisting>
    <para>
If an SPI bus driver does not support the exact clock rate specified
it will normally use the nearest valid one. SPI bus drivers may define
additional keys appropriate for specific hardware. This means that the
valid keys are not known by the generic code, and theoretically it is
possible to use a key that is not valid for the SPI bus to which the
device is attached. It is also possible that the argument used with
one of these keys is invalid. Hence both
<function>cyg_spi_get_config</function> and
<function>cyg_spi_set_config</function> can return error codes. The
return value will be 0 for success, non-zero for failure. The SPI bus
driver's documentation should be consulted for further details.
    </para>
    <para>
Both configuration functions will lock the bus, in the same way as
<function>cyg_spi_transfer</function>. Changing the clock rate in the
middle of a transfer or manipulating other parameters would have
unexpected consequences.
    </para>
  </refsect1>

</refentry>

<refentry id="spi-porting">
  <refmeta>
    <refentrytitle>Porting to New Hardware</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname>Porting</refname>
    <refpurpose>Adding SPI support to new hardware</refpurpose>
  </refnamediv>

  <refsect1 id="spi-porting-description"><title>Description</title>
    <para>
Adding SPI support to an eCos port can take two forms. If there is
already an SPI bus driver for the target hardware then both that
driver and this generic SPI package <varname>CYGPKG_IO_SPI</varname>
should be included in the <database>ecos.db</database> target entry.
Typically the platform HAL will need to supply some platform-specific
information needed by the bus driver. In addition the platform HAL
should provide <structname>cyg_spi_device</structname> structures for
every device attached to the bus. The exact details of this depend on
the bus driver so its documentation should be consulted for further
details. If there is no suitable SPI bus driver yet then a new driver
package will have to be written.
    </para>
  </refsect1>

  <refsect1 id="spi-porting-devices"><title>Adding a Device</title>
    <para>
The generic SPI package <varname>CYGPKG_IO_SPI</varname> defines a
data structure <structname>cyg_spi_device</structname>. This contains
the information needed by the generic package, but not the additional
information needed by a bus driver to interact with the device. Each
bus driver will define a larger data structure, for example
<structname>cyg_mcf52xx_qspi_device</structname>, which contains a
<structname>cyg_spi_device</structname> as its first field. This is
analogous to C++ base and derived classes, but without any use of
virtual functions. The bus driver package should be consulted for the
details.
    </para>
    <para>
During initialization an SPI bus driver may need to know about all the
devices attached to that bus. For example it may need to know which
cpu pins should be configured as chip selects rather than GPIO pins.
To achieve this all device definitions should specify the particular
bus to which they are attached, for example:
    </para>
    <programlisting>
struct cyg_mcf52xx_qspi_device hal_spi_atod = {
    .spi_common.spi_bus = &amp;cyg_mcf52xx_qspi_bus,
    &hellip;
} CYG_SPI_DEVICE_ON_BUS(0);
    </programlisting>
    <para>
The <function>CYG_SPI_DEVICE_ON_BUS</function> macro adds information
to the structure which causes the linker to group all such structures
in a single table. The bus driver's initialization code can then
iterate over this table. 
    </para>
  </refsect1>

  <refsect1 id="spi-porting-bus"><title>Adding Bus Support</title>
    <para>
An SPI bus driver usually involves a new hardware package. This needs
to perform the following:
    </para>
    <orderedlist>
      <listitem><para>
Define a device structure which contains a
<structname>cyg_spi_device</structname> as its first element. This
should contain all the information needed by the bus driver to
interact with a device on that bus.
      </para></listitem>
      <listitem><para>
Provide functions for the following operations:
      </para>
      <simplelist type="vert" columns="1">
        <member><function>spi_transaction_begin</function></member>
        <member><function>spi_transaction_transfer</function></member>
        <member><function>spi_transaction_tick</function></member>
        <member><function>spi_transaction_end</function></member>
        <member><function>spi_get_config</function></member>
        <member><function>spi_set_config</function></member>
      </simplelist>
      <para>
These correspond to the main API functions, but can assume that the
bus is already locked so no other thread will be manipulating the bus
or any of the attached devices. Some of these operations may be no-ops.
      </para></listitem>
      <listitem><para>
Define a bus structure which contains a
<structname>cyg_spi_bus</structname> as its first element. This should
contain any additional information needed by the bus driver.
      </para></listitem>
      <listitem><para>
Optionally, instantiate the bus structure. The instance should have a
well-known name since it needs to be referenced by the device
structure initializers. For some drivers it may be best to create the
bus inside the driver package. For other drivers it may be better to
leave this to the platform HAL or the application. It depends on how
much platform-specific knowledge is needed to fill in the bus
structure.
      </para></listitem>
      <listitem><para>
Create a HAL table for the devices attached to this bus.
      </para></listitem>
      <listitem><para>
Arrange for the bus to be initialized early on during system
initialization. Typically this will happen via a prioritized static
constructor with priority <literal>CYG_INIT_BUS_SPI</literal>.
As part of this initialization the bus driver should
invoke the <function>CYG_SPI_BUS_COMMON_INIT</function> macro on its
<structname>cyg_spi_bus</structname> field.
      </para></listitem>
      <listitem><para>
Provide the appropriate documentation, including details of how the
SPI device structures should be initialized.
      </para></listitem>
    </orderedlist>
    <para>
There are no standard SPI testcases. It is not possible to write SPI
code without knowing about the devices attached to the bus, and those
are inherently hardware-specific.
    </para>
  </refsect1>

</refentry>
</part>
