// eCos memory layout - Tue Apr 02 09:21:22 2002

// This is a generated file - do not edit

#include <cyg/infra/cyg_type.inc>

MEMORY
{
    ram : ORIGIN = 0, LENGTH = 0x8000000
    rom : ORIGIN = 0x40000000, LENGTH = 0x100000
}

SECTIONS
{
    SECTIONS_BEGIN
    SECTION_fixed_vectors (ram, 0x20, LMA_EQ_VMA)
    CYG_LABEL_DEFN(__heap1) = 0x8000;
    SECTION_rom_vectors (ram, 0x7f80000, AT (0x40000000))
    SECTION_text (ram, ALIGN (0x4), FOLLOWING (.rom_vectors))
    SECTION_fini (ram, ALIGN (0x4), FOLLOWING (.text))
    SECTION_rodata (ram, ALIGN (0x4), FOLLOWING (.fini))
    SECTION_rodata1 (ram, ALIGN (0x4), FOLLOWING (.rodata))
    SECTION_fixup (ram, ALIGN (0x4), FOLLOWING (.rodata1))
    SECTION_gcc_except_table (ram, ALIGN (0x4), FOLLOWING (.fixup))
    SECTION_data (ram, ALIGN (0x1), FOLLOWING (.gcc_except_table))
    SECTION_bss (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTIONS_END
}
