cdl_savefile_version 1;
cdl_savefile_command cdl_savefile_version {};
cdl_savefile_command cdl_savefile_command {};
cdl_savefile_command cdl_configuration { description hardware template package };
cdl_savefile_command cdl_package { value_source user_value wizard_value inferred_value };
cdl_savefile_command cdl_component { value_source user_value wizard_value inferred_value };
cdl_savefile_command cdl_option { value_source user_value wizard_value inferred_value };
cdl_savefile_command cdl_interface { value_source user_value wizard_value inferred_value };

cdl_configuration eCos {
    description "" ;
    hardware    eb40a ;
    template    redboot ;
    package -hardware CYGPKG_HAL_ARM current ;
    package -hardware CYGPKG_HAL_ARM_AT91 current ;
    package -hardware CYGPKG_DEVS_FLASH_EB40A current ;
    package -template CYGPKG_HAL current ;
    package -template CYGPKG_INFRA current ;
    package -template CYGPKG_REDBOOT current ;
    package CYGPKG_IO_FLASH current ;
};

cdl_option CYGNUM_HAL_COMMON_INTERRUPTS_STACK_SIZE {
    user_value 6144
};

cdl_option CYGDBG_HAL_COMMON_INTERRUPTS_SAVE_MINIMUM_CONTEXT {
    user_value 0
};

cdl_option CYGDBG_HAL_COMMON_CONTEXT_SAVE_MINIMUM {
    inferred_value 0
};

cdl_option CYGDBG_HAL_DEBUG_GDB_INCLUDE_STUBS {
    inferred_value 1
};

cdl_option CYGSEM_HAL_USE_ROM_MONITOR {
    inferred_value 0 0
};

cdl_component CYGBLD_BUILD_REDBOOT {
    user_value 1
};

cdl_option CYGOPT_REDBOOT_FIS {
    user_value 0
};

cdl_component CYGSEM_REDBOOT_FLASH_CONFIG {
    user_value 0
};

cdl_option CYGBLD_BUILD_REDBOOT_WITH_EXEC {
    user_value 0
};

