// eCos memory layout - Fri Oct 20 09:51:30 2000

// This is a generated file - do not edit

#include <cyg/infra/cyg_type.inc>

MEMORY
{
    ram : ORIGIN = 0x88000200, LENGTH = 0xffe00
    rom : ORIGIN = 0x80000000, LENGTH = 0x20000
}

SECTIONS
{
    SECTIONS_BEGIN
    SECTION_vectors (ram, 0x88000200, AT (0x80000000))
    SECTION_text (ram, ALIGN (0x10), FOLLOWING (.vectors))
    SECTION_fini (ram, ALIGN (0x10), FOLLOWING (.text))
    SECTION_rodata1 (ram, ALIGN (0x10), FOLLOWING (.fini))
    SECTION_rodata (ram, ALIGN (0x10), FOLLOWING (.rodata1))
    SECTION_fixup (ram, ALIGN (0x10), FOLLOWING (.rodata))
    SECTION_gcc_except_table (ram, ALIGN (0x10), FOLLOWING (.fixup))
    SECTION_data (ram, ALIGN (0x10), FOLLOWING (.gcc_except_table))
    SECTION_bss (ram, ALIGN (0x10), LMA_EQ_VMA)
    CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
    SECTIONS_END
}
