// eCos memory layout - Tue Jan 23 18:50:05 2001

// This is a generated file - do not edit

#include <cyg/infra/cyg_type.inc>

MEMORY
{
    rom : ORIGIN = 0x100000, LENGTH = 0x80000
    ram : ORIGIN = 0xfc0000, LENGTH = 0x3c000
}

SECTIONS
{
    SECTIONS_BEGIN
    SECTION_rom_vectors (ram, 0xfc0000, AT (0x100000))
    SECTION_ram_vectors (ram, ALIGN (0x4), FOLLOWING (.rom_vectors))
    SECTION_text (ram, ALIGN (0x4), FOLLOWING (.ram_vectors))
    SECTION_fini (ram, ALIGN (0x4), FOLLOWING (.text))
    SECTION_rodata (ram, ALIGN (0x4), FOLLOWING (.fini))
    SECTION_rodata1 (ram, ALIGN (0x4), FOLLOWING (.rodata))
    SECTION_fixup (ram, ALIGN (0x4), FOLLOWING (.rodata1))
    SECTION_gcc_except_table (ram, ALIGN (0x4), FOLLOWING (.fixup))
    SECTION_data (ram, ALIGN (0x4), FOLLOWING (.gcc_except_table))
    SECTION_bss (ram, ALIGN (0x4), LMA_EQ_VMA)
    CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
    SECTIONS_END
}
