// eCos memory layout - Fri Jan 26 09:07:19 2001

// This is a generated file - do not edit

#include <cyg/infra/cyg_type.inc>

MEMORY
{
    ram : ORIGIN = 0xfc0000, LENGTH = 0x3c000
}

SECTIONS
{
    SECTIONS_BEGIN
    CYG_LABEL_DEFN(__reserved) = 0xfc0000; . = CYG_LABEL_DEFN(__reserved) + 0x4000;
    SECTION_text (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_ram_vectors (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_fini (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_rodata (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_rodata1 (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_fixup (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_gcc_except_table (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_data (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_bss (ram, ALIGN (0x4), LMA_EQ_VMA)
    CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
    SECTIONS_END
}
