// eCos memory layout - Fri Oct 20 10:35:23 2000

// This is a generated file - do not edit

#include <cyg/infra/cyg_type.inc>

MEMORY
{
    ram : ORIGIN = 0, LENGTH = 0x400000
}

SECTIONS
{
    SECTIONS_BEGIN
    CYG_LABEL_DEFN(__reserved_vectors) = 0; . = CYG_LABEL_DEFN(__reserved_vectors) + 0x3000;
    CYG_LABEL_DEFN(__reserved_vsr_table) = ALIGN (0x10); . = CYG_LABEL_DEFN(__reserved_vsr_table) + 0x200;
    CYG_LABEL_DEFN(__reserved_virtual_table) = ALIGN (0x10); . = CYG_LABEL_DEFN(__reserved_virtual_table) + 0x100;
    CYG_LABEL_DEFN(__reserved_for_rom) = ALIGN (0x10); . = CYG_LABEL_DEFN(__reserved_for_rom) + 0x1cd00;
    SECTION_vectors (ram, ALIGN (0x10), LMA_EQ_VMA)
    SECTION_text (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_fini (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_rodata1 (ram, ALIGN (0x8), LMA_EQ_VMA)
    SECTION_rodata (ram, ALIGN (0x8), LMA_EQ_VMA)
    SECTION_fixup (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_gcc_except_table (ram, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_data (ram, ALIGN (0x8), LMA_EQ_VMA)
    SECTION_sbss (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_bss (ram, ALIGN (0x10), LMA_EQ_VMA)
    CYG_LABEL_DEFN(__heap1) = ALIGN (0x8);
    SECTIONS_END
}
