version 0
region ram 0 1000000 0 !
region rom 41000000 400000 1 !
section fixed_vectors 0 1 0 1 1 0 1 0 20 20 !
section data 0 1 1 1 1 1 0 0 8000 bss !
section bss 0 4 0 1 0 1 0 1 heap1 heap1 !
section heap1 0 8 0 0 0 0 0 0 !
section pci_window 100000 1 0 0 1 0 1 0 f00000 f00000 !This is the memory area that is dual-ported to devices onthe PCI bus.  Such devices can read and write this memory areaas their own.  Examples include the EBSA-285 Ethernet driver, which receives and transmits packets via this memory area.  It must be 1Mb aligned, so that the MMU initialization can arrange for it to be uncacheable.
section rom_vectors 0 1 0 1 1 1 1 1 41000000 41000000 text text !
section text 0 4 0 1 0 1 0 1 fini fini !
section fini 0 4 0 1 0 1 0 1 rodata rodata !
section rodata 0 4 0 1 0 1 0 1 rodata1 rodata1 !
section rodata1 0 4 0 1 0 1 0 1 fixup fixup !
section fixup 0 4 0 1 0 1 0 1 gcc_except_table gcc_except_table !
section gcc_except_table 0 4 0 1 0 0 0 1 data !
