===========================================================================
#####ECOSGPLCOPYRIGHTBEGIN####
# -------------------------------------------
# This file is part of eCos, the Embedded Configurable Operating System.
# Copyright (C) 1998, 1999, 2000, 2001, 2002 Red Hat, Inc.
#
# eCos is free software; you can redistribute it and/or modify it under
# the terms of the GNU General Public License as published by the Free
# Software Foundation; either version 2 or (at your option) any later version.
#
# eCos is distributed in the hope that it will be useful, but WITHOUT ANY
# WARRANTY; without even the implied warranty of MERCHANTABILITY or
# FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
# for more details.
#
# You should have received a copy of the GNU General Public License along
# with eCos; if not, write to the Free Software Foundation, Inc.,
# 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA.
#
# As a special exception, if other files instantiate templates or use macros
# or inline functions from this file, or you compile this file and link it
# with other works to produce a work based on this file, this file does not
# by itself cause the resulting work to be covered by the GNU General Public
# License. However the source code for this file must still be made available
# in accordance with section (3) of the GNU General Public License.
#
# This exception does not invalidate any other reasons why a work based on
# this file might be covered by the GNU General Public License.
#
# Alternative licenses for eCos may be arranged by contacting Red Hat, Inc.
# at http://sources.redhat.com/ecos/ecos-license
# -------------------------------------------
#####ECOSGPLCOPYRIGHTEND####
===========================================================================

1999-01-05, revised 1999-03-11, revised 2000.01.26

How to build and install the GDB module on the AEB-1
====================================================

Overview
--------

The ARM AEB-1 comes with tools in ROM.  These include a simple FLASH
management tool and the Angel (R) monitor.  eCos for the ARM AEB-1
comes with GDB stubs suitable for programming into the onboard FLASH.
GDB is the preferred debug environment for eCos, but Angel must be
used to initially install the GDB stubs.

Once this bootstrapping is done, you can use GDB to load and debug
programs on the AEB-1 board.

The following steps will have you:

* talk to the AEB-1 board with a terminal emulator (or a real
  terminal!)

* enable ARM's Angel ROM monitor

* use GDB with Angel or the Angel ROM monitor to download a
  configuration of eCos with GDB stubs which will act as a ROM monitor

* talk to the AEB-1 with a terminal emulator again, and tell it to
  write the new module to flash

* tell the board to use this new monitor, and then hook GDB up to it
  for real debugging

Talking to the board
--------------------

Connect a terminal or computer's serial port to the ARM AEB-1.  On a
PC with a 9-pin serial port, you can use the cable shipped by ARM with
no modification.

Set the terminal or terminal emulator to 9600N1 (9600 baud, no parity,
1 stop bit).

Reset the board by pressing the little reset button on the top.  You
will see the following text:

	ARM Evaluation Board Boot Monitor 0.01 (19 APR 1998)
	Press ENTER within 2 seconds to stop autoboot

Press ENTER quickly, and you will get the boot prompt:

	Boot:


Downloading the GDB stubs
-------------------------

Run the angel monitor by typing the following at the Boot: prompt:

    Boot: plugin angel
    Boot: angel

Then exit the terminal emulator and start up gdb with the GDB module:

    $ arm-elf-gdb -nw loaders/arm-aeb/gdb_module.img
    (gdb) set remotebaud 9600
    (gdb) target rdi s=<YOUR SERIAL PORT>

On Windows, the serial port could be com1, com2, etc.  On a UNIX or
Linux system, the serial port would be /dev/cua0 or /dev/cua1.
Examples are:

    (gdb) target rdi s=com1
    (gdb) target rdi s=/dev/cua0

Finally, load the GDB stubs image:

    (gdb) load
    Loading section .rom_vectors, size 0x44 lma 0xc000
    Loading section .text, size 0x3544 lma 0xc044
    Loading section .rodata, size 0x164 lma 0xf588
    Loading section .data, size 0x110 lma 0xf6ec
    Start address 0xc044 , load size 14332
    Transfer rate: 12739 bits/sec.

(Note that the sizes may not exactly match the ones you see on your
system.)

Once the loading is done, quit GDB:

    (gdb) quit


Activating the GDB stubs
------------------------

Connect a terminal emulator to the board again, reset the board, and
type enter within two seconds to get the Boot: prompt.  This is the
same thing you did at the beginning of this procedure.

Commit the GDB stubs module to flash:

	Boot: flashwrite 4018000 C000 8000

Verify that the eCos/"GDB stubs" module is now added in the list of
modules in the board:

	Boot: rommodules

You should see the following output:

	Header   Base     Limit
	04000004 04000000 040034a8 BootStrap       1.00 (14 Aug 1998) 
	04003a74 04003800 04003bc0 Production Test 1.00 (13 Aug 1998) 
	0400e4f4 04004000 0400e60f Angel           1.02 (12 MAY 1998) 
	0401ac00 04018000 0401aed8 eCos            1.2  (26 Feb 1999) GDB stubs

Now make the eCos/"GDB stubs" module be the default monitor:

	Boot: plugin eCos


Running and debugging an application
------------------------------------

Configure eCos from scratch for the ARM AEB-1 platform, and build your
application.  Remember that the AEB-1 board only has 128K of RAM.

Exit from the terminal emulator (you will not need it anymore for
normal operations), and run gdb:

    $ arm-elf-gdb -nw executable
    (gdb) set remotebaud 38400
    (gdb) target remote <YOUR SERIAL PORT>
    (gdb) load

You can now run your program in the usual way under GDB'S control

Notice that the GDB stub runs at 38400 baud.


Building the GDB stubs
----------------------

We provide the GDB stubs image in the directory
loaders/arm-aeb/gdb_module.img, but here are instructions on how to
rebuild them if you should ever need to.

 % ecosconfig new aeb stubs
 % ecosconfig tree
 % make

The newlt built files are installed in ./bin/install.


Alternate way of loading the initial stubs
------------------------------------------

Using the AEB-1 module tool, install the GDB stubs from the provided
".UU" file.

>>> This is an annotated 'terminal' session with the AEB-1 monitor:

ARM Evaluation Board Boot Monitor 0.01 (19 APR 1998)
Press ENTER within 2 seconds to stop autoboot
Boot: help
Module is BootStrap       1.00 (14 Aug 1998)

Help is available on:
  Help          Modules       ROMModules    UnPlug        PlugIn
  Kill          SetEnv        UnSetEnv      PrintEnv      DownLoad
  Go            GoS           Boot          PC            FlashWrite
  FlashLoad     FlashErase

Boot: download c000
Ready to download. Use 'transmit' option on terminal emulator to download file.

 ... at this point, I told my terminal emulator (minicom) to download
     the ASCII file gdb_module.img.UU (probably needs a different name
     on Win/NT) I had to enter ^D when the download was complete to
     get the monitor to come back.

Loaded file gdb_module.img.raw at address 0000c000, size = 13905

Boot: flashwrite 4018000 c000 8000

  As above, this command actually programs the FLASH.

Boot: rommodules
Header   Base     Limit
04000004 04000000 040034a8 BootStrap       1.00 (14 Aug 1998)
04003a74 04003800 04003bc0 Production Test 1.00 (13 Aug 1998)
0400e4f4 04004000 0400e60f Angel           1.02 (12 MAY 1998)
0401b608 04018000 0401b844 eCos            1.3  (Jan 26 2000) GDB stubs

  This verifies that the eCos GDB stubs are available in FLASH.

Boot: plugin ecos

  This makes the eCos GDB stubs the default "monitor."  When reset the
  AEB-1 will start the GDB stubs, after the initial 2 second escape
  period.
