    NAME
         bridge - Ethernet bridge interface

    SYNOPSIS
         pseudo-device bridge 2

    DESCRIPTION
         The bridge device creates a logical link between two or more Ethernet in
         terfaces.  This link between the interfaces selectively forwards frames
         from each interface on the bridge to every other interface on the bridge.
         A bridge can serve several services, including, isolation of traffic be
         tween sets of machines so that traffic local to one set of machines is
         not available on the wire of another set of machines, and it can act as a
         transparent filter for ip(4) datagrams.

         The bridges provided by this interface are learning bridges with IP fil
         tering, see ipf(4).  In general a bridge works like a hub, forwarding
         traffic from one interface to another.  It differs from a hub in that it
         will "learn" which machines are on each of its attached segments by ac
         tively listening to incoming traffic and examining the headers of each
         frame.  A table is built containing the MAC address and segment to which
         the MAC address is attached.  This allows a bridge to be more selective
         about what it forwards, which can be used to reduce traffic on a set of
         segments and also to provide an IP firewall without changing the topology
         of the network.

         The algorithm works as follows by default, but can be modified via
         ioctl(2) or the utility brconfig(8).  When a frame comes in, the origin
         segment and the source address are recorded.  If the bridge has no knowl
         edge about where the destination is to be found, the bridge will forward
         the frame to all attached segments.  If the destination is known to be on
         a different segment from its origin, the bridge will forward the packet
         only to the destination segment.  If the destination is on the same seg
         ment as the origin segment, the bridge will drop the packet because the
         receiver has already had a chance to see the frame.  Before forwarding a
         frame, the bridge will check to see if the packet contains an ip(4) data
         gram; if so, the datagram is run through the ipf(4) interface so that it
         can be filtered.  Only the ipf(4) input rules for the source interface
         are checked with the datagram; output rules have no effect.

    IOCTLS
         A bridge interface responds to all of the ioctl(2) calls specific to oth
         er interfaces listed in netintro(4).  The following ioctl(2) calls are
         specific to bridge devices.  They are defined in .

         SIOCBRDGIFS      (struct ifbifconf) Retrieve member interface list from a
                          bridge.  This request takes an ifbifconf structure (see
                          below) as a value-result parameter.  The ifbic_len field
                          should be initially set to the size of the buffer point
                          ed to by ifbic_buf. On return it will contain the
                          length, in bytes, of the configuration list.  Alterna
                          tively, if the ifbic_len passed in is set to 0,
                          SIOCBRDGIFS will set ifbic_len to the size that
                          ifbic_buf needs to be to fit the entire configuration
                          list, and will not fill in the other parameters.  This
                          is useful for determining the exact size that ifbic_buf
                          needs to be in advance.

                          The argument structure is defined as follows:

                                struct ifbreq {
                                        char ifbr_name[IFNAMSIZ];    /* brdg nam */
                                        char ifbr_ifsname[IFNAMSIZ]; /* if name */
                                        u_int32_t ifbr_ifsflags;     /* if flags */
                                };

                                #define IFBIF_LEARNING  0x1 /* learns addrs */
                                #define IFBIF_DISCOVER  0x2 /* gets fwd'd pkts */

                                struct ifbifconf {
                                        char ifbic_name[IFNAMSIZ]; /* brdg name */
                                        u_int32_t       ifbic_len; /* buf size */
                                        union {
                                                caddr_t ifbicu_buf; /* buffer */
                                                struct  ifbreq *ifbicu_req;
                                        } ifbic_ifbicu;
                                #define ifbic_buf       ifbic_ifbicu.ifbicu_buf
                                #define ifbic_req       ifbic_ifbicu.ifbicu_req
                                };

         SIOCBRDGADD      (struct ifbreq) Add the interface named in ifbr_ifsname
                          to the bridge named in ifbr_name.

         SIOCBRDGDEL      (struct ifbreq) Delete the interface named in
                          ifbr_ifsname from the bridge named in ifbr_name.

         SIOCBRDGSIFFLGS  (struct ifbreq) Set the bridge member interface flags
                          for the interface named in ifbr_ifsname attached to the
                          bridge ifbr_name. If the flag IFBIF_LEARNING is set on
                          an interface, source addresses from frames received on
                          the interface are recorded in the address cache.  If the
                          flag IFBIF_DISCOVER is set, the interface will receive
                          packets destined for unknown destinations, otherwise a
                          frame that has a destination not found in the address
                          cache is not forwarded to this interface.  The default
                          for newly added interfaces has both flags set.  If the
                          flag IFBIF_BLOCKNONIP is set, packets that are one of
                          ip(4),  ip6(4),  arp(4),  or Reverse ARP, will not be
                          bridged from and to the interface.

         SIOCBRDGGIFFLGS  Retrieve the bridge member interface flags for the in
                          terface named in ifbr_ifsname attached to the bridge
                          ifbr_name.

         SIOCBRDGRTS      (struct ifbaconf) Retrieve the address cache of the
                          bridge named in ifbac_name. This request takes an
                          ifbaconf structure (see below) as a value result parame
                          ter.  The ifbac_len field should be initially set to the
                          size of the buffer pointed to by ifbac_buf. On return,
                          it will contain the length, in bytes, of the configura
                          tion list.  Alternatively, if the ifbac_len passed in is
                          set to 0, SIOCBRDGRTS will set it to the size that
                          ifbac_buf needs to be to fit the entire configuration
                          list and not fill in the other parameters.  As with
                          SIOCBRDGIFS, this is useful for determining the exact
                          size that ifbac_buf needs to be in advance.

                          The argument structure is defined as follows:

                                struct ifbareq {
                                        char ifba_name[IFNAMSIZ];   /* brdg nam */
                                        char ifba_ifsname[IFNAMSIZ];/* dest ifs */
                                        u_int8_t ifba_age;          /* addr age */
                                        u_int8_t ifba_flags;        /* addr flag */
                                        struct ether_addr ifba_dst; /* dst addr */
                                };

                                #define IFBAF_TYPEMASK 0x03  /* addr type mask */
                                #define IFBAF_DYNAMIC  0x00  /* dynamic addr */
                                #define IFBAF_STATIC   0x01  /* static address */

                                struct ifbaconf {
                                        char ifbac_name[IFNAMSIZ]; /* brdg name */
                                        u_int32_t ifbac_len;       /* buf size */
                                        union {
                                                caddr_t ifbacu_buf;     /* buf */
                                                struct ifbareq *ifbacu_req;
                                        } ifbac_ifbacu;
                                #define ifbac_buf       ifbac_ifbacu.ifbacu_buf
                                #define ifbac_req       ifbac_ifbacu.ifbacu_req
                                };
                          Address cache entries with the type set to IFBAF_DYNAMIC
                          in ifba_flags are entries learned by the bridge.  En
                          tries with the type set to IFBAF_STATIC are manually
                          added entries.

         SIOCBRDGSADDR    (struct ifbareq) Add an entry, manually, to the address
                          cache for the bridge named in ifba_name. The address and
                          its associated interface and flags are set in the
                          ifba_dst, ifba_ifsname, ifba_flags fields, respectively.

         SIOCBRDGDADDR    (struct ifbareq) Delete an entry from the address cache
                          of the bridge named in ifba_name. Entries are deleted
                          strictly based on the address field ifba_dst.

         SIOCBRDGSCACHE   (struct ifbcachereq) Set the maximum address cache size
                          for the bridge named in ifbc_name to ifbc_size entries.

                          The argument structure is as follows:

                                struct ifbcachereq {
                                        char ifbc_name[IFNAMSIZ]; /* bridge */
                                        u_int32_t ifbc_size;      /* size */
                                };

         SIOCBRDGGCACHE   (struct ifbcachereq) Retrieve the maximum size of the
                          address cache for the bridge ifbc_name.

         SIOCBRDGSTO      (struct ifbcachetoreq) Set the time, in seconds, that
                          addresses which have not been seen on the network
                          (transmitted a packet) remain in the cache.  If the time
                          is set to zero, no aging is performed on the address
                          cache.  The argument structure is as follows:

                                struct ifbcachetoreq {
                                        char ifbct_name[IFNAMSIZ]; /* bridge */
                                        u_int32_t ifbct_time;      /* time */
                                };

         SIOCBRDGGTO      (struct ifbcachetoreq) Retrieve the address cache expi
                          ration time (see above).

         SIOCBRDGFLUSH    (struct ifbreq) Flush addresses from the cache.
                          ifbr_name contains the name of the bridge device, and
                          ifbr_ifsflags should be set to IFBF_FLUSHALL to flush
                          all addresses from the cache or IFBF_FLUSHDYN to flush
                          only the dynamically learned addresses from the cache.

         SIOCBRDGARL      (struct ifbrlreq) Add a filtering rule to the bridge
                          named in ifbr_name on the interface named in
                          ifbr_ifsname. The argument structure is as follows:

                                struct ifbrlreq {
                                        char ifbr_name[IFNAMSIZ];    /* bridge */
                                        char ifbr_ifsname[IFNAMSIZ]; /* ifs */
                                        u_int8_t ifbr_action;        /* handling */
                                        u_int8_t ifbr_flags;         /* flags */
                                        struct ether_addr ifbr_src;  /* src mac */
                                        struct ether_addr ifbr_dst;  /* dst mac */
                                };
                                #define BRL_ACTION_BLOCK        0x01
                                #define BRL_ACTION_PASS         0x02
                                #define BRL_FLAG_IN             0x08
                                #define BRL_FLAG_OUT            0x04
                                #define BRL_FLAG_SRCVALID       0x02
                                #define BRL_FLAG_DSTVALID       0x01

                          Rules are applied in the order in which they were added
                          to the bridge, and the first matching rule's action pa
                          rameter determines the fate of the packet.  The
                          ifbr_action parameter specifies whether a frame matching
                          the rule is to be blocked or passed.

                          If the BRL_FLAG_IN bit is set in ifbr_flags, then the
                          rule applies to frames received by the interface.  If
                          the BRL_FLAG_OUT bit is set, then the rule applies to
                          frame transmitted by the interface.  At least one of
                          BRL_FLAG_IN or BRL_FLAG_OUT must be set.

                          The source ethernet address in ifbr_src is checked if
                          the BRL_FLAG_SRCVALID bit is set in ifbr_flags. The des
                          tination address in ifbr_dst is check if the
                          BRL_FLAG_DSTVALID bit is set.  If neither bit is set,
                          the rule is matches all frames.

         SIOCBRDGFRL      (struct ifbrlreq) Remove all filtering rules from a
                          bridge interface member.  ifbr_name contains the name of
                          the bridge device, and ifbr_ifsname contains the name of
                          the bridge member interface.

         SIOCBRDGGRL      (struct ifbrlconf) Retrieve all of the rules from the
                          bridge, ifbrl_name, for the member interface,
                          ifbrl_ifsname.

                          This request takes an ifbrlconf structure (see below) as
                          a value result parameter.  The ifbrl_len field should be
                          initially set to the size of the buffer pointed to by
                          ifbrl_buf. On return, it will contain the length, in
                          bytes, of the configuration list.  Alternatively, if the
                          ifbrl_len passed in is set to 0, SIOCBRDGGRL will set it
                          to the size that ifbrl_buf needs to be to fit the entire
                          configuration list and not fill in the other parameters.
                          As with SIOCBRDGIFS, this is useful for determining the
                          exact size that ifbrl_buf needs to be in advance.

                          The argument structure is defined as follows:

                                struct ifbrlconf {
                                        char ifbrl_name[IFNAMSIZ];   /* brdg nam */
                                        char ifbrl_ifsname[IFNAMSIZ];/* ifs name */
                                        u_int32_t ifbr_len;         /* buf len */
                                        union {
                                                caddr_t ifbrlu_buf;
                                                struct ifbrlreq *ifbrlu_req;
                                        } ifrl_ifbrlu;
                                #define ifbrl_buf ifbrl_ifbrlu.ifbrlu_buf
                                #define ifbrl_req ifbrl_ifbrlu.ifbrlu_req
                                };

    ERRORS
         If the ioctl(2) call fails, errno(2) is set to one of the following val
         ues:

         [ENOENT]      For an add request, this means that the named interface is
                       not configured into the system.  For delete operation, it
                       means that the named interface is not a member of the
                       bridge.  For a address cache deletion, the address was not
                       found in the table.

         [ENOMEM]      Memory could not be allocated for an interface or cache en
                       try to be added to the bridge.

         [EEXIST]      The named interface is already a member of the bridge.

         [EBUSY]       The named interface is already a member of another bridge.

         [EINVAL]      The named interface is not an Ethernet interface or an in
                       valid ioctl was performed on the bridge.

         [ENETDOWN]    Address cache operation (flush, add, delete) on a bridge
                       that is in the down state.

         [EPERM]       Super-user privilege is required to add and delete inter
                       faces to and from bridges and to set the bridge interface
                       flags.

         [EFAULT]      The buffer used in a SIOCBRDGIFS or SIOCBRDGRTS request

                       points outside of the process's allocated address space.

         [ESRCH]       No such member interface in the bridge.

    SEE ALSO
         errno(2),  ioctl(2),  ip(4),  ipf(4),  netintro(4),  bridgename.if(5),
         brconfig(8)

    HISTORY
         The brconfig(8) command and the bridge(4) kernel interface first appeared
         in

    AUTHOR
         The brconfig(8) command and the bridge(4) kernel interface were written
         by Jason L. Wright  as part of an undergraduate inde
         pendent study at the University of North Carolina at Greensboro.

    BUGS
         There is currently no loop detection.  Care must be taken to make sure
         that loops are not created when a bridge is brought up.

         Only ipf(4) input rules are checked with incoming packet; there is no
         easy way to handle output rules.