    NAME
           socket - create an endpoint for communication

    SYNOPSIS
           #include <network.h>

           int socket(int domain, int type, int protocol);

    DESCRIPTION
           Socket creates an endpoint for communication and returns a
           descriptor.

           The domain parameter  specifies  a  communications  domain
           within  which  communication will take place; this selects
           the protocol family which should be used.  These  families
           are  defined  in <network.h>.  The currently understood
           formats include:

           PF_INET
                  IPv4 Internet protocols; see ip(4)

           The socket has the indicated  type,  which  specifies  the
           semantics of communication.  Currently defined types are:

           SOCK_STREAM
                  Provides  sequenced,  reliable, two-way connection-
                  based byte streams.  An out-of-band data  transmis-
                  sion mechanism may be supported.

           SOCK_DGRAM
                  Supports datagrams (connectionless, unreliable mes-
                  sages of a fixed maximum length).

           SOCK_SEQPACKET
                  Provides a sequenced, reliable, two-way connection-
                  based data transmission path for datagrams of fixed
                  maximum length; a consumer is required to  read  an
                  entire packet with each read system call.

           SOCK_RAW
                  Provides raw network protocol access.

           The  protocol  specifies  a particular protocol to be used
           with the socket.  Normally only a single  protocol  exists
           to  support a particular socket type within a given proto-
           col family.  However, it is possible that  many  protocols
           may  exist,  in  which  case a particular protocol must be
           specified in this manner.  The protocol number to  use  is
           particular to the "communication domain" in which communi-
           cation is to take place; see  protocols(5).   See  getpro-
           toent(3)  on  how to map protocol name strings to protocol
           numbers.

           Sockets of type SOCK_STREAM are full-duplex byte  streams,
           similar  to pipes.  A stream socket must be in a connected
           state before any data may be sent or received  on  it.   A
           connection  to another socket is created with a connect(2)
           call.  Once  connected,  data  may  be  transferred  using
           read(2)  and write(2) calls or some variant of the send(2)
           and recv(2) calls.  When a session has  been  completed  a
           close(2)  may  be performed.  Out-of-band data may also be
           transmitted  as  described  in  send(2)  and  received  as
           described in recv(2).

           The communications protocols which implement a SOCK_STREAM
           ensure that data is not lost or duplicated.  If a piece of
           data  for  which the peer protocol has buffer space cannot
           be successfully transmitted within a reasonable length  of
           time,  then the connection is considered When SO_KEEPALIVE
           is enabled on the socket the protocol checks in  a  proto-
           col-specific  manner  if  the other end is still alive.

           SOCK_DGRAM and SOCK_RAW sockets allow sending of datagrams
           to correspondents named in send(2) calls.   Datagrams  are
           generally  received  with  recvfrom(2),  which returns the
           next datagram with its return address.

           When  the network signals an error condition to the proto-
           col module (e.g.  using a ICMP message for IP) the pending
           error  flag  is set for the socket.  The next operation on
           this socket will return the  error  code  of  the  pending
           error.  For some protocols it is possible to enable a per-
           socket error queue to retrieve detailed information  about
           the error; see IP_RECVERR in ip(4).

           The  operation  of  sockets  is controlled by socket level
           options.  These options  are  defined  in  .
           Setsockopt(2)  and  getsockopt(2)  are used to set and get
           options, respectively.

    RETURN VALUES
           -1 is returned if an error occurs;  otherwise  the  return
           value is a descriptor referencing the socket.

    ERRORS
           EPROTONOSUPPORT
                   The protocol type or the specified protocol is not
                   supported within this domain.

           EMFILE  There are too many open files.

           EACCES  Permission  to  create  a  socket of the specified
                   type and/or protocol is denied.

           ENOBUFS or ENOMEM
                   Insufficient memory is available.  The socket can-
                   not  be  created  until  sufficient  resources are
                   freed.

           EINVAL  Unknown protocol, or protocol  family  not  avail-
                   able.