<!-- DOCTYPE part  PUBLIC "-//OASIS//DTD DocBook V3.1//EN" -->

<!-- {{{ Banner                                                     -->

<!-- =============================================================== -->
<!--                                                                 -->
<!--     twr_k60f120m.sgml                                        -->
<!--                                                                 -->
<!--     TWR-K60F120M board documentation.                        -->
<!--                                                                 -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTBEGIN####                                   -->
<!-- =============================================================== -->
<!-- Copyright (C) 2012 Free Software Foundation, Inc. -->
<!-- This material may be distributed only subject to the terms      -->
<!-- and conditions set forth in the Open Publication License, v1.0  -->
<!-- or later (the latest version is presently available at          -->
<!-- http://www.opencontent.org/openpub/)                            -->
<!-- Distribution of the work or derivative of the work in any       -->
<!-- standard (paper) book form is prohibited unless prior           -->
<!-- permission obtained from the copyright holder                   -->
<!-- =============================================================== -->
<!-- ####ECOSDOCCOPYRIGHTEND####                                     -->
<!-- =============================================================== -->
<!-- #####DESCRIPTIONBEGIN####                                       -->
<!--                                                                 -->
<!-- Author(s):   Ilija Kocho                                        -->
<!-- Contrib(s):  Mike Jones                                         -->
<!-- Contact(s):  mjones@proclivis.com                               -->
<!-- Date:        2013/06/02                                         -->
<!-- Version:     0.01                                               -->
<!--                                                                 -->
<!-- ####DESCRIPTIONEND####                                          -->
<!-- =============================================================== -->

<!-- }}} -->

<!--<part id="hal-cortexm-kinetis"><title>Freescale Kinetis Family Support</title>-->

<refentry id="kinetis-twr-k60f120m">
  <refmeta>
    <refentrytitle>TWR-K60F120M Development kit</refentrytitle>
  </refmeta>
  <refnamediv>
    <refname>CYGPKG_HAL_CORTEXM_KINETIS_TWR_K60F120M</refname>
    <refpurpose>eCos Support for Freescale TWR-K60F120M development kit</refpurpose>
  </refnamediv>
  
  <refsect1 id="kinetis-twr-k60f120m-description"><title>Description</title>
    <para>
    The Freescale TWR-K60F120M is a development kit for <link linkend="hal-cortexm-kinetis-var">
    Freescale Kinetis</link> Cortex-M4 based micro-controllers. It covers the K60
    microcontroller subfamily. K60FN1M0 is a high end member comprising on-chip 1 MiB FLASH
    and 128 KiB SRAM memory as well as a 16 KiB unified cache.
    K60 parts are equipped with a rich set of communication interfaces including Ethernet USB, UARTs
    CAN, SPI and I2C. They also have a Graphics controller and a DMA controller, as well as FlexBus and SDRAM
    external memory interfaces. They are mixed signal devices featuring a 16 bit ADC and a 12 bit DAC. 
    </para>
  </refsect1>
  <refsect1 id="kinetis-twr-k60f120m-config"><title>Configuration</title>
    <refsect2 id="kinetis-twr-k60f120m-config-hardware"><title>Hardware Setup</title>
      <refsect3 id="kinetis-twr-k60f120m-config-hardware-cpu"><title>TWR-K60F120M setup</title>
      <para>
      Factory jumper settings on TWR-K60F120M are fitted for standalone operation of the board.
      In order to use it with the Ethernet PHY from TWR-SER, some jumpers have to be changed
      on both TWR-K60F120M and TWR-SER. Jumper settings for TWR-SER are given in
      <link linkend="kinetis-twr-k60n512-config">TWR-K60N512 Configuration</link> and here are the TWR-K60F120M
      settings.
      </para>
      <table frame="all"><title>TWR-K60F120M Jumper setting</title>
        <tgroup cols="3" align="center">
          <colspec colnum="1" colname="jumper" colwidth="1*" >
          <colspec colnum="2" colname="jumpset" colwidth="1*" >
          <colspec colnum="3" colname="desc" colwidth="3*" >
          <thead>
            <row>
              <entry>Jumper</entry>
              <entry>Setting</entry>
              <entry>Description</entry>
            </row>
          </thead>
          <tbody>
            <row>
              <entry>J18</entry>
              <entry>ON</entry>
              <entry>On board 50MHz oscillator is disabled</entry>
            </row>
            <row>
              <entry>J19</entry>
              <entry>ON</entry>
              <entry>On board 50MHz oscillator is powered</entry>
            </row>
          </tbody>
        </tgroup>
      </table>
      </refsect3>
    </refsect2>
    <refsect2 id="kinetis-twr-k60f120m-config-ecos"><title>eCos Configuration</title>
      <refsect3 id="twr-k60f120m-clocking"><title>Clocking</title>
      <para>
      The TWR-K60F120M package defines requirements for the platform clocking.
      </para>
      </refsect3>  
      <refsect3 id="twr-k60f120m-memory"><title>Memory</title>
      <para>
      The K60 has two 64 KiB SRAM banks giving a total of 128KiB on chip SRAM.
      </para>
      </refsect3>
    </refsect2>
  </refsect1>
</refentry>

<!--</part>-->
