//===========================================================================
//
// MLT linker script export - Tue Jan 13 10:14:27 1999
//
//===========================================================================
//####COPYRIGHTBEGIN####
//                                                                          
// -------------------------------------------                              
// The contents of this file are subject to the Red Hat eCos Public License 
// Version 1.1 (the "License"); you may not use this file except in         
// compliance with the License.  You may obtain a copy of the License at    
// http://www.redhat.com/                                                   
//                                                                          
// Software distributed under the License is distributed on an "AS IS"      
// basis, WITHOUT WARRANTY OF ANY KIND, either express or implied.  See the 
// License for the specific language governing rights and limitations under 
// the License.                                                             
//                                                                          
// The Original Code is eCos - Embedded Configurable Operating System,      
// released September 30, 1998.                                             
//                                                                          
// The Initial Developer of the Original Code is Red Hat.                   
// Portions created by Red Hat are                                          
// Copyright (C) 1998, 1999, 2000 Red Hat, Inc.                             
// All Rights Reserved.                                                     
// -------------------------------------------                              
//                                                                          
//####COPYRIGHTEND####
//===========================================================================

MEMORY
{
    rom : ORIGIN = 0x40000000, LENGTH = 0x80000
    ram : ORIGIN = 0x48000000, LENGTH = 0x200000
}

SECTIONS
{
    SECTIONS_BEGIN
    SECTION_rom_vectors (rom, 0x40000000, LMA_EQ_VMA)
    SECTION_text (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_fini (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_rodata (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_rodata1 (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_fixup (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_gcc_except_table (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_data (ram, 0x48000000, FOLLOWING (.gcc_except_table))
    SECTION_bss (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTIONS_END
}
