//===========================================================================
//
// MLT linker script for MN10300
// adapted from packages\hal\mn10300\stdeval1\v1_1\src\stdeval1.ld
//
//===========================================================================
//####COPYRIGHTBEGIN####
//                                                                          
// -------------------------------------------                              
// The contents of this file are subject to the Red Hat eCos Public License 
// Version 1.1 (the "License"); you may not use this file except in         
// compliance with the License.  You may obtain a copy of the License at    
// http://www.redhat.com/                                                   
//                                                                          
// Software distributed under the License is distributed on an "AS IS"      
// basis, WITHOUT WARRANTY OF ANY KIND, either express or implied.  See the 
// License for the specific language governing rights and limitations under 
// the License.                                                             
//                                                                          
// The Original Code is eCos - Embedded Configurable Operating System,      
// released September 30, 1998.                                             
//                                                                          
// The Initial Developer of the Original Code is Red Hat.                   
// Portions created by Red Hat are                                          
// Copyright (C) 1998, 1999, 2000 Red Hat, Inc.                             
// All Rights Reserved.                                                     
// -------------------------------------------                              
//                                                                          
//####COPYRIGHTEND####
//===========================================================================

#include <pkgconf/system.h>
STARTUP(vectors.o)
ENTRY(reset_vector)
#ifdef EXTRAS
INPUT(extras.o)
#endif
GROUP(libtarget.a libgcc.a)


#define ALIGN_LMA 4
#define FOLLOWING(_section_) AT ((LOADADDR (_section_) + SIZEOF (_section_) + ALIGN_LMA - 1) & ~ (ALIGN_LMA - 1))
#define LMA_EQ_VMA
#define FORCE_OUTPUT . = .

#define SECTIONS_BEGIN

#define SECTION_rom_vectors(_region_, _vma_, _lma_) \
    .rom_vectors _vma_ : _lma_ \
    { FORCE_OUTPUT; KEEP (*(.vectors)) } \
    > _region_

#define SECTION_text(_region_, _vma_, _lma_) \
    .text _vma_ : _lma_ \
    { _stext = ABSOLUTE(.); \
    *(.text*) *(.gnu.warning) *(.gnu.linkonce*) *(.init) } \
    > _region_ \
    _etext = .; PROVIDE (etext = .);

#define SECTION_fini(_region_, _vma_, _lma_) \
    .fini _vma_ : _lma_ \
    { FORCE_OUTPUT; *(.fini) } \
    > _region_

#define SECTION_rodata(_region_, _vma_, _lma_) \
    .rodata _vma_ : _lma_ \
    { FORCE_OUTPUT; *(.rodata*) } \
    > _region_

#define SECTION_rodata1(_region_, _vma_, _lma_) \
    .rodata1 _vma_ : _lma_ \
    { FORCE_OUTPUT; *(.rodata1) } \
    > _region_

#define SECTION_fixup(_region_, _vma_, _lma_) \
    .fixup _vma_ : _lma_ \
    { FORCE_OUTPUT; *(.fixup) } \
    > _region_

#define SECTION_gcc_except_table(_region_, _vma_, _lma_) \
    .gcc_except_table _vma_ : _lma_ \
    { FORCE_OUTPUT; *(.gcc_except_table) } \
    > _region_

#define SECTION_data(_region_, _vma_, _lma_) \
    .data _vma_ : _lma_ \
    { __ram_data_start = ABSOLUTE (.); *(.data*) *(.data1) \
    . = ALIGN(4); \
    ___DEVTAB__ = ABSOLUTE (.); KEEP (*(SORT (.devtab*))) ___DEVTAB_END__ = ABSOLUTE (.); \
    __NETDEVTAB__ = ABSOLUTE (.); KEEP (*(SORT (.netdevtab*))) __NETDEVTAB_END__ = ABSOLUTE (.); \
    _GOT1_START_ = ABSOLUTE (.); *(.got1) _GOT1_END_ = ABSOLUTE (.); \
    _GOT2_START_ = ABSOLUTE (.); *(.got2) _GOT2_END_ = ABSOLUTE (.); \
    . = ALIGN (4); \
    __CTOR_LIST__ = ABSOLUTE (.); KEEP (*(SORT (.ctors*))) __CTOR_END__ = ABSOLUTE (.); \
    __DTOR_LIST__ = ABSOLUTE (.); KEEP (*(SORT (.dtors*))) __DTOR_END__ = ABSOLUTE (.); \
    _GOT_START = ABSOLUTE (.); _GLOBAL_OFFSET_TABLE_ = ABSOLUTE (.) + 32768; _SDA_BASE_ = ABSOLUTE (.); \
    *(.got.plt) *(.got) _GOT_END_ = ABSOLUTE (.); \
    *(.dynamic) *(.sdata*) *(.sbss*) } \
    > _region_ \
    __rom_data_start = LOADADDR (.data); \
    __ram_data_end = .; PROVIDE (__ram_data_end = .); _edata = .; PROVIDE (edata = .);

#define SECTION_bss(_region_, _vma_, _lma_) \
    .bss _vma_ : _lma_ \
    { __bss_start = ABSOLUTE (.); \
    *(.scommon) *(.dynbss) *(.bss) *(COMMON) \
    __bss_end = ABSOLUTE (.); } \
    > _region_

#define SECTIONS_END . = ALIGN(4); _end = .; PROVIDE (end = .);

#include CYGHWR_MEMORY_LAYOUT_LDI

_mn10300_interrupt_control = 0xD4000000;
_mn10300_interrupt_vectors = 0xC0000000;

_hal_vsr_table = 0x50000100;
_hal_virtual_vector_table = 0x50000200;
