===========================================================================
#####ECOSGPLCOPYRIGHTBEGIN####
## -------------------------------------------
## This file is part of eCos, the Embedded Configurable Operating System.
## Copyright (C) 1998, 1999, 2000, 2001, 2002 Red Hat, Inc.
##
## eCos is free software; you can redistribute it and/or modify it under
## the terms of the GNU General Public License as published by the Free
## Software Foundation; either version 2 or (at your option) any later version.
##
## eCos is distributed in the hope that it will be useful, but WITHOUT ANY
## WARRANTY; without even the implied warranty of MERCHANTABILITY or
## FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
## for more details.
##
## You should have received a copy of the GNU General Public License along
## with eCos; if not, write to the Free Software Foundation, Inc.,
## 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA.
##
## As a special exception, if other files instantiate templates or use macros
## or inline functions from this file, or you compile this file and link it
## with other works to produce a work based on this file, this file does not
## by itself cause the resulting work to be covered by the GNU General Public
## License. However the source code for this file must still be made available
## in accordance with section (3) of the GNU General Public License.
##
## This exception does not invalidate any other reasons why a work based on
## this file might be covered by the GNU General Public License.
##
## Alternative licenses for eCos may be arranged by contacting Red Hat, Inc.
## at http://sources.redhat.com/ecos/ecos-license/
## -------------------------------------------
#####ECOSGPLCOPYRIGHTEND####
===========================================================================

How to build and install the GDB module on ARM Integrator

Make GDB module
~~~~~~~~~~~~~~~
Configure and build using the 'stubs' template for the PID
target. These are the necessary CLI instructions. It can also be done
from the Configtool by selecting the appropriate templates.

 % cd /tmp
 % mkdir stubs
 % cd stubs
 % ecosconfig new integrator stubs
 % ecosconfig tree
 % make

This will install some files in ./install/bin:

 gdb_module.elf:   The built stubs image
 gdb_module.bin:   The image converted to binary (suitable for burning to ROM)
 gdb_module.img:   The relocated ELF image (suitable for FLASH writing, see below)


Prepare board for eCos
~~~~~~~~~~~~~~~~~~~~~~

Program FLASH
~~~~~~~~~~~~~
The GDB module can be programmed into the begining of the user flash using an ARM debugger 
connected to the board either via Angel or Multi-ICE. 

