//===========================================================================
//
// ROM start linker control script
//
//===========================================================================
//####COPYRIGHTBEGIN####
//
// -------------------------------------------
// The contents of this file are subject to the Cygnus eCos Public License
// Version 1.0 (the "License"); you may not use this file except in
// compliance with the License.  You may obtain a copy of the License at
// http://sourceware.cygnus.com/ecos
// 
// Software distributed under the License is distributed on an "AS IS"
// basis, WITHOUT WARRANTY OF ANY KIND, either express or implied.  See the
// License for the specific language governing rights and limitations under
// the License.
// 
// The Original Code is eCos - Embedded Cygnus Operating System, released
// September 30, 1998.
// 
// The Initial Developer of the Original Code is Cygnus.  Portions created
// by Cygnus are Copyright (C) 1998,1999 Cygnus Solutions.  All Rights Reserved.
// -------------------------------------------
//
//####COPYRIGHTEND####
//===========================================================================

MEMORY
{
    rom : ORIGIN = 0xfff00000, LENGTH = 0x40000
    ram : ORIGIN = 0x00002000, LENGTH = 0x7fe000
}

SECTIONS
{
    SECTIONS_BEGIN
    SECTION_vectors (rom, 0xfff00000, LMA_EQ_VMA)
    SECTION_text (rom, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_fini (rom, ALIGN (0x8), LMA_EQ_VMA)
    SECTION_rodata1 (rom, ALIGN (0x8), LMA_EQ_VMA)
    SECTION_rodata (rom, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_fixup (rom, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_gcc_except_table (rom, ALIGN (0x1), LMA_EQ_VMA)
    SECTION_data (ram, 0x2000, FOLLOWING (.gcc_except_table))
    SECTION_sbss (ram, ALIGN (0x4), LMA_EQ_VMA)
    SECTION_bss (ram, ALIGN (0x10), LMA_EQ_VMA)
    SECTIONS_END
}
